Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B847	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:	Burwilla Hole 12, 202m W of Peg No. 0
	Date Desc.:	19/09/74	Elevation:	125 metres
	Map Ref.:	Sheet No. : 9545-IV   1:50000	Rainfall:	No Data
	Northing/Long.:	153.0886738	Runoff:	No Data
	Easting/Lat.:	-26.03876295	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	120 metres
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	48.6 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Podosol     	Principal Profile Form:	Uc3.21
	ASC Confidence:	Great Soil Group:	Podzol
	Confidence level not specified
	Site Disturbance:
	Vegetation:	Low Strata - , 1.01-3m, . *Species includes - Themeda australis, Pteridium aquilinum, Leptospermum stellatum, Acacia 
	cunninghamii	Mid Strata - , 6.01-12m, . *Species includes - Banksia serrata, Banksia integrifolia, Casuarina suberosa
	Tall Strata - , 20.01-35m, . *Species includes - Angophora intermedia, Eucalyptus pilularis
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.03 m	Greyish brown (10YR5/2-Moist); , 10YR51; Sand; Single grain grade of structure; Loose 
	consistence; Field pH 6.8 (Raupach); Wavy change to - 
	A2	0.03 - 0.06 m	Greyish brown (10YR5/2-Moist); , 10YR62; , 10YR72; Sand; Single grain grade of structure; 
	Very weak consistence; Field pH 6.5 (Raupach); Wavy change to - 
	B1	0.06 - 0.1 m	Brownish yellow (10YR6/6-Moist); , 10YR56; , 10YR54; Sand; Single grain grade of structure; 
	Very weak consistence; Field pH 7 (Raupach); Diffuse change to - 
	B2	0.1 - 0.2 m	Brownish yellow (10YR6/6-Moist); , 10YR54; , 10YR75; Sand; Single grain grade of structure; 
	Very weak consistence; Field pH 6.8 (Raupach); Diffuse change to - 
	B31	0.2 - 0.3 m	Brownish yellow (10YR6/6-Moist); , 10YR75; Sand; Single grain grade of structure; Loose 
	consistence; Field pH 7 (Raupach); , coarse (>5mm) roots; 
	B32	0.3 - 0.4 m	Yellow (10YR7/5-Moist); , 10YR66; Sand; Single grain grade of structure; Loose consistence; 
	Field pH 7 (Raupach); Diffuse change to - 
	C1	0.4 - 0.6 m	Yellow (10YR7/6-Moist); , 10YR62; Sand; Single grain grade of structure; Loose consistence; 
	Field pH 7 (Raupach); 
	C1	0.6 - 0.9 m	Yellow (10YR7/6-Moist); , 10YR62; Sand; Single grain grade of structure; Loose consistence; 
	Field pH 7 (Raupach); 
	C1	0.9 - 1.2 m	Yellow (10YR7/6-Moist); , 10YR62; Sand; Single grain grade of structure; Loose consistence; 
	Field pH 7 (Raupach); 
	C1	1.2 - 1.5 m	Yellow (10YR7/6-Moist); , 10YR62; Sand; Single grain grade of structure; Loose consistence; 
	Field pH 7 (Raupach); 
	C1	1.5 - 1.8 m	Yellow (10YR7/6-Moist); , 10YR66; Sand; Single grain grade of structure; Field pH 7.5 
	C1	1.8 - 2.1 m	Yellow (10YR7/6-Moist); , 10YR66; Sand; Single grain grade of structure; Field pH 7.5 
	C1	2.1 - 2.4 m	Yellow (10YR7/6-Moist); , 10YR66; Sand; Single grain grade of structure; Field pH 7.5 

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B847	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	C1	2.4 - 2.7 m	Yellow (10YR7/6-Moist); , 10YR66; Sand; Single grain grade of structure; Field pH 7.5 
	C1	2.7 - 3 m	Yellow (10YR7/6-Moist); , 10YR66; Sand; Single grain grade of structure; 
	C1	3 - 3.3 m	Yellow (10YR7/6-Moist); , 10YR62; Sand; Single grain grade of structure; 
	C1	3.3 - 3.6 m	Yellow (10YR7/6-Moist); , 10YR62; Sand; Single grain grade of structure; 
	C1	3.6 - 3.9 m	Yellow (10YR7/5-Moist); , 10YR62; Sand; Single grain grade of structure; 
	C1	3.9 - 4.2 m	Yellow (10YR7/5-Moist); , 10YR62; Sand; Single grain grade of structure; 
	C1	4.2 - 4.5 m	Yellow (10YR7/5-Moist); , 10YR62; Single grain grade of structure; 
	Morphological Notes
	A11	Discrete OM
	B1	yB patches are weakly organic
	B2	yB patches of OM + Fe
	B31	Tree roots
	C1	Paler patches along old rootlines - few OM segregations also.
	Observation Notes
	Parent material: Quaternary silica sands (Burwilla formation).  Landform: Eroded nose of stabilised sandblow - middle slope.
	Site Notes
	State forest for indigenous hardwoods esp. E.pilularis

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B847	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	5.6H	<0.02B
	0.03 - 0.06	5.5H	<0.02B	0.2K	0.1	<0.1	<0.1	0.6D	0.9F
	0.06 - 0.1	5.7H	<0.02B
	0.1 - 0.2	5.6H	<0.02B	<0.1K	<0.1	<0.1	<0.1	0.3D	0.3F
	0.2 - 0.3	5.6H	<0.02B
	0.3 - 0.4	5.8H	<0.02B
	0.4 - 0.6	5.7H	<0.02B
	0.6 - 0.9	5.8H	<0.02B
	0.9 - 1.2	5.7H	<0.02B
	1.2 - 1.5	5.8H	<0.02B	<0.1K	<0.1	<0.1	<0.1	0.3D	0.3F
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3	5.3H	<0.02B
	3 - 3.3
	3.3 - 3.6
	3.6 - 3.9
	3.9 - 4.2
	4.2 - 4.5	5.4H	<0.02B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	0.54E	2B	0.015B
	0.03 - 0.06	0.4E	2B	0.011B
	0.06 - 0.1	0.24E	1B	0.008B
	0.1 - 0.2	0.17E	1B	0.005B
	0.2 - 0.3	0.09E	1B	0.004B
	0.3 - 0.4	0.08E	1B	0.003B
	0.4 - 0.6	0.05E	1B	0.003B
	0.6 - 0.9	0.02E	2B	0.004B
	0.9 - 1.2	0.03E	3B	0.003B
	1.2 - 1.5	0.03E	3B	0.001B
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3	0.1E	2B	0.001B
	3 - 3.3
	3.3 - 3.6
	3.6 - 3.9
	3.9 - 4.2
	4.2 - 4.5	0.02E	5B	<0.001B
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B847	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.03 - 0.06
	0.06 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3
	3 - 3.3
	3.3 - 3.6
	3.6 - 3.9
	3.9 - 4.2
	4.2 - 4.5

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B847	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J1	Effective CEC
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	8A1	Total organic carbon/total nitrogen ratio
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)