Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B851	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:	124m W 4m North of Ref Peg No 0.
	Date Desc.:	02/10/74	Elevation:	190 metres
	Map Ref.:	Sheet No. : 9545-IV   1:50000	Rainfall:	No Data
	Northing/Long.:	153.0875127	Runoff:	No Data
	Easting/Lat.:	-26.02475398	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	120 metres
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	37.8 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Podosol     	Principal Profile Form:	Uc2.21
	ASC Confidence:	Great Soil Group:	Podzol
	Confidence level not specified
	Site Disturbance:
	Vegetation:	Low Strata - , 6.01-12m, . *Species includes - Banksia integrifolia
	Mid Strata - , 12.01-20m, . *Species includes - Casuarina torulosa
	Tall Strata - , 20.01-35m, . *Species includes - Angophora woodsiana, Eucalyptus pilularis
	Surface Coarse Fragments:
	Profile Morphology
	A00	0 - 0.01 m	; ; 
	A11a12	0.01 - 0.11 m	Grey (10YR6/1-Moist); Light grey (10YR7/1-Moist); ; Sand; Single grain grade of structure; Very
	 weak consistence; Field pH 7 (Raupach); Wavy change to - 
	A12	0.11 - 0.21 m	Grey (10YR5/1-Moist); Dark grey (10YR4/1-Moist); ; Sand; Single grain grade of structure; Very
	 weak consistence; Field pH 6 (Raupach); 
	A12	0.21 - 0.31 m	Grey (10YR5/1-Moist); , 10YR61; Sand; Single grain grade of structure; Weak consistence; 
	Field pH 6 (Raupach); Diffuse change to - 
	A13	0.31 - 0.61 m	Grey (10YR5/1-Moist); , 10YR71; Sand; Single grain grade of structure; Weak consistence; 
	Field pH 5.8 (Raupach); 
	A13	0.61 - 0.76 m	Grey (10YR5/1-Moist); , 10YR71; Sand; Single grain grade of structure; Weak consistence; 
	Field pH 5.8 (Raupach); Diffuse change to - 
	A21	0.76 - 0.91 m	Light grey (10YR7/2-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	Field pH 6 (Raupach); 
	A21	0.91 - 1.21 m	; Sand; Single grain grade of structure; Very weak consistence; Field pH 6 (Raupach); 
	A21	1.21 - 1.51 m	; Sand; Single grain grade of structure; Loose consistence; Field pH 7 (Raupach); 
	A21	1.51 - 1.81 m	; Sand; Single grain grade of structure; Loose consistence; Field pH 7 (Raupach); Wavy change
	 to - 
	B1	1.81 - 2.11 m	; Sand; Single grain grade of structure; Weak consistence; Field pH 6 (Raupach); Diffuse 
	change to - 
	B2	2.11 - 2.41 m	; Sand; Single grain grade of structure; Weak consistence; Field pH 6 (Raupach); 
	B2	2.41 - 2.71 m	; Sand; Single grain grade of structure; Weak consistence; Field pH 6.2 (Raupach); 
	B22	2.71 - 3.01 m	; Sand; Single grain grade of structure; Weak consistence; Field pH 6.5 (Raupach); 

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B851	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B22	3.01 - 3.31 m	; Sand; Single grain grade of structure; Firm consistence; Field pH 7 (Raupach); 
	B3	3.31 - 3.61 m	; Sand; Single grain grade of structure; Weak consistence; Field pH 7 (Raupach); 
	B3	3.61 - 3.91 m	; Sand; Single grain grade of structure; Weak consistence; Field pH 7 (Raupach); 
	B3	3.91 - 4.21 m	; Sand; Single grain grade of structure; Weak consistence; Field pH 6.5 (Raupach); 
	B3	4.21 - 4.51 m	; Sand; Single grain grade of structure; Weak consistence; Field pH 6.5 (Raupach); 
	B3	4.51 - 4.81 m	; Sand; Single grain grade of structure; Weak consistence; Field pH 7 (Raupach); 
	B3	4.81 - 5.11 m	; Sand; Single grain grade of structure; Weak consistence; Field pH 7 (Raupach); 
	B3	5.11 - 5.41 m	; Sand; Single grain grade of structure; Weak consistence; Field pH 7 (Raupach); 
	B3	5.41 - 5.71 m	; Sand; Single grain grade of structure; Weak consistence; Field pH 7 (Raupach); 
	B3	5.71 - 6.01 m	; Sand; Single grain grade of structure; Weak consistence; Field pH 7 (Raupach); 
	Morphological Notes
	A00	Leaf litter from E.pilularis, C.torulosa, B.integrifolia, A. woodsiana, T.australis.
	A11a12	Discrete OM, charcoal, leaves, seed pods etc.
	A12	Diffuse OM and roots.
	A12	VDbG 12-15mm worm channels, many roots.
	A21	Gradually becomes paler with depth.
	A21	Uneven undulating bdy to: organic accumulation.
	B2	tr Fe OM lumps.
	B22	Organic hard pan.
	B3	Fairly large organic patches 25mm.
	B3	Soft OM patches.
	Observation Notes
	Parent material: Quaternary silica sand. Micro-relief: Some unevenness due to sand trapping. Landform: nose of stabilised 
	sandblow.  Surface accumulation ranges from 10 - 15cm.  Locally 0 - 10cm is representative.  Uneven Podzol B.
	Site Notes
	Surface accummulation ranges from 10 - 15cm.  Locally 0 - 10cm is representative.  Grassy forest.

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B851	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01
	0.01 - 0.11	5.8H	<0.02B
	0.11 - 0.21
	0.21 - 0.31	5.2H	<0.02B
	0.31 - 0.61
	0.61 - 0.76	5.4H	<0.02B
	0.76 - 0.91
	0.91 - 1.21	6H	<0.02B
	1.21 - 1.51
	1.51 - 1.81
	1.81 - 2.11	5.7H	<0.02B
	2.11 - 2.41	5.5H	<0.02B
	2.41 - 2.71
	2.71 - 3.01	5.4H	<0.02B
	3.01 - 3.31
	3.31 - 3.61	5.8H	<0.02B
	3.61 - 3.91
	3.91 - 4.21
	4.21 - 4.51	5.8H	<0.02B
	4.51 - 4.81
	4.81 - 5.11
	5.11 - 5.41
	5.41 - 5.71
	5.71 - 6.01	6.5H	<0.02B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01
	0.01 - 0.11	0.29E	2B	0.009B
	0.11 - 0.21
	0.21 - 0.31	0.46E	2B	0.015B
	0.31 - 0.61
	0.61 - 0.76	0.14E	2B	0.006B
	0.76 - 0.91
	0.91 - 1.21	<0.02E	2B	0.004B
	1.21 - 1.51
	1.51 - 1.81
	1.81 - 2.11	0.004E	2B	0.004B
	2.11 - 2.41	0.1E	2B	0.004B
	2.41 - 2.71
	2.71 - 3.01	0.07E	4B	0.021B
	3.01 - 3.31
	3.31 - 3.61	0.21E	6B	0.009B
	3.61 - 3.91
	3.91 - 4.21
	4.21 - 4.51	0.16E	9B	0.013B
	4.51 - 4.81
	4.81 - 5.11
	5.11 - 5.41
	5.41 - 5.71

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B851	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	5.71 - 6.01	0.05E	12B	0.004B
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.01
	0.01 - 0.11
	0.11 - 0.21
	0.21 - 0.31
	0.31 - 0.61
	0.61 - 0.76
	0.76 - 0.91
	0.91 - 1.21
	1.21 - 1.51
	1.51 - 1.81
	1.81 - 2.11
	2.11 - 2.41
	2.41 - 2.71
	2.71 - 3.01
	3.01 - 3.31
	3.31 - 3.61
	3.61 - 3.91
	3.91 - 4.21
	4.21 - 4.51
	4.51 - 4.81
	4.81 - 5.11
	5.11 - 5.41
	5.41 - 5.71
	5.71 - 6.01

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B851	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	8A1	Total organic carbon/total nitrogen ratio
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)