Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B858	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:	23m S 178m W of Ref Peg 150m
	Date Desc.:	20/11/74	Elevation:	No Data
	Map Ref.:	Sheet No. : 9545-IV   1:50000	Rainfall:	No Data
	Northing/Long.:	153.1253261	Runoff:	No Data
	Easting/Lat.:	-26.04565379	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	25.7 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Uc2.21
	ASC Confidence:	Great Soil Group:	Alluvial soil
	Confidence level not specified
	Site Disturbance:
	Vegetation:	Low Strata - , 1.01-3m, . *Species includes - Themeda australis, Petalostigma species, Acacia cunninghamii, 
	Leptospermum stellatum	Mid Strata - , 12.01-20m, . *Species includes - Casuarina torulosa, Banksia integrifolia, Angophora woodsiana, Tristania 
	conferta
	Surface Coarse Fragments:
	Profile Morphology
	A00	0 - 0.01 m	; ; 
	A11	0.01 - 0.11 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; Loose 
	consistence; Field pH 7 (Raupach); Diffuse change to - 
	A12	0.11 - 0.21 m	Greyish brown (10YR5/2-Moist); , 10YR62; Sand; Single grain grade of structure; Loose 
	consistence; Field pH 6.8 (Raupach); Clear change to - 
	2A1	0.21 - 0.31 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Weak 
	consistence; Field pH 6.5 (Raupach); 
	2A1	0.31 - 0.41 m	Dark grey (10YR4/1-Moist); ; Sand; Single grain grade of structure; Weak consistence; Field pH 
	7 (Raupach); 
	2Ac	0.41 - 0.61 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; Field pH 7 (Raupach); 
	3A1	0.61 - 0.71 m	Very dark greyish brown (10YR3/2-Moist); ; Sand; Single grain grade of structure; Weak 
	consistence; Field pH 6.5 (Raupach); 
	3A1	0.71 - 0.91 m	Dark greyish brown (10YR4/2-Moist); Pale brown (10YR6/3-Moist); ; Sand; Single grain grade 
	of structure; Weak consistence; Field pH 6.8 (Raupach); 
	3Ac	0.91 - 1.21 m	Dark greyish brown (10YR4/2-Moist); Pale brown (10YR6/3-Moist); ; Sand; Single grain grade 
	of structure; Weak consistence; Field pH 6.8 (Raupach); 
	3Ac	1.21 - 1.41 m	Dark greyish brown (10YR4/2-Moist); Pale brown (10YR6/3-Moist); ; Sand; Single grain grade 
	of structure; Weak consistence; Field pH 6.8 (Raupach); 
	4A1	1.41 - 1.51 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Weak 
	2Ac	1.51 - 1.81 m	Dark greyish brown (10YR4/2-Moist); Pale brown (10YR6/3-Moist); ; Sand; Single grain grade 
	of structure; Very weak consistence; 
	2Ac	1.81 - 2.11 m	Dark greyish brown (10YR4/2-Moist); Pale brown (10YR6/3-Moist); ; Sand; Single grain grade 
	of structure; Very weak consistence; 

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B858	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	2C	2.11 - 2.41 m	Light olive brown (2.5Y5/4-Moist); , 10YR52; Sand; Single grain grade of structure; Loose 
	consistence; 
	2C	2.41 - 2.61 m	Light olive brown (2.5Y5/4-Moist); , 10YR52; Sand; Single grain grade of structure; Loose 
	consistence; 
	3A1	2.61 - 2.71 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Weak 
	3A1	2.71 - 3.01 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Weak 
	3A1	3.01 - 3.31 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Weak 
	3A1	3.31 - 3.61 m	Dark greyish brown (10YR4/2-Moist); Pale brown (10YR6/3-Moist); ; Sand; Single grain grade 
	of structure; Very weak consistence; 
	3B	3.61 - 3.91 m	Brown (10YR5/3-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	3B	3.91 - 4.21 m	Brown (10YR5/3-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	3C	4.21 - 4.51 m	Light yellowish brown (2.5Y6/4-Moist); ; Sand; Single grain grade of structure; Loose 
	3C	4.51 - 4.81 m	Light yellowish brown (2.5Y6/4-Moist); ; Sand; Single grain grade of structure; Loose 
	3C	4.81 - 5.11 m	Light yellowish brown (2.5Y6/4-Moist); ; Sand; Single grain grade of structure; Loose 
	3C	5.11 - 5.41 m	Light yellowish brown (2.5Y6/4-Moist); ; Sand; Single grain grade of structure; Loose 
	3C	5.41 - 5.71 m	Light yellowish brown (2.5Y6/4-Moist); ; Sand; Single grain grade of structure; Loose 
	3A	5.71 - 6.01 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Weak 
	2C	6.01 - 6.31 m	Light yellowish brown (2.5Y6/4-Moist); , 10YR42; Sand; Single grain grade of structure; Weak 
	consistence; 
	2C	6.31 - 6.61 m	Light yellowish brown (2.5Y6/4-Moist); , 10YR42; Sand; Single grain grade of structure; Weak 
	consistence; 
	3A	6.61 - 6.91 m	Dark greyish brown (10YR4/2-Moist); , 10YR54; Sand; Single grain grade of structure; Weak 
	consistence; 
	3A	6.91 - 7.21 m	Dark greyish brown (10YR4/2-Moist); , 10YR54; Sand; Single grain grade of structure; Weak 
	consistence; 
	3C	7.21 - 7.51 m	Light olive brown (2.5Y5/4-Moist); , 10YR42; Sand; Single grain grade of structure; Very weak 
	consistence; 
	3C	7.51 - 7.81 m	Light olive brown (2.5Y5/4-Moist); , 10YR42; Sand; Single grain grade of structure; Very weak 
	consistence; 
	3A	7.81 - 8.11 m	Very dark grey (10YR3/1-Moist); , 10YR51; Sand; Single grain grade of structure; Weak 
	consistence; 
	3A	8.11 - 8.41 m	Very dark grey (10YR3/1-Moist); , 10YR51; Sand; Single grain grade of structure; Weak 
	consistence; 
	3B2	8.41 - 8.56 m	Brown (10YR4/3-Moist); ; Sand; Single grain grade of structure; Weak consistence; 
	3B2	8.56 - 8.71 m	Yellowish brown (10YR5/6-Moist); Brownish yellow (10YR6/6-Moist); , 10YR43; Sand; Single 
	grain grade of structure; Weak consistence; 
	3B2	8.71 - 9.01 m	Yellowish brown (10YR5/6-Moist); Brownish yellow (10YR6/6-Moist); , 10YR43; Sand; Single 
	grain grade of structure; Weak consistence; 
	3B3	9.01 - 9.61 m	Brownish yellow (10YR6/5-Moist); , 10YR56; Sand; Single grain grade of structure; Weak 
	consistence; 
	3C	9.61 - 10.21 m	Yellow (2.5Y7/5-Moist); ; Sand; Single grain grade of structure; Weak consistence; 
	Morphological Notes
	A00	Distcontinous litter cover (T.conferta and A. woodsiana leaves)
	A11	Some discrete OM.
	A12	Some diffuse OM.
	3A1	sl charcoal
	3A1	sl charcoal

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B858	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	4A1	sl charcoal. Diffuse OM.
	2C	sl charcoal.
	3A1	Diffuse Om. Traces of charcoal, 8mm.
	3B	Diffuse OM and may be very weak B.
	3A	Diffuse OM and charcoal.
	3A	Diffuse OM.
	3A	sl charcoal
	3A	Diffuse OM.
	3A	sl charcoal.
	3B2	Translocated OM.
	3B2	Translocated OM and Fe.
	3C	Raw Chalambar aeolin sand.
	Observation Notes
	Parent material: Recent siliceous sand.  Landform: Lower middle of 16degree sloping fan, see sketch on sheet. Micro-relief: 
	Slightly uneven due to sandtrapping by vegetation.  Veg: Open Grassy Forest.  GSG: Regosol?
	Site Notes
	State Forest Reserve for indigenous hardwoods - controlled burning every 3rd year, but not burned in area burn July 1974.

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B858	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01
	0.01 - 0.11	6.1H	<0.02B
	0.11 - 0.21	5.6H	<0.02B
	0.21 - 0.31	5.5H	<0.02B
	0.31 - 0.41
	0.41 - 0.61	5.5H	<0.02B
	0.61 - 0.71	5.9H	<0.02B
	0.71 - 0.91
	0.91 - 1.21	5.9H	<0.02B
	1.21 - 1.41
	1.41 - 1.51	5.9H	<0.02B
	1.51 - 1.81
	1.81 - 2.11
	2.11 - 2.41	5.7H	<0.02B
	2.41 - 2.61
	2.61 - 2.71	5.9H	<0.02B
	2.71 - 3.01
	3.01 - 3.31
	3.31 - 3.61	5.7H	<0.02B
	3.61 - 3.91	5.7H	<0.02B
	3.91 - 4.21
	4.21 - 4.51	5.7H	<0.02B
	4.51 - 4.81
	4.81 - 5.11
	5.11 - 5.41
	5.41 - 5.71	5.6H	<0.02B
	5.71 - 6.01	5.9H	<0.02B
	6.01 - 6.31
	6.31 - 6.61	5.8H	<0.02B
	6.61 - 6.91	5.8H	<0.02B
	6.91 - 7.21
	7.21 - 7.51
	7.51 - 7.81	6.2H	<0.02B
	7.81 - 8.11	6.2H	<0.02B
	8.11 - 8.41
	8.41 - 8.56	5.6H	<0.02B
	8.56 - 8.71
	8.71 - 9.01
	9.01 - 9.61
	9.61 - 10.21	5.7H	<0.02B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01
	0.01 - 0.11	0.34E	1B	0.018B
	0.11 - 0.21	0.42E	0.021B
	0.21 - 0.31	0.52E	2B	0.025B
	0.31 - 0.41
	0.41 - 0.61	0.31E	0.011B

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B858	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.61 - 0.71	0.25E	1B	0.011B
	0.71 - 0.91
	0.91 - 1.21	0.17E	2B	0.008B
	1.21 - 1.41
	1.41 - 1.51	0.27E	3B	0.01B
	1.51 - 1.81
	1.81 - 2.11
	2.11 - 2.41	0.14E	0.008B
	2.41 - 2.61
	2.61 - 2.71	0.18E	4B	0.011B
	2.71 - 3.01
	3.01 - 3.31
	3.31 - 3.61
	3.61 - 3.91	0.15E	4B	0.006B
	3.91 - 4.21
	4.21 - 4.51	0.11E	3B	0.005B
	4.51 - 4.81
	4.81 - 5.11
	5.11 - 5.41
	5.41 - 5.71	0.09E	0.02B
	5.71 - 6.01	0.16E	6B	0.008B
	6.01 - 6.31
	6.31 - 6.61	0.1E	8B	0.005B
	6.61 - 6.91	0.08E	6B	0.005B
	6.91 - 7.21
	7.21 - 7.51
	7.51 - 7.81	0.13E	9B	0.006B
	7.81 - 8.11	0.25E	5B	0.008B
	8.11 - 8.41
	8.41 - 8.56	0.16E	4B	0.008B
	8.56 - 8.71
	8.71 - 9.01
	9.01 - 9.61
	9.61 - 10.21	0.09E	10B	0.003B
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.01
	0.01 - 0.11
	0.11 - 0.21
	0.21 - 0.31
	0.31 - 0.41
	0.41 - 0.61
	0.61 - 0.71
	0.71 - 0.91
	0.91 - 1.21
	1.21 - 1.41
	1.41 - 1.51
	1.51 - 1.81
	1.81 - 2.11
	2.11 - 2.41
	2.41 - 2.61
	2.61 - 2.71
	2.71 - 3.01
	3.01 - 3.31
	3.31 - 3.61
	3.61 - 3.91

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B858	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	3.91 - 4.21
	4.21 - 4.51
	4.51 - 4.81
	4.81 - 5.11
	5.11 - 5.41
	5.41 - 5.71
	5.71 - 6.01
	6.01 - 6.31
	6.31 - 6.61
	6.61 - 6.91
	6.91 - 7.21
	7.21 - 7.51
	7.51 - 7.81
	7.81 - 8.11
	8.11 - 8.41
	8.41 - 8.56
	8.56 - 8.71
	8.71 - 9.01
	9.01 - 9.61
	9.61 - 10.21

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B858	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	8A1	Total organic carbon/total nitrogen ratio
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)