Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B860	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:	4m E 2m S of Ref Peg 0.
	Date Desc.:	22/11/74	Elevation:	No Data
	Map Ref.:	Sheet No. : 9545-IV   1:50000	Rainfall:	No Data
	Northing/Long.:	153.1043856	Runoff:	No Data
	Easting/Lat.:	-26.04926048	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Podosol     	Principal Profile Form:	Uc2.21
	ASC Confidence:	Great Soil Group:	Podzol
	Confidence level not specified
	Site Disturbance:
	Vegetation:	Low Strata - , 1.01-3m, . *Species includes - Xanthorrhoea species, Acacia cunninghamii
	Mid Strata - , 12.01-20m, . *Species includes - Banksia serrata, Casuarina torulosa
	Tall Strata - , 20.01-35m, . *Species includes - Angophora woodsiana, Tristania conferta
	Surface Coarse Fragments:
	Profile Morphology
	A00	0 - 0.01 m	 (10YR7/2-Moist);  (/-Moist); ; 
	A11	0.01 - 0.06 m	Light grey (10YR7/2-Moist); Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of 
	structure; Loose consistence; Field pH 6.6 (Raupach); Gradual change to - 
	A12	0.06 - 0.11 m	Light brownish grey (10YR6/2-Moist); Greyish brown (10YR5/2-Moist); , 10YR21; Sand; Single 
	grain grade of structure; Weak consistence; Field pH 6.2 (Raupach); 
	A12	0.11 - 0.21 m	Light brownish grey (10YR6/2-Moist); Greyish brown (10YR5/2-Moist); , 10YR21; Sand; Single 
	grain grade of structure; Weak consistence; Diffuse change to - 
	A13	0.21 - 0.31 m	Grey (10YR5/1-Moist); Light brownish grey (10YR6/2-Moist); , 10YR21; , 10YR31; Sand; Single 
	grain grade of structure; Weak consistence; Field pH 5.5 (Raupach); Many
	A13	0.31 - 0.36 m	Grey (10YR5/1-Moist); Light brownish grey (10YR6/2-Moist); , 10YR21; , 10YR31; Sand; Single 
	grain grade of structure; Weak consistence; Diffuse change to - 
	A2	0.36 - 0.41 m	Light brownish grey (10YR6/2-Moist); Light grey (10YR7/2-Moist); , 10YR51; , 10YR53; Sand; 
	Single grain grade of structure; Very weak consistence; Field pH 6.6 (Raupach); Diffuse 
	change to - 
	B12	0.41 - 0.51 m	Brown (10YR5/3-Moist); , 10YR62; , 10YR33; Sand; Single grain grade of structure; Weak 
	consistence; Field pH 5.5 (Raupach); Diffuse change to - 
	B21	0.51 - 0.61 m	Dark brown (10YR3/3-Moist); , 10YR54; Sand; Single grain grade of structure; Weak 
	consistence; Field pH 5.5 (Raupach); Diffuse change to - 
	B22	0.61 - 0.81 m	Dark brown (7.5YR3/3-Moist); , 10YR56; , 10YR23; Sand; Single grain grade of structure; Firm 
	consistence; Field pH 5.2 (Raupach); Diffuse change to - 
	B23	0.81 - 0.91 m	Dark brown (10YR3/3-Moist); ; Sand; Single grain grade of structure; Firm consistence; Diffuse 
	change to - 
	B31	0.91 - 1.21 m	Yellowish brown (10YR5/4-Moist); , 10YR66; , 10YR43; Sand; Single grain grade of structure; 
	Weak consistence; Diffuse change to - 

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B860	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B32	1.21 - 1.51 m	Brownish yellow (10YR6/6-Moist); , 10YR54; , 10YR43; Sand; Single grain grade of structure; 
	Very weak consistence; Field pH 6.5 (Raupach); Diffuse change to - 
	B33	1.51 - 1.81 m	Brownish yellow (10YR6/5-Moist); , 10YR54; , 10YR44; Sand; Single grain grade of structure; 
	Loose consistence; Field pH 6.8 (Raupach); Diffuse change to - 
	C1	1.81 - 2.11 m	Brownish yellow (10YR6/5-Moist); ; Sand; Single grain grade of structure; Loose consistence; 
	Field pH 7 (Raupach); 
	C1	2.11 - 2.41 m	; Sand; Single grain grade of structure; Loose consistence; Diffuse change to - 
	C2	2.41 - 2.71 m	Yellow (10YR7/5-Moist); ; Sand; Single grain grade of structure; Loose consistence; Field pH 7 
	(Raupach); 
	C2	2.71 - 3.01 m	; Sand; Single grain grade of structure; Loose consistence; 
	Morphological Notes
	A00	Litter - mainly leaves from Banksia, Angophora, Tristania, Pteridium and Imperata genera.
	A11	Discrete OM. Heavily rain splashed despite almost 100% cover of litter and grass - 
	probably after-burning effects.
	A12	Discrete and diffuse OM
	A12	Black 12mm worm fills.
	A13	Many roots. Worm fills.
	A13	yB (10YR5/4) fauna trails.
	A2	Probably about 80% of A2 will dry to bleached colour ie. It meets the conspicuous 
	bleach requirement.
	B12	Black with patches of A2.
	B21	General augered colour 10YR3/4
	B22	VDB patches are (F1 - 12)
	B23	Some VDB (F1-1+1) patches.
	B31	yB is weak OM enrichment.
	B32	Weak OM enrichment.
	Observation Notes
	Veg: Open grassy forest.  Landform: Crest (narrow and convex) of sandblow wing.
	Site Notes
	Indigenous hardwood forest with natural regeneration management under controlled culling and fire control.  Controlled burning 
	every 3 years to reduce combustible material.

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B860	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01
	0.01 - 0.06	5.7H	<0.02B
	0.06 - 0.11	5.6H	<0.02B
	0.11 - 0.21	5.7H	<0.02B	<0.1K	<0.1	<0.1	<0.1	1D	1.1F
	0.21 - 0.31
	0.31 - 0.36	5.6H	<0.02B
	0.36 - 0.41	5H	<0.02B
	0.41 - 0.51	5.1H	<0.02B	<0.1K	<0.1	<0.1	<0.1	0.8F
	0.51 - 0.61	5.1H	<0.02B	<0.1K	<0.1	<0.1	<0.1	1.2F
	0.61 - 0.81
	0.81 - 0.91	5.5H	<0.02B	<0.1K	<0.1	<0.1	<0.1	0.6F
	0.91 - 1.21
	1.21 - 1.51	5.8H	<0.02B
	1.51 - 1.81	<0.1K	<0.1	<0.1	<0.1	<0.1D	0.4F
	1.81 - 2.11
	2.11 - 2.41	6.1H	<0.02B
	2.41 - 2.71
	2.71 - 3.01	5.9H	<0.02B	<0.1K	<0.1	<0.1	<0.1	0.3F
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01
	0.01 - 0.06	0.81E	2B	0.033B
	0.06 - 0.11	0.6E	3B	0.021B
	0.11 - 0.21	0.55E	2B	0.019B	99I	0	0
	0.21 - 0.31	0.48E	3B	0.02B
	0.31 - 0.36	0.32E	2B	0.013B
	0.36 - 0.41	0.23E	1B	0.011B
	0.41 - 0.51	0.18E	1B	0.011B
	0.51 - 0.61	0.31E	2B	0.018B	96I	1	2
	0.61 - 0.81	0.71E	4B	0.024B
	0.81 - 0.91	0.5E	6B	0.02B	97I	0	2
	0.91 - 1.21	0.3E	8B	0.015B
	1.21 - 1.51	0.15E	6B	0.008B
	1.51 - 1.81	0.08E	7B	0.008B
	1.81 - 2.11	0.11E	6B	0.004B	100I	0	0
	2.11 - 2.41	0.04E	5B	0.004B
	2.41 - 2.71
	2.71 - 3.01	0.04E	4B	0.004B
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.01
	0.01 - 0.06
	0.06 - 0.11
	0.11 - 0.21
	0.21 - 0.31

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B860	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.31 - 0.36
	0.36 - 0.41
	0.41 - 0.51
	0.51 - 0.61
	0.61 - 0.81
	0.81 - 0.91
	0.91 - 1.21
	1.21 - 1.51
	1.51 - 1.81
	1.81 - 2.11
	2.11 - 2.41
	2.41 - 2.71
	2.71 - 3.01

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B860	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J1	Effective CEC
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	8A1	Total organic carbon/total nitrogen ratio
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded