Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B867	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:	High wing overlying and above Warrawonga South 
	B866
	Date Desc.:	09/07/75	Elevation:	200 metres
	Map Ref.:	Sheet No. : 9545-IV   1:50000	Rainfall:	No Data
	Northing/Long.:	153.0941809	Runoff:	No Data
	Easting/Lat.:	-26.04033333	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	45 metres
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Podosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Podzol
	Confidence level not specified
	Site Disturbance:
	Vegetation:	Low Strata - , , . *Species includes - Acacia cunninghamii
	Mid Strata - , 6.01-12m, . *Species includes - Banksia integrifolia, Casuarina torulosa, Eucalyptus pilularis, Angophora 
	woodsiana
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.1 m	Grey (10YR6/1-Moist); Light grey (10YR7/1-Moist); ; Sand; Single grain grade of structure; 
	Loose consistence; Field pH 7 (Raupach); 
	A12	0.1 - 0.2 m	Grey (10YR5/1-Moist); Grey (10YR6/1-Moist); ; Sand; Single grain grade of structure; Loose 
	consistence; Field pH 6.7 (Raupach); 
	A13	0.2 - 0.3 m	Grey (10YR5/1-Moist); Dark grey (10YR4/1-Moist); ; Sand; Single grain grade of structure; Very
	 weak consistence; Field pH 6.5 (Raupach); 
	A21	0.3 - 0.4 m	Light brownish grey (10YR6/2-Moist); Light grey (10YR7/2-Moist); , 10YR56; Sand; Single grain 
	grade of structure; Very weak consistence; Field pH 6.3 (Raupach); 
	A22	0.4 - 0.5 m	Light brownish grey (10YR6/2-Moist); Light grey (10YR7/2-Moist); , 10YR53; , 10YR56; Sand; 
	Single grain grade of structure; Very weak consistence; Field pH 6 (Raupach); 
	A3	0.5 - 0.6 m	Pale brown (10YR6/3-Moist); , 10YR72; , 10YR56; Sand; Single grain grade of structure; Very 
	weak consistence; Field pH 6 (Raupach); Diffuse change to - 
	B1	0.6 - 0.8 m	Pale brown (10YR6/3-Moist); , 7.5YR56; Sand; Single grain grade of structure; Very weak 
	consistence; Field pH 6 (Raupach); Diffuse change to - 
	B21	0.8 - 0.9 m	Reddish yellow (7.5YR6/6-Moist); , 7.5YR44; Sand; Single grain grade of structure; Very weak 
	consistence; 
	B21	0.9 - 1.2 m	Reddish yellow (7.5YR6/6-Moist); , 7.5YR44; Sand; Single grain grade of structure; Very weak 
	consistence; Field pH 6 (Raupach); 
	B21	1.2 - 1.5 m	Reddish yellow (7.5YR6/6-Moist); , 7.5YR44; Sand; Single grain grade of structure; Very weak 
	consistence; 
	B22	1.5 - 1.8 m	Reddish yellow (7.5YR6/6-Moist); , 10YR44; , 10YR56; Sand; Single grain grade of structure; 
	Very weak consistence; Field pH 6.5 (Raupach); 
	B3	1.8 - 2.1 m	Brownish yellow (10YR6/6-Moist); , 10YR44; , 10YR64; Sand; Single grain grade of structure; 
	Loose consistence; Field pH 7 (Raupach); 

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B867	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B3	2.1 - 2.4 m	Brownish yellow (10YR6/6-Moist); , 10YR44; , 10YR64; Sand; Single grain grade of structure; 
	Loose consistence; Field pH 7 (Raupach); 
	C	2.4 - 2.7 m	Yellowish brown (10YR5/4-Moist); , 10YR64; Sand; Single grain grade of structure; Loose 
	consistence; Field pH 7 (Raupach); 
	C	2.7 - 3 m	Yellowish brown (10YR5/4-Moist); , 10YR64; Sand; Single grain grade of structure; Loose 
	consistence; Field pH 7 (Raupach); 
	C	3 - 3.3 m	Light yellowish brown (10YR6/4-Moist); , 10YR54; Sand; Single grain grade of structure; Loose
	 consistence; Field pH 7 (Raupach); 
	C	3.3 - 3.6 m	Light yellowish brown (10YR6/4-Moist); , 10YR54; Sand; Single grain grade of structure; Loose
	 consistence; Field pH 7 (Raupach); 
	C	3.6 - 3.9 m	Olive yellow (2.5Y6/5-Moist); ; Sand; Single grain grade of structure; Loose consistence; Field 
	pH 7 (Raupach); 
	C	3.9 - 4.2 m	; 
	C	4.2 - 4.5 m	; 
	Morphological Notes
	A11	Discrete OM.
	A12	Discrete and diffuse OM
	A13	Diffuse OM.
	A21	YB patches appear to be of faunal origin.
	A22	Few bleached pockets of YB faunal patches as above.
	B1	Occassional LB patch
	B21	Fe hummate B horizon
	B3	B hummate patches > with depth.
	C	Raw sand.
	Observation Notes
	Parent material: Silica sand.  Landform: Sandblow wing crest.  Veg: Grassy Forest.
	Site Notes

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B867	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.2H	<0.02B
	0.1 - 0.2	5.3H	<0.02B
	0.2 - 0.3	5.2H	<0.02B
	0.3 - 0.4	5.3H	<0.02B
	0.4 - 0.5	5.4H	<0.02B
	0.5 - 0.6	5.3H	<0.02B
	0.6 - 0.8	5.3H	<0.02B
	0.8 - 0.9	5.3H	<0.02B
	0.9 - 1.2	5.5H	<0.02B
	1.2 - 1.5	5.8H	<0.02B
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4	5.8H	<0.02B
	2.4 - 2.7
	2.7 - 3	5.5H	<0.02B
	3 - 3.3
	3.3 - 3.6
	3.6 - 3.9
	3.9 - 4.2
	4.2 - 4.5	5.6H	<0.02B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.38E	3B	0.009B
	0.1 - 0.2	0.25E	2B	0.01B
	0.2 - 0.3	0.24E	3B	0.015B
	0.3 - 0.4	0.12E	3B	0.009B
	0.4 - 0.5	0.09E	2B	0.005B
	0.5 - 0.6	0.07E	2B	0.006B
	0.6 - 0.8	0.05E	1B	0.004B
	0.8 - 0.9	0.16E	1B	0.01B
	0.9 - 1.2	0.1E	3B	0.008B
	1.2 - 1.5	0.1E	2B	0.005B
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4	0.09E	7B	0.006B
	2.4 - 2.7
	2.7 - 3	0.05E	5B	0.004B
	3 - 3.3
	3.3 - 3.6
	3.6 - 3.9
	3.9 - 4.2
	4.2 - 4.5	0.03E	4B	0.004B
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B867	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.8
	0.8 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3
	3 - 3.3
	3.3 - 3.6
	3.6 - 3.9
	3.9 - 4.2
	4.2 - 4.5

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B867	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	8A1	Total organic carbon/total nitrogen ratio
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)