Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B875	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:	North side of road on crest YB sandhill just east of 
	YB/LbG sands bdy on road.
	Date Desc.:	13/07/76	Elevation:	45 metres
	Map Ref.:	Sheet No. : 9545-IV   1:50000	Rainfall:	No Data
	Northing/Long.:	153.1099261	Runoff:	No Data
	Easting/Lat.:	-26.10363179	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Crest	Relief:	15 metres
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Podosol     	Principal Profile Form:	Uc3.21
	ASC Confidence:	Great Soil Group:	Podzol
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.03 m	Light brownish grey (10YR6/2-Moist); Light grey (10YR7/2-Moist); , 10YR52; Sand; Single grain 
	grade of structure; Loose consistence; Field pH 6 (Raupach); 
	A12	0.03 - 0.1 m	Greyish brown (10YR5/2-Moist); , 10YR31; Sand; Single grain grade of structure; Weak 
	consistence; Field pH 5.5 (Raupach); 
	A13	0.1 - 0.15 m	Brown (10YR5/3-Moist); , 10YR51; , 10YR52; Sand; Single grain grade of structure; Very weak
	 consistence; Field pH 5.8 (Raupach); 
	A2	0.15 - 0.2 m	Light yellowish brown (10YR6/4-Moist); Pale brown (10YR6/3-Dry); , 10YR73; Sand; Single 
	grain grade of structure; Very weak consistence; Field pH 6 (Raupach); 
	A2	0.2 - 0.3 m	Light yellowish brown (10YR6/4-Moist); Pale brown (10YR6/3-Dry); , 10YR73; Sand; Single 
	grain grade of structure; Very weak consistence; 
	B1	0.3 - 0.4 m	Yellowish brown (10YR5/4-Moist); , 10YR64; , 10YR44; Sand; Single grain grade of structure; 
	Very weak consistence; Field pH 6.2 (Raupach); 
	B21	0.4 - 0.6 m	Yellowish brown (10YR5/4-Moist); , 10YR44; , 10YR64; Sand; Single grain grade of structure; 
	Very weak consistence; Field pH 6.3 (Raupach); 
	B21	0.6 - 0.8 m	Dark yellowish brown (10YR4/4-Moist); Light yellowish brown (10YR6/4-Moist); , 10YR44; , 
	10YR64; Sand; Single grain grade of structure; Very weak consistence; 
	B3	0.8 - 0.9 m	Brownish yellow (10YR6/5-Moist); , 10YR54; , 10YR64; Sand; Single grain grade of structure; 
	Very weak consistence; Field pH 6.4 (Raupach); 
	B3	0.9 - 1.05 m	Brownish yellow (10YR6/5-Moist); , 10YR54; , 10YR64; Sand; Single grain grade of structure; 
	Very weak consistence; 
	C	1.05 - 1.2 m	Brownish yellow (10YR6/5-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; Field pH 6.5 (Raupach); 
	C	1.2 - 1.5 m	Brownish yellow (10YR6/5-Moist); ; Sand; Single grain grade of structure; Very weak 
	Morphological Notes
	A11	Rain washed - discrete OM.

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B875	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	A12	Diffuse OM and root and worm channels.
	A13	Diffuse OM patches.
	A2	Few paler patches.
	A2	A2 has a scattered array of bleached paler patches, very random distribution through 
	A2,B2&B3 horizons - prob. due to earlier root lines…….
	B1	Trans hummate patches few.
	B21	Mod. Hummate patches.
	B21	Worm sample - large worm at 70cm.
	Observation Notes
	Parent material: Siliceous Sand.  Landform: Sand dune (young) wing crest.  Veg: Woodland.  A very soft soil - surface is loose
	 - A horizons are held together by root mass, B horizons are very soft to barely coherant, C are virtually loose.
	Site Notes

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B875	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	5.6H	<0.03B
	0.03 - 0.1	4.8H	<0.03B	<0.1K	<0.1	1.1F
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.3	5.2H	<0.03B
	0.3 - 0.4	5.3H	<0.03B
	0.4 - 0.6	5.2H	<0.03B
	0.6 - 0.8
	0.8 - 0.9
	0.9 - 1.05	5H	<0.03B
	1.05 - 1.2
	1.2 - 1.5	5H	<0.03B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0.03 - 0.1	96I	1	2
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.6	98I	0	0
	0.6 - 0.8
	0.8 - 0.9
	0.9 - 1.05
	1.05 - 1.2
	1.2 - 1.5	99I	0	0
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.1
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.6
	0.6 - 0.8
	0.8 - 0.9
	0.9 - 1.05
	1.05 - 1.2
	1.2 - 1.5

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B875	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15J1	Effective CEC
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded