Project Name:	EAR
	Project Code:	EAR	Site ID:	T343	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.J. Coventry	Locality:
	Date Desc.:	06/12/77	Elevation:	No Data
	Map Ref.:	Sheet No. : 7956   1:100000	Rainfall:	600
	Northing/Long.:	145.115277777778	Runoff:	No Data
	Easting/Lat.:	-20.7486111111111	Drainage:	No Data
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	N/A
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Ferric Orthic Tenosol     	Principal Profile Form:	Uc5.22
	ASC Confidence:	Great Soil Group:	Earthy sand
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, 0.26-0.5m, Very sparse. *Species includes - Triodia pungens
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Grevillea glauca
	Tall Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus similis
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); Brown (10YR5/3-Dry); ; Loamy sand (Light); Dry; Loose 
	consistence; Diffuse change to - 
	B1	0.1 - 0.2 m	Yellowish brown (10YR5/6-Moist); Brownish yellow (10YR6/6-Dry); ; Loamy sand; Dry; Weak 
	consistence; 
	B1	0.2 - 0.3 m	Yellowish brown (10YR5/6-Moist); ; Loamy sand; Dry; Weak consistence; 
	B1	0.3 - 0.6 m	Yellowish brown (10YR5/6-Moist); Brownish yellow (10YR6/6-Dry); ; Loamy sand; Dry; Weak 
	consistence; Diffuse change to - 
	B21	0.6 - 0.75 m	Brownish yellow (10YR6/6-Moist); Yellowish brown (10YR5/6-Dry); ; Sandy loam; Dry; Weak 
	consistence; Very few (0 - 2 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Gradual change to
	B22	0.75 - 0.9 m	Brownish yellow (10YR6/6-Moist); ; Sandy loam; Dry; Firm consistence; Many (20 - 50 %), 
	Ferruginous, Coarse (6 - 20 mm), Nodules; 
	B22	0.9 - 1 m	Brownish yellow (10YR6/6-Moist); ; Sandy loam; Dry; Firm consistence; Very many (50 - 100 
	%), Ferruginous, Coarse (6 - 20 mm), Nodules; Clear change to - 
	B3	1 - 1.05 m	Dark red (2.5YR3/6-Moist); ; Sandy loam; Dry; Firm consistence; Many (20 - 50 %), Ferruginous,
	 Coarse (6 - 20 mm), Nodules; 
	1.05 - 1.15 m	; 
	Morphological Notes
	Observation Notes
	MATERIAL FROM 75 CM IS VERY HARD TO AUGER BUT A SMALL CLOD IS FRIABLE.                                                  
	Site Notes

	Project Name:	EAR
	Project Code:	EAR	Site ID:	T343	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.7A	 0.023A	 0.22H	 0.05	 0.09	 0.02	 0.26F	 1.8A	 0.6F	1.11
	0.1 - 0.2	5.7A	 0.017A
	0.2 - 0.3	5.4A	 0.014A	 0.22H	 0.05	 0.06	 0.02	 0.35F	 1.4A	 0.7F	1.43
	0.3 - 0.6	5.3A	 0.011A
	0.6 - 0.75	5.8A	 0.013A	 0.02H	 0.68	 0.05	 0.02	 0.2F	 1.3A	 1F	1.54
	0.75 - 0.9	5.7A	 0.016A
	0.9 - 1	5.7A	 0.016A	 0.02H	 0.81	 0.05	 0.02	 0.19F	 1.5A	 1.1F	1.33
	1 - 1.05	5.6A	 0.014A
	1.05 - 1.15	6A	 0.014A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.46D	 0.04A	 1	 55A	 34	 3	 8
	0.1 - 0.2	 0.31D	 0.02A	 2	 51A	 36	 3	 10
	0.2 - 0.3	 0.82D	 0.03A	 3	 55A	 34	 3	 9
	0.3 - 0.6	 2	 53A	 35	 2	 10
	0.6 - 0.75	 6	 51A	 36	 26	 11
	0.75 - 0.9	 48	 51A	 35	 3	 11
	0.9 - 1	 56	 51A	 34	 3	 12
	1 - 1.05	 38	 56A	 31	 4	 10
	1.05 - 1.15	 44	 48A	 28	 7	 18
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.75
	0.75 - 0.9
	0.9 - 1
	1 - 1.05
	1.05 - 1.15

	Project Name:	EAR
	Project Code:	EAR	Site ID:	T343	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	MIN_EC	Exchange Capacity - Minerology
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	XRD_C_Ch	Chlorite - X-Ray Diffraction
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_Vm	Vermiculte - X-Ray Diffraction