Project Name:	FGR
	Project Code:	FGR	Site ID:	TL33	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	J.R. Sleeman	Locality:	36km north of Inverleigh Homestead:
	Date Desc.:	11/02/53	Elevation:	No Data
	Map Ref.:	Rainfall:	864
	Northing/Long.:	140.55	Runoff:	No Data
	Easting/Lat.:	-17.8666666666667	Drainage:	Very poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Tidal flat
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Tidal flat	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Saline
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solonchak
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.006 m	White (10YR8/1-Dry); ; Weak grade of structure, Platy; Abrupt change to - 
	0.006 - 0.02 m	Dark greyish brown (10YR4/2-Dry); ; Heavy clay; Weak grade of structure, Platy; Sharp 
	change to - 
	0.02 - 0.15 m	Dark greyish brown (10YR4/2-Dry); ; Heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Moderate grade of structure, 50-100 mm, Prismatic; 0-2%, Quartz, coarse 
	fragments; Very few (0 - 2 %), , , ; Diffuse change to - 
	0.15 - 0.25 m	Dark grey (10YR4/1-Dry); ; Heavy clay; 0-2%, coarse gravelly, 20-60mm, Quartz, coarse 
	fragments; Very few (0 - 2 %), , Coarse (6 - 20 mm), ; Very few (0 - 2 %), Gypseous, , ; 
	Diffuse change to - 
	0.25 - 0.43 m	Dark grey (10YR4/1-Dry); ; Heavy clay; Diffuse change to - 
	0.43 - 0.6 m	Dark grey (10YR4/1-Dry); ; Medium clay; Very few (0 - 2 %), Gypseous, , ; Clear change to - 
	0.6 - 0.91 m	Brownish yellow (10YR6/6-Dry); ; Medium clay; Very few (0 - 2 %), Gypseous, , ; Diffuse 
	change to - 
	0.91 - 1.22 m	Brownish yellow (10YR6/6-Dry); ; Medium clay; Diffuse change to - 
	1.22 - 1.37 m	Brownish yellow (10YR6/6-Dry); ; Medium clay; 
	Morphological Notes
	Observation Notes
	0-0.6 IS SALT:   LAYERS RE NUMBERED 16/10/92                                                                            
	Site Notes
	NORMANTON

	Project Name:	FGR
	Project Code:	FGR	Site ID:	TL33	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.006	7.6A	 0.007A
	0.006 - 0.02	7.9A	 0.012A
	0.02 - 0.15	8.2A	 0.005A
	0.15 - 0.25	8.5A	 0.003A
	0.25 - 0.43	8.6A	 0.003A
	0.6 - 0.91	8.5A	 0.005A
	1.22 - 1.37	8.7A	 0.005A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.006
	0.006 - 0.02	 0.04C	 190B	 0.024A	 2	 30	 42
	0.02 - 0.15	 0.03C	 160B	 1	 23D	 17	 14	 44
	0.15 - 0.25	 0.36C	 2
	0.25 - 0.43	 0.36C	<1	 31D	 19	 7	 35
	0.6 - 0.91	 0.95C	 1	 32D	 27	 3	 29
	1.22 - 1.37	 6.3C	 27	 20D	 21	 7	 39
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.006
	0.006 - 0.02
	0.02 - 0.15
	0.15 - 0.25
	0.25 - 0.43
	0.6 - 0.91
	1.22 - 1.37

	Project Name:	FGR
	Project Code:	FGR	Site ID:	TL33	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance