Project Name:	FGR
	Project Code:	FGR	Site ID:	TL46	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	J.R. Sleeman	Locality:	8km south west of Glenore:
	Date Desc.:	01/01/53	Elevation:	No Data
	Map Ref.:	Rainfall:	762
	Northing/Long.:	141.166666666667	Runoff:	Slow
	Easting/Lat.:	-18.3333333333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn2
	ASC Confidence:	Great Soil Group:	Yellow earth
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.08 m	Greyish brown (10YR5/2-Dry); ; Fine sandy clay loam; Massive grade of structure; Dry; Firm 
	consistence; Very few (0 - 2 %), Ferruginous, Fine (0 - 2 mm), Nodules; Gradual change to - 
	B1	0.08 - 0.18 m	Brown (10YR5/3-Dry); , 10YR78; Fine sandy light clay; Massive grade of structure; Dry; Firm 
	consistence; Very few (0 - 2 %), Ferruginous, Fine (0 - 2 mm), Nodules; Diffuse change to - 
	B21	0.18 - 0.3 m	Yellow (10YR7/8-Dry); , 5YR66; Medium clay; Massive grade of structure; Dry; Very strong 
	consistence; Few (2 - 10 %), Ferruginous, Fine (0 - 2 mm), Nodules; Diffuse change to - 
	B22	0.43 - 0.76 m	Yellow (10YR7/8-Dry); , 2.5YR46; Medium clay; Massive grade of structure; Dry; Very strong 
	consistence; Few (2 - 10 %), Ferruginous, Fine (0 - 2 mm), Nodules; 
	0.99 - 1.27 m	Brownish yellow (10YR6/8-Dry); , 10YR78; , 2.5YR46; Medium clay; Massive grade of 
	structure; Very strong consistence; Few (2 - 10 %), Ferruginous, Fine (0 - 2 mm), Nodules; 
	1.27 - 1.57 m	Brownish yellow (10YR6/8-Dry); , 10YR78; , 2.5YR46; Medium clay; Massive grade of 
	structure; Very strong consistence; Few (2 - 10 %), Ferruginous, Fine (0 - 2 mm), Nodules; 
	Morphological Notes
	Observation Notes
	Site Notes
	GLENORE

	Project Name:	FGR
	Project Code:	FGR	Site ID:	TL46	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.9A	 0.01A	 6.3K	 1.9	 0.3	 0.05	 0.2B
	0.08 - 0.18	6.6A	 0.006A
	0.18 - 0.3	6.6A	 0.006A	 4.7K	 2.5	 0.13	 0.11	 2.9B
	0.43 - 0.76	6.8A	 0.007A
	0.99 - 1.27	7.1A	 0.007A
	1.27 - 1.57	7.4A	 0.008A	 2.8K	 4	 0.04	 0.74	 2.5B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 1.3D	 4B	 0.013C	 0.072A	 13D	 53	 16	 12
	0.08 - 0.18	 0.61D	 2B	 0.011C	 0.039A	 11D	 49	 13	 22
	0.18 - 0.3	 10D	 42	 11	 32
	0.43 - 0.76	 13D	 33	 11	 43
	0.99 - 1.27	 10D	 38	 12	 37
	1.27 - 1.57	 0.11D	 8D	 36	 12	 40
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.18
	0.18 - 0.3
	0.43 - 0.76
	0.99 - 1.27
	1.27 - 1.57

	Project Name:	FGR
	Project Code:	FGR	Site ID:	TL46	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCLP2O5	Total element - P(%) - By boiling HCl(P2O5)
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance