Project Name:	GYC
	Project Code:	GYC	Site ID:	B523	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	18/11/63	Elevation:	 90 metres
	Map Ref.:	Sheet No. : 9445   1:100000	Rainfall:	1270
	Northing/Long.:	152.515277777778	Runoff:	Rapid
	Easting/Lat.:	-26.1611111111111	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	C-Pa	Substrate Material:	Soil pit, 0.74 m deep,Andesite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Upper-slope	Relief:	46 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Epipedal Brown Vertosol     	Principal Profile Form:	Gn3.72
	ASC Confidence:	Great Soil Group:	Prairie soil
	All necessary analytical data are available.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Dark brown (7.5YR3/2-Moist); ; Clay loam (Heavy); Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Moist; Weak consistence; 10-20%, medium gravelly, 6-20mm, coarse 
	fragments; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Soft segregations; Field pH 6 
	(pH meter); Abrupt change to - 
	A12	0.05 - 0.11 m	Very dark greyish brown (10YR3/2-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Moist; Weak consistence; 2-10%, fine gravelly, 2-6mm, coarse fragments; 
	Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Soft segregations; Field pH 5.9 (pH meter); 
	Clear change to - 
	B21	0.11 - 0.28 m	Yellowish brown (10YR5/6-Moist); ; Light medium clay (Heavy); Moderate grade of structure, 
	50-100 mm, Prismatic; Moderate grade of structure, 20-50 mm, Angular blocky; Moist; Firm 
	consistence; 0-2%, fine gravelly, 2-6mm, coarse fragments; Very few (0 - 2 %), 
	Manganiferous, Fine (0 - 2 mm), Nodules; Field pH 6.6 (pH meter); Gradual change to - 
	B22	0.28 - 0.56 m	Yellowish brown (10YR5/6-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Moist; Firm consistence; 0-2%, fine gravelly, 2-6mm, coarse fragments; Very 
	few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; Field pH 7 (pH meter); Gradual change 
	B3	0.56 - 0.74 m	Yellowish brown (10YR5/6-Moist); ; Medium clay; Weak grade of structure, Angular blocky; 
	Moist; Firm consistence; 2-10%, medium gravelly, 6-20mm, coarse fragments; Very few (0 - 2 
	%), Manganiferous, Fine (0 - 2 mm), Nodules; Field pH 7.4 (pH meter); Gradual change to - 
	C	0.74 - 0.99 m	Yellowish brown (10YR5/6-Moist); , 10YR44; , 10YR62; Light clay; Massive grade of structure; 
	10-20%, coarse gravelly, 20-60mm, Substrate material, coarse fragments; Very few (0 - 2 %), 
	Manganiferous, Medium (2 -6 mm), Soft segregations; Field pH 7.8 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	GLASTONBURY

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B523	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6H	 0.02B	 11.8K	 7.5	 0.58	 0.21	 17.6D
	0.05 - 0.11	5.9H	 0.03B	 9.3K	 6.2	 0.11	 0.12	 11.5D
	0.11 - 0.28	6.6H	 0.01B	 13.9K	 10.9	 0.11	 0.27	 14.3D
	0.28 - 0.56	7H	 0.01B	 16.6K	 14.4	 0.04	 0.43	 8.2D
	0.56 - 0.74	7.4H	 0.01B	 21.5K	 19.4	 0.04	 0.73	 2.7D
	0.74 - 0.99	7.8H	 0.01B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 3.3A	 2C	 0.054F	 0.287B	 13	 15C	 18	 23	 36
	0.05 - 0.11	 1.93A	 0.18B	 6	 17C	 17	 21	 41
	0.11 - 0.28	 1.08A	 0.03F	 2	 7C	 11	 16	 65
	0.28 - 0.56
	0.56 - 0.74	 0.009F	 4	 17C	 21	 21	 44
	0.74 - 0.99
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.11
	0.11 - 0.28
	0.28 - 0.56
	0.56 - 0.74
	0.74 - 0.99

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B523	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded