Project Name:	GYC
	Project Code:	GYC	Site ID:	B524	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	19/11/63	Elevation:	 76 metres
	Map Ref.:	Sheet No. : 9445   1:100000	Rainfall:	1143
	Northing/Long.:	152.569444444444	Runoff:	Rapid
	Easting/Lat.:	-26.1722222222222	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	R-Jy	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	15 metres
	Elem. Type:	Scarp-foot slope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Kandosol     	Principal Profile Form:	Uc5.21
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:	Low Strata - Tussock grass, , Closed or dense. *Species includes - Aristida species, Chloris gayana
	Tall Strata - Tree, , Closed or dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.15 m	Dark reddish brown (5YR3/3-Moist); ; Sandy loam; Weak grade of structure, 5-10 mm, 
	Subangular blocky; Many (>5 per 0.01m2) Coarse (>5mm) macropores, Moist; Very weak 
	consistence; Field pH 6.1 (pH meter); Clear change to - 
	A3	0.15 - 0.38 m	Dark reddish brown (5YR3/4-Moist); ; Sandy loam; Massive grade of structure; Common (1-5 
	per 0.01m2) Coarse (>5mm) macropores, Dry; Weak consistence; Field pH 5.8 (pH meter); 
	Diffuse change to - 
	B1	0.38 - 0.76 m	Dark reddish brown (5YR3/4-Moist); ; Clayey sand (Heavy); Massive grade of structure; Earthy
	 fabric; Common (1-5 per 0.01m2) Medium (2-5mm) macropores, Dry; Weak consistence; 2-
	10%, medium gravelly, 6-20mm, Sandstone, coarse fragments; Field pH 5.7 (pH meter); Diffuse 
	change to - 
	B21	0.76 - 1.09 m	Dark reddish brown (2.5YR3/3-Moist); ; Sandy clay loam; Massive grade of structure; Earthy 
	fabric; Few (<1 per 0.01m2) Medium (2-5mm) macropores, Dry; Weak consistence; 2-10%, 
	medium gravelly, 6-20mm, Sandstone, coarse fragments; Field pH 5.6 (pH meter); Diffuse 
	change to - 
	B22	1.09 - 1.55 m	Reddish brown (2.5YR4/4-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Moist; Very weak consistence; 2-10%, medium gravelly, 6-20mm, Sandstone, coarse 
	fragments; Field pH 5.7 (pH meter); Diffuse change to - 
	B3	1.55 - 2.08 m	Red (2.5YR4/5-Moist); ; Clayey sand (Heavy); Massive grade of structure; Moist; Very weak 
	consistence; 2-10%, medium gravelly, 6-20mm, Sandstone, coarse fragments; Field pH 6.1 (pH 
	meter); Diffuse change to - 
	B3	2.14 - 2.49 m	Red (2.5YR4/5-Moist); ; Clayey sand (Heavy); Massive grade of structure; Moist; Very weak 
	consistence; 10-20%, medium gravelly, 6-20mm, Sandstone, coarse fragments; Field pH 6.2 (pH
	 meter); Diffuse change to - 
	B3	2.49 - 2.67 m	Red (2.5YR4/5-Moist); , 10YR67, 20-50% , 5-15mm, Distinct; , 5YR66, 20-50% , 5-15mm, 
	Distinct; Clayey sand; Massive grade of structure; Moist; Very weak consistence; 2-10%, 
	medium gravelly, 6-20mm, Sandstone, coarse fragments; Field pH 6.3 (pH meter); 
	Morphological Notes
	Observation Notes

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B524	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Notes
	GREENDALE

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B524	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	6.1H	 0.01B	 1.4K	 0.51	 0.69	 0.08	 5.8D
	0.15 - 0.38	5.8H	 0.01B
	0.38 - 0.76	5.7H	 0.01B	 0.89K	 0.26	 0.48	 0.08	 4.1D
	0.76 - 1.09	5.6H	 0.01B
	1.09 - 1.55	5.7H	 0.01B	 1.7K	 0.7	 0.31	 0.22	 1.5D
	1.55 - 2.08	6.1H	 0.01B
	2.14 - 2.49	6.2H	 0.01B
	2.49 - 2.67	6.3H	 0.01B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 0.69A	 73C	 0.046F	 0.077B	 62C	 16	 6	 13
	0.15 - 0.38
	0.38 - 0.76	 0.11A	 0.023F	 2	 61C	 16	 8	 16
	0.76 - 1.09
	1.09 - 1.55	 6	 56C	 18	 8	 19
	1.55 - 2.08
	2.14 - 2.49	 0.022F	 12	 60C	 16	 8	 16
	2.49 - 2.67
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.38
	0.38 - 0.76
	0.76 - 1.09
	1.09 - 1.55
	1.55 - 2.08
	2.14 - 2.49
	2.49 - 2.67

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B524	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded