Project Name:	GYC
	Project Code:	GYC	Site ID:	B531	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	21/11/63	Elevation:	 185 metres
	Map Ref.:	Sheet No. : 9445   1:100000	Rainfall:	1520
	Northing/Long.:	152.819444444444	Runoff:	Very rapid
	Easting/Lat.:	-26.2161111111111	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  RW	Substrate Material:	Auger boring, Diorite 
	Land Form
	Rel/Slope Class: 	Steep hills 90-300m 32-56%	Pattern Type:	Hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	31.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Dermosol     	Principal Profile Form:	Gn3.14
	ASC Confidence:	Great Soil Group:	Euchrozem
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tussock grass, 12.01-20m, Closed or dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Very dark brown (10YR2/2-Moist); ; Clay loam; Strong grade of structure, 2-5 mm, Subangular 
	blocky; Few (<1 per 0.01m2) Medium (2-5mm) macropores, Moist; Weak consistence; Very few
	 (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; Field pH 6 (pH meter); Many, fine (1-2mm) 
	roots; Clear change to - 
	B1	0.08 - 0.25 m	Reddish brown (5YR4/4-Moist); ; Light clay; Strong grade of structure, 2-5 mm, Subangular 
	blocky; Common (1-5 per 0.01m2) Coarse (>5mm) macropores, Moist; Weak consistence; Very 
	few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; Field pH 6 (pH meter); Common, fine (1-
	2mm) roots; Gradual change to - 
	B2	0.25 - 0.53 m	Red (10R4/6-Moist); ; Medium heavy clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Few (<1 per 0.01m2) Coarse (>5mm) macropores, Moist; Firm consistence; Very few (0
	 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; Field pH 5.9 (pH meter); Common, fine (1-
	2mm) roots; Gradual change to - 
	B31	0.53 - 0.79 m	Dark red (2.5YR3/6-Moist); ; Light medium clay; Moderate grade of structure, 5-10 mm, Angular 
	blocky; Few (<1 per 0.01m2) Coarse (>5mm) macropores, Moist; Firm consistence; Very few (0
	 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; Field pH 5.8 (pH meter); Gradual change to - 
	B32	0.79 - 1.27 m	Red (2.5YR4/6-Moist); ; Light clay; Massive grade of structure; Moist; Weak consistence; Field 
	pH 6 (pH meter); Gradual change to - 
	C	1.32 - 1.83 m	Red (10R4/6-Moist); , 2.5Y44; Loam; Massive grade of structure; Moist; Weak consistence; 
	Field pH 6.4 (pH meter); Diffuse change to - 
	C	1.83 - 2.03 m	; Field pH 6.7 (pH meter); 
	Morphological Notes
	C	Speckled OLB; W; GR; BL soft weathered granodiorite.
	Observation Notes
	VIRGIN VEGETATION WAS `VINE SCRUB':                                                                                     
	Site Notes
	MT. TIETSEL

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B531	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6H	 0.03B	 5.6K	 1.9	 1	 0.17	 10.4D
	0.08 - 0.25	6H	 0.02B	 6.2K	 2.2	 0.29	 0.13	 5.3D
	0.25 - 0.53	5.9H	 0.02B	 4.3K	 4.9	 0.08	 0.15	 12D
	0.53 - 0.79	5.8H	 0.01B	 2.9K	 9.1	 0.13	 0.76	 6.8D
	0.79 - 1.27	6H	 0.01B
	1.32 - 1.83	6.4H	 0.01B
	1.83 - 2.03	6.7H	 0.01B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 2.12A	 10C	 0.046F	 0.292B	 26C	 28	 9	 29
	0.08 - 0.25
	0.25 - 0.53	 0.61A	 0.023F	 14C	 17	 11	 56
	0.53 - 0.79
	0.79 - 1.27
	1.32 - 1.83
	1.83 - 2.03	 0.041F
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.25
	0.25 - 0.53
	0.53 - 0.79
	0.79 - 1.27
	1.32 - 1.83
	1.83 - 2.03

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B531	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	MIN_EC	Exchange Capacity - Minerology
	MIN_NR_K2O	Kaolin minerals
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_Vm	Vermiculte - X-Ray Diffraction