Project Name:	GYC
	Project Code:	GYC	Site ID:	B568	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	26/10/66	Elevation:	 61 metres
	Map Ref.:	Sheet No. : 9445   1:100000	Rainfall:	1615
	Northing/Long.:	152.85	Runoff:	Very rapid
	Easting/Lat.:	-26.25	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Auger boring, 3.6 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Hills
	10%
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epiacidic Epipedal Red Vertosol     	Principal Profile Form:	Gn3.54
	ASC Confidence:	Great Soil Group:	Xanthozem
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Tall Strata - Sod grass, <0.25m, Closed or dense. *Species includes - Pennisetum clandestinum, Imperata cylindrica
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Brown (10YR4/3-Moist); ; Clay loam (Light); Strong grade of structure, <2 mm, Granular; Many (>5
	 per 100mm2)  macropores, Moist; Very weak consistence; 0-2%, medium gravelly, 6-20mm, 
	Quartz, coarse fragments; Field pH 6.1 (pH meter); Abundant, fine (1-2mm) roots; 
	A1	0.05 - 0.1 m	Brown (10YR4/3-Moist); ; Clay loam; Strong grade of structure, 5-10 mm, Subangular blocky; 
	Many (>5 per 100mm2)  macropores, Moist; Very weak consistence; 0-2%, medium gravelly, 6-
	20mm, Phyllite, coarse fragments; Field pH 5.9 (pH meter); Abundant, fine (1-2mm) roots; Clear 
	change to - 
	A2	0.1 - 0.2 m	Strong brown (7.5YR5/6-Moist); ; Clay loam; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Moist; Very weak consistence; 0-2%, medium gravelly, 6-20mm, Quartz, coarse 
	fragments; Field pH 5.7 (pH meter); Many, fine (1-2mm) roots; Gradual change to - 
	B1	0.2 - 0.3 m	Yellowish red (5YR5/6-Moist); ; Light clay; 2-5 mm, Polyhedral; Strong grade of structure, 20-50 
	mm, Angular blocky; Moist; Weak consistence; 0-2%, medium gravelly, 6-20mm, Quartz, coarse 
	fragments; Very few (0 - 2 %), Manganiferous, , Nodules; Field pH 5 (pH meter); Common, fine 
	(1-2mm) roots; 
	B1	0.3 - 0.45 m	Yellowish red (5YR5/6-Moist); ; Light medium clay; Strong grade of structure, Polyhedral; Strong
	 grade of structure, 20-50 mm, Angular blocky; Moist; Weak consistence; 0-2%, medium 
	gravelly, 6-20mm, Phyllite, coarse fragments; Very few (0 - 2 %), Manganiferous, , Nodules; Field
	 pH 4.9 (pH meter); Common, fine (1-2mm) roots; Diffuse change to - 
	B21	0.45 - 0.6 m	Yellowish red (5YR4/6-Moist); , 10YR68, 10-20% , 0-5mm, Faint; , 2.5YR46, 10-20% , 0-5mm, 
	Faint; Medium clay; Strong grade of structure, 2-5 mm, Polyhedral; Moist; Weak consistence; 0-
	2%, medium gravelly, 6-20mm, Quartz, coarse fragments; Very few (0 - 2 %), Manganiferous, , 
	Nodules; Field pH 4.8 (pH meter); Few, fine (1-2mm) roots; 
	B21	0.6 - 0.9 m	Yellowish red (5YR4/6-Moist); , 10YR68, 10-20% , 0-5mm, Faint; , 2.5YR46, 10-20% , 0-5mm, 
	Faint; Medium clay; Strong grade of structure, 2-5 mm, Polyhedral; Moist; Weak consistence; 0-
	2%, medium gravelly, 6-20mm, Quartz, coarse fragments; Very few (0 - 2 %), Manganiferous, , 
	Nodules; Field pH 4.8 (pH meter); Few, fine (1-2mm) roots; Diffuse change to - 

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B568	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B22	0.9 - 1.2 m	Red (2.5YR4/6-Moist); , 10YR78, 10-20% , 5-15mm, Distinct; , 5YR58, 10-20% , 5-15mm, 
	Distinct; Medium heavy clay; Strong grade of structure, 2-5 mm, Polyhedral; Moist; Firm 
	consistence; 0-2%, medium gravelly, 6-20mm, Quartz, coarse fragments; Field pH 4.7 (pH 
	meter); 
	B22	1.2 - 1.5 m	Red (2.5YR4/6-Moist); , 10YR78, 10-20% , 5-15mm, Distinct; , 5YR58, 10-20% , 5-15mm, 
	Distinct; Medium heavy clay; Strong grade of structure, 2-5 mm, Polyhedral; Moist; Firm 
	consistence; 0-2%, medium gravelly, 6-20mm, Quartz, coarse fragments; Field pH 4.7 (pH 
	meter); 
	B22	1.5 - 1.8 m	Red (2.5YR4/6-Moist); , 10YR78, 20-50% , 5-15mm, Distinct; , 5YR58, 20-50% , 5-15mm, 
	Distinct; Medium heavy clay; Strong grade of structure, 2-5 mm, Polyhedral; Moist; Firm 
	consistence; 0-2%, medium gravelly, 6-20mm, Quartz, coarse fragments; Field pH 4.7 (pH 
	meter); 
	B22	1.8 - 2.1 m	Red (2.5YR4/6-Moist); , 10YR78, 20-50% , 5-15mm, Distinct; , 5YR58, 20-50% , 5-15mm, 
	Distinct; Medium heavy clay; Strong grade of structure, 2-5 mm, Polyhedral; Moist; Firm 
	consistence; 0-2%, Quartz, coarse fragments; 
	B22	2.1 - 2.4 m	Red (2.5YR4/6-Moist); , 10YR78, 20-50% , 5-15mm, Distinct; , 5YR58, 20-50% , 5-15mm, 
	Distinct; Medium heavy clay; Strong grade of structure, 2-5 mm, Polyhedral; Moist; Firm 
	consistence; 0-2%, Quartz, coarse fragments; Diffuse change to - 
	B3	2.4 - 2.7 m	Red (10R4/6-Moist); , 5YR58, 20-50% , 15-30mm, Prominent; , 10YR78, 20-50% , 15-30mm, 
	Prominent; Medium clay; Moderate grade of structure, 5-10 mm, Polyhedral; Moist; Firm 
	consistence; 0-2%, Quartz, coarse fragments; 
	B3	2.7 - 3 m	Red (10R4/6-Moist); , 5YR58, 20-50% , 15-30mm, Prominent; , 10YR78, 20-50% , 15-30mm, 
	Prominent; Medium clay; Moderate grade of structure, 5-10 mm, Polyhedral; Moist; Firm 
	consistence; 0-2%, Quartz, coarse fragments; 
	B3	3 - 3.3 m	Red (10R4/6-Moist); , 5YR58, 20-50% , 15-30mm, Prominent; , 10YR78, 20-50% , 15-30mm, 
	Prominent; Medium clay; Moderate grade of structure, 5-10 mm, Polyhedral; Moist; Firm 
	consistence; 0-2%, Quartz, coarse fragments; 
	B3	3.3 - 3.6 m	Red (10R4/6-Moist); , 5YR58, 20-50% , 15-30mm, Prominent; , 10YR78, 20-50% , 15-30mm, 
	Prominent; Medium clay; Moderate grade of structure, 5-10 mm, Polyhedral; Moist; Firm 
	consistence; 0-2%, Quartz, coarse fragments; Diffuse change to - 
	D	3.6 - 3.9 m	Red (10R4/8-Moist); , 2.5Y71, 20-50% , 15-30mm, Prominent; , 10YR78, 20-50% , 15-30mm, 
	Prominent; Light medium clay; Weak grade of structure, 5-10 mm, Angular blocky; Moist; Firm 
	consistence; 0-2%, Quartz, coarse fragments; 
	D	3.9 - 4.2 m	Red (10R4/8-Moist); , 2.5Y71, 20-50% , 15-30mm, Prominent; , 10YR78, 20-50% , 15-30mm, 
	Prominent; Light medium clay; Weak grade of structure, 5-10 mm, Angular blocky; Moist; Firm 
	consistence; 10-20%, Phyllite, coarse fragments; Diffuse change to - 
	D	4.2 - 4.5 m	Red (10R4/8-Moist); , 10R36, 20-50% , 30-mm, Prominent; , 2.5Y71, 20-50% , 30-mm, 
	Prominent; Light medium clay; Weak grade of structure, Angular blocky; Moist; Firm 
	consistence; 10-20%, Phyllite, coarse fragments; 
	D	4.5 - 4.8 m	Red (10R4/8-Moist); , 10R36, 20-50% , 30-mm, Prominent; , 2.5Y71, 20-50% , 30-mm, 
	Prominent; Light medium clay; Weak grade of structure, Angular blocky; Moist; Firm 
	consistence; 2-10%, Phyllite, coarse fragments; 
	Morphological Notes
	Observation Notes
	0-5CM POROUS GRANULAR STRUCTURE:PARENT MATERIAL COLLUVIUM - ALLUVIUM FROM PHYLLITE:3.6-4.8M 
	PHYLLITE WEATHERED IN SITU: 
	Site Notes
	KIN KIN

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B568	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.1A	 0.141A	 5.1B	 2.6	 1.8	 0.6	 5.8D
	0.05 - 0.1	5.9A	 0.068A	 3.3B	 1.5	 1.3	 0.52	 3.2D
	0.1 - 0.2	5.7A	 0.049A	 2.2B	 1.5	 0.67	 0.16	 2.6D
	0.2 - 0.3	5A	 0.043A	 0.63B	 0.5	 0.3	 0.13	 3.6D
	0.3 - 0.45	4.9A	 0.038A	 0.52B	 0.57	 0.18	 0.2	 4.5D
	0.45 - 0.6	4.8A	 0.038A	 0.36B	 0.49	 0.1	 0.15	 4.9D
	0.6 - 0.9	4.8A	 0.038A
	0.9 - 1.2	4.7A	 0.035A	 0.05B	 0.8	 0.05	 0.09	 15.2D
	1.2 - 1.5	4.7A	 0.03A
	1.5 - 1.8	4.7A	 0.035A	 0.05B	 0.6	 0.05	 0.13	 3.9D
	1.8 - 2.1	4.5A	 0.041A
	2.1 - 2.4	4.6A	 0.035A
	2.4 - 2.7	4.6A	 0.035A
	2.7 - 3	4.6A	 0.035A
	3 - 3.3	4.6A	 0.032A
	3.3 - 3.6	4.6A	 0.032A	 0.11B	 0.38	 0.08	 0.14	 4.5D
	3.6 - 3.9	4.5A	 0.032A
	3.9 - 4.2	4.6A	 0.035A
	4.2 - 4.5	4.5A	 0.037A
	4.5 - 4.8	4.6A	 0.032A	 0.02B	 0.18	 0.07	 0.1	 4.1D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 5.81A	 20A	 0.08A	 0.52B	 1.1A	1.01	 2C	 18	 32	 38
	 12B
	0.05 - 0.1	 2.96A	 19A	 0.077A	 0.34B	 1.1A	 4	 6C	 14	 31	 40
	 8.2B
	0.1 - 0.2	 2.33A	 3.9A	 0.057A	 0.22B	 1.2A	1.29	 6C	 12	 35	 45
	 4.9B
	0.2 - 0.3	 0.99A	 0.046A	 0.13B	 1.3A	1.41	 3	 4C	 13	 35	 49
	0.3 - 0.45	 0.76A	 0.043A	 0.096B	 1.3A	 4	 4C	 11	 24	 51
	0.45 - 0.6	 0.58A	 0.035A	 0.071B	 1.5A	1.46	 2	 7C	 12	 28	 54
	0.6 - 0.9
	0.9 - 1.2	 0.033A	 0.066B	 1.9A	1.55	 1	 2C	 8	 26	 62
	1.2 - 1.5
	1.5 - 1.8	 0.031A	 0.053B	 2A	 1	 1C	 9	 30	 59
	1.8 - 2.1
	2.1 - 2.4	 2	 1C	 8	 35	 57
	2.4 - 2.7	 3	 1C	 8	 39	 55
	2.7 - 3
	3 - 3.3
	3.3 - 3.6	 2	 2C	 7	 39	 53
	3.6 - 3.9
	3.9 - 4.2
	4.2 - 4.5
	4.5 - 4.8	 9	 2C	 8	 44	 47
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B568	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0 - 0.05	0.41F	0.26H
	0.05 - 0.1
	0.1 - 0.2	0.41F	0.25H
	0.2 - 0.3	0.37F	0.26H
	0.3 - 0.45
	0.45 - 0.6	0.39F	0.3H
	0.6 - 0.9
	0.9 - 1.2	0.42F	0.36H
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3
	3 - 3.3
	3.3 - 3.6
	3.6 - 3.9
	3.9 - 4.2
	4.2 - 4.5
	4.5 - 4.8

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B568	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A1	Bulk density - g/cm3
	P3B3VLe004	0.04 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	suction plate
	P3B3VLe01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	suction plate
	P3B3VLe03	0.3 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	suction plate
	P3B3VLe06	0.6 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate
	P3B3VLe15	15 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate
	P3B3VLe2	2 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate
	P3B3VLe7	7 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate