Project Name:	GYC
	Project Code:	GYC	Site ID:	B646	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	27/08/69	Elevation:	 91 metres
	Map Ref.:	Sheet No. : 9445   1:100000	Rainfall:	1270
	Northing/Long.:	152.706944444444	Runoff:	Rapid
	Easting/Lat.:	-26.1941666666667	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Rlk	Substrate Material:	Undisturbed soil core, 0.4 m deep,Phyllite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	No Data	Relief:	35 metres
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	1.7 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Paralithic Orthic Tenosol     	Principal Profile Form:	Um2.12
	ASC Confidence:	Great Soil Group:	Lithosol
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Tall Strata - Tree, , Mid-dense. *Species includes - Eucalyptus propinqua, Eucalyptus crebra
	Surface Coarse Fragments:	10-20%, , , Phyllite
	Profile Morphology
	A11	0 - 0.06 m	Very dark brown (7.5YR2/2-Moist); ; Loam; Moderate grade of structure, <2 mm, Granular; Moist; 
	Weak consistence; 20-50%, medium gravelly, 6-20mm, Phyllite, coarse fragments; 
	A12	0.06 - 0.2 m	Brown (7.5YR4/4-Moist); ; Loam; Weak grade of structure, Subangular blocky; Dry; Firm 
	consistence; 20-50%, medium gravelly, 6-20mm, Phyllite, coarse fragments; 
	A2	0.2 - 0.4 m	Brown (7.5YR5/4-Moist); ; Loam; Massive grade of structure; Dry; Firm consistence; 20-50%, 
	medium gravelly, 6-20mm, Phyllite, coarse fragments; 
	C	0.4 - 0.6 m	Light olive brown (2.5Y5/4-Moist); ; Massive grade of structure; Strong consistence; 50-90%, 
	Phyllite, coarse fragments; 
	0.6 - 0.75 m	Light olive brown (2.5Y5/4-Moist); ; Massive grade of structure; Strong consistence; 90-100%, 
	Phyllite, coarse fragments; 
	Morphological Notes
	Observation Notes
	0-6CM POROUS GRANULAR STRUCTURE.                                                                                        
	Site Notes
	DEEP CREEK

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B646	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.4 - 0.6
	0.6 - 0.7
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.4 - 0.6
	0.6 - 0.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.4 - 0.6
	0.6 - 0.7

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B646	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile