Project Name:	GYC
	Project Code:	GYC	Site ID:	B655	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	06/08/69	Elevation:	 244 metres
	Map Ref.:	Sheet No. : 9445   1:100000	Rainfall:	1143
	Northing/Long.:	152.696111111111	Runoff:	Very rapid
	Easting/Lat.:	-26.06	Drainage:	Rapidly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Rlk	Substrate Material:	Undisturbed soil core, 0.7 m deep,Phyllite 
	Land Form
	Rel/Slope Class: 	Steep hills 90-300m 32-56%	Pattern Type:	Hills
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	31.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Chromosol     	Principal Profile Form:	Dr2.21
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	No analytical data and little or no knowledge of this soil.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Tall Strata - Tree, , Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.01 m	Dark reddish brown (5YR3/2-Moist); ; Loam; Moderate grade of structure, <2 mm, Granular; Dry; 
	Firm consistence; 
	A12	0.01 - 0.1 m	Dark reddish grey (5YR4/2-Moist); ; Loam (Heavy); Weak grade of structure, 2-5 mm, Polyhedral; 
	Dry; Firm consistence; 2-10%, medium gravelly, 6-20mm, Phyllite, coarse fragments; 
	A2	0.1 - 0.18 m	Reddish brown (5YR5/4-Moist); , 5YR64, 10-20% , 0-5mm, Faint; , 10-20% , 0-5mm, Faint; Silty 
	clay loam; Weak grade of structure, 2-5 mm, Polyhedral; Dry; Firm consistence; 20-50%, 
	medium gravelly, 6-20mm, Phyllite, coarse fragments; 
	B21	0.18 - 0.4 m	Red (2.5YR4/6-Moist); ; Medium clay; Moderate grade of structure, 2-5 mm, Polyhedral; Dry; Firm 
	consistence; 2-10%, medium gravelly, 6-20mm, Phyllite, coarse fragments; 
	B22	0.4 - 0.6 m	Red (2.5YR4/6-Moist); , 2.5Y64, 20-50% , 0-5mm, Faint; , 20-50% , 0-5mm, Faint; Medium clay; 
	Moderate grade of structure, 2-5 mm, Polyhedral; Dry; Firm consistence; 10-20%, medium 
	gravelly, 6-20mm, Phyllite, coarse fragments; 
	B3	0.6 - 0.7 m	Very pale brown (10YR7/4-Moist); , 2.5YR36, 20-50% , 0-5mm, Faint; , 20-50% , 0-5mm, Faint; 
	Light medium clay; Weak grade of structure, 2-5 mm, Polyhedral; Dry; Very firm consistence; 50-
	90%, coarse gravelly, 20-60mm, Phyllite, coarse fragments; 
	C	0.7 - 0.9 m	Red (2.5YR4/6-Moist); , 2.5Y72, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; 
	Massive grade of structure; Very firm consistence; 50-90%, Phyllite, coarse fragments; 
	0.9 - 1.1 m	Dark reddish brown (2.5YR3/4-Moist); , 2.5Y72; Massive grade of structure; Strong consistence; 
	90-100%, Phyllite, coarse fragments; 
	1.1 - 1.4 m	Dark reddish brown (2.5YR3/4-Moist); , 2.5Y72; Massive grade of structure; Strong consistence; 
	50-90%, Phyllite, coarse fragments; 
	1.4 - 1.6 m	Dark reddish brown (2.5YR3/4-Moist); , 2.5Y72; Massive grade of structure; Strong consistence; 
	90-100%, Phyllite, coarse fragments; 
	Morphological Notes
	Observation Notes
	0-1CM POROUS GRANULAR STRUCTURE.                                                                                        

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B655	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Notes
	BUTLERS KNOB

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B655	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.4 - 0.6
	0.6 - 0.7
	0.7 - 0.9
	0.9 - 1.1
	1.1 - 1.4
	1.4 - 1.6
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.4 - 0.6
	0.6 - 0.7
	0.7 - 0.9
	0.9 - 1.1
	1.1 - 1.4
	1.4 - 1.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.01
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.4 - 0.6
	0.6 - 0.7
	0.7 - 0.9
	0.9 - 1.1
	1.1 - 1.4
	1.4 - 1.6

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B655	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile