Project Name:	GYC
	Project Code:	GYC	Site ID:	B656	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	06/08/69	Elevation:	 168 metres
	Map Ref.:	Sheet No. : 9445   1:100000	Rainfall:	1270
	Northing/Long.:	152.731944444444	Runoff:	Rapid
	Easting/Lat.:	-26.0161111111111	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Rlk	Substrate Material:	Undisturbed soil core, 0.5 m deep,Phyllite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Mesotrophic Red Chromosol     	Principal Profile Form:	Dr3.31
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	No analytical data and little or no knowledge of this soil.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Tall Strata - Tree, , Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.01 m	Very dark greyish brown (10YR3/2-Moist); ; Loam; Weak grade of structure, <2 mm, Granular; Dry;
	 Firm consistence; 
	A21	0.01 - 0.1 m	Reddish brown (5YR5/3-Moist); ; Loam; Weak grade of structure, <2 mm, Granular; Dry; Firm 
	consistence; 20-50%, medium gravelly, 6-20mm, Phyllite, coarse fragments; 
	A22	0.1 - 0.2 m	Reddish brown (5YR5/4-Moist); ; Loam; Weak grade of structure, 5-10 mm, Polyhedral; Dry; Firm 
	consistence; 20-50%, medium gravelly, 6-20mm, Phyllite, coarse fragments; 
	B2	0.2 - 0.5 m	Red (2.5YR4/6-Moist); , 10YR64, 10-20% , 0-5mm, Distinct; , 10-20% , 0-5mm, Distinct; Medium 
	clay; Moderate grade of structure, 2-5 mm; Dry; Very firm consistence; 2-10%, medium gravelly, 
	6-20mm, Phyllite, coarse fragments; 
	C	0.5 - 0.8 m	Red (2.5YR4/8-Moist); , 10YR62; Massive grade of structure; Strong consistence; 90-100%, 
	Phyllite, coarse fragments; 
	0.8 - 1 m	Red (2.5YR4/8-Moist); , 5Y81; Massive grade of structure; Strong consistence; 90-100%, 
	Phyllite, coarse fragments; 
	Morphological Notes
	Observation Notes
	0-10CM POROUS GRANULAR STRUCTURE.                                                                                       
	Site Notes
	NEERDIE

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B656	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.5
	0.5 - 0.8
	0.8 - 1
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.5
	0.5 - 0.8
	0.8 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.01
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.5
	0.5 - 0.8
	0.8 - 1

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B656	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile