Project Name:	GYC
	Project Code:	GYC	Site ID:	B667	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	07/08/69	Elevation:	 122 metres
	Map Ref.:	Sheet No. : 9445   1:100000	Rainfall:	1524
	Northing/Long.:	152.820277777778	Runoff:	Slow
	Easting/Lat.:	-26.1861111111111	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Rlk	Substrate Material:	Undisturbed soil core, 1.4 m deep,Phyllite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	<1.7 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Mesotrophic Red Dermosol     	Principal Profile Form:	Gn3.74
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data and little or no knowledge of this soil.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, , Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.02 m	Very dark greyish brown (10YR3/2-Moist); ; Silty loam; Weak grade of structure, 5-10 mm, 
	Subangular blocky; Dry; Very firm consistence; 
	A12	0.02 - 0.1 m	Brown (7.5YR4/2-Moist); ; Silty loam (Heavy); Weak grade of structure, 5-10 mm, Subangular 
	blocky; Dry; Very firm consistence; 0-2%, fine gravelly, 2-6mm, Phyllite, coarse fragments; 
	A2	0.1 - 0.13 m	Strong brown (7.5YR5/6-Moist); ; Silty clay loam; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Dry; Very firm consistence; 0-2%, fine gravelly, 2-6mm, Phyllite, coarse 
	fragments; 
	B1	0.13 - 0.2 m	Yellowish red (5YR5/6-Moist); , 2-10% , 5-15mm, Faint; , 2-10% , 5-15mm, Faint; Silty medium 
	clay; Moderate grade of structure, 10-20 mm, Polyhedral; Dry; Very firm consistence; 0-2%, fine 
	gravelly, 2-6mm, Phyllite, coarse fragments; 
	B21	0.2 - 0.6 m	Yellowish red (5YR5/6-Moist); , 10YR66, 20-50% , 0-5mm, Distinct; , 2.5YR46, 20-50% , 0-5mm,
	 Distinct; Silty medium clay; Strong grade of structure, 10-20 mm, Polyhedral; Dry; Very firm 
	consistence; 
	B22	0.6 - 0.8 m	Red (2.5YR4/6-Moist); , 10YR66, 20-50% , 0-5mm, Distinct; , 2.5Y71, 20-50% , 0-5mm, Distinct; 
	Medium clay; Moderate grade of structure, 10-20 mm, Polyhedral; Dry; Very firm consistence; 
	B31	0.8 - 1 m	Red (2.5YR4/6-Moist); , 2.5Y71, 20-50% , 5-15mm, Distinct; , 2.5Y64, 20-50% , 5-15mm, 
	Distinct; Silty light clay (Heavy); Moderate grade of structure, Polyhedral; Dry; Very firm 
	consistence; 10-20%, Phyllite, coarse fragments; 
	B32	1 - 1.4 m	Light grey (2.5Y7/1-Moist); , 2.5YR36, 10-20% , 5-15mm, Distinct; , 2.5Y74, 10-20% , 5-15mm, 
	Distinct; Silty medium clay; Moderate grade of structure, Polyhedral; Dry; Firm consistence; 10-
	20%, Phyllite, coarse fragments; 
	C	1.4 - 1.6 m	Weak red (10R5/3-Moist); , 2.5Y71; Massive grade of structure; Very firm consistence; 90-100%, 
	Phyllite, coarse fragments; 
	1.6 - 1.9 m	Light grey (2.5Y7/1-Moist); , 10R53; Massive grade of structure; Very firm consistence; 90-100%,
	 Phyllite, coarse fragments; 

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B667	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	1.9 - 2.6 m	Weak red (10R5/3-Moist); , 2.5Y71; Massive grade of structure; Very firm consistence; 90-100%, 
	Phyllite, coarse fragments; 
	2.6 - 2.8 m	Weak red (2.5YR5/2-Moist); ; Massive grade of structure; Very firm consistence; 90-100%, 
	Phyllite, coarse fragments; 
	2.8 - 2.9 m	Light grey (2.5Y7/1-Moist); , 10R53; Massive grade of structure; Strong consistence; 90-100%, 
	Phyllite, coarse fragments; 
	Morphological Notes
	Observation Notes
	GRADATIONAL RED - YELLOW PODZOLIC SOIL.                                                                                 
	Site Notes
	NEUSAVALE

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B667	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02
	0 - 0.1
	0.1 - 0.13
	0.1 - 0.2
	0.2 - 0.6
	0.6 - 0.8
	0.8 - 1
	1 - 1.4
	1.4 - 1.6
	1.6 - 1.9
	1.9 - 2.6
	2.6 - 2.8
	2.8 - 2.9
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02
	0 - 0.1
	0.1 - 0.13
	0.1 - 0.2
	0.2 - 0.6
	0.6 - 0.8
	0.8 - 1
	1 - 1.4
	1.4 - 1.6
	1.6 - 1.9
	1.9 - 2.6
	2.6 - 2.8
	2.8 - 2.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0 - 0.1
	0.1 - 0.13
	0.1 - 0.2
	0.2 - 0.6
	0.6 - 0.8
	0.8 - 1
	1 - 1.4
	1.4 - 1.6
	1.6 - 1.9
	1.9 - 2.6
	2.6 - 2.8
	2.8 - 2.9

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B667	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile