Project Name:	GYC
	Project Code:	GYC	Site ID:	B673	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	25/09/69	Elevation:	 167 metres
	Map Ref.:	Sheet No. : 9445   1:100000	Rainfall:	1778
	Northing/Long.:	152.965	Runoff:	Very rapid
	Easting/Lat.:	-26.4430555555556	Drainage:	Rapidly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Rlk	Substrate Material:	Undisturbed soil core, 0.74 m deep,Phyllite
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	29.7 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Mesotrophic Red Dermosol     	Principal Profile Form:	Gn3.74
	ASC Confidence:	Great Soil Group:	Xanthozem
	No analytical data and little or no knowledge of this soil.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tussock grass, , . *Species includes - Unknown species, Imperata cylindrica
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.04 m	Dark greyish brown (10YR4/2-Moist); ; Clay loam; Weak grade of structure, Granular; Moist; Weak
	 consistence; 
	A2	0.04 - 0.12 m	Yellowish brown (10YR5/4-Moist); ; Light clay (Light); Weak grade of structure, 10-20 mm, 
	Polyhedral; Moist; Firm consistence; 0-2%, Phyllite, coarse fragments; 
	A2	0.12 - 0.2 m	Yellowish brown (10YR5/6-Moist); ; Light clay; Weak grade of structure, 10-20 mm, Polyhedral; 
	Moist; Firm consistence; 0-2%, medium gravelly, 6-20mm, Phyllite, coarse fragments; 
	B1	0.2 - 0.3 m	Yellowish brown (10YR5/6-Moist); , 5YR56, 10-20% , 15-30mm, Faint; , 10YR66, 10-20% , 15-
	30mm, Faint; Light medium clay; Moderate grade of structure, 10-20 mm, Polyhedral; Smooth-
	ped fabric; Moist; Weak consistence; 0-2%, medium gravelly, 6-20mm, Phyllite, coarse 
	fragments; 
	B2	0.3 - 0.5 m	Yellowish red (5YR5/6-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, 
	Polyhedral; Smooth-ped fabric; Moist; Weak consistence; 10-20%, Phyllite, coarse fragments; 
	B2	0.5 - 0.6 m	Yellowish red (5YR5/6-Moist); , 5YR46; Medium clay; Strong grade of structure, 5-10 mm, 
	Polyhedral; Moist; Weak consistence; 2-10%, Phyllite, coarse fragments; 
	B2	0.6 - 0.74 m	Yellowish red (5YR5/6-Moist); , 2.5YR46, 10-20% , 15-30mm, Faint; , 10-20% , 15-30mm, Faint; 
	Medium clay; Strong grade of structure, 5-10 mm, Polyhedral; Moist; Weak consistence; 2-10%, 
	Phyllite, coarse fragments; 
	C	0.74 - 0.9 m	Yellowish red (5YR5/6-Moist); , 7.5YR54; Massive grade of structure; Strong consistence; 50-
	90%, Phyllite, coarse fragments; 
	0.9 - 1 m	Yellowish red (5YR5/6-Moist); , 7.5YR54; , 2.5Y72; Massive grade of structure; Strong 
	consistence; 90-100%, Phyllite, coarse fragments; 
	1 - 1.11 m	Brownish yellow (10YR6/8-Moist); , 7.5YR66; , 2.5Y72; Massive grade of structure; Strong 
	consistence; 90-100%, Phyllite, coarse fragments; 
	Morphological Notes
	Observation Notes
	0-4CM POROUS GRANULAR STRUCTURE.                                                                                        

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B673	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	MT. COOROY
	Site Notes

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B673	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.9
	0.9 - 1
	1 - 1.11
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.9
	0.9 - 1
	1 - 1.11
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.9
	0.9 - 1
	1 - 1.11

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B673	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile