Project Name:	GYC
	Project Code:	GYC	Site ID:	B692	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	23/10/69	Elevation:	 182 metres
	Map Ref.:	Sheet No. : 9445   1:100000	Rainfall:	1520
	Northing/Long.:	152.820833333333	Runoff:	Very rapid
	Easting/Lat.:	-26.2161111111111	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Rw	Substrate Material:	Undisturbed soil core, 0.8 m deep,Diorite 
	Land Form
	Rel/Slope Class: 	Steep hills 90-300m 32-56%	Pattern Type:	Hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	26.2 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Dermosol     	Principal Profile Form:	Gn3.11
	ASC Confidence:	Great Soil Group:	Prairie soil
	No analytical data and little or no knowledge of this soil.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tussock grass, , . *Species includes - Unknown species, Chloris species
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.09 m	Dark reddish brown (5YR3/2-Moist); ; Fine sandy clay loam; Moderate grade of structure, 5-10 
	mm, Polyhedral; Moist; Weak consistence; 
	A12	0.09 - 0.18 m	Dark reddish brown (5YR3/3-Moist); ; Fine sandy clay loam (Heavy); Moderate grade of structure, 
	5-10 mm, Polyhedral; Moist; Weak consistence; 
	A3	0.18 - 0.24 m	Dark reddish brown (5YR3/4-Moist); ; Fine sandy medium clay; Moderate grade of structure, 5-10 
	mm, Polyhedral; Moist; Weak consistence; 
	B2	0.24 - 0.3 m	Dark red (2.5YR3/6-Moist); ; Light medium clay; Strong grade of structure, Polyhedral; Moist; 
	Firm consistence; 
	B2	0.3 - 0.64 m	Dark red (2.5YR3/6-Moist); ; Medium heavy clay; Strong grade of structure, Polyhedral; Moist; 
	Firm consistence; 
	B3	0.64 - 0.8 m	Dark red (2.5YR3/6-Moist); ; Sandy light clay; Weak grade of structure, Polyhedral; Moist; Weak 
	consistence; 
	C	0.8 - 1.1 m	Dark red (2.5YR3/6-Moist); , 5YR36; Sandy clay loam; Massive grade of structure; Moist; Weak 
	consistence; 
	1.1 - 1.6 m	Yellowish red (5YR3/6-Moist); , 10YR54; Sandy loam; Massive grade of structure; Weak 
	consistence; 
	1.6 - 1.9 m	Brown (10YR4/3-Moist); , 10YR54; , 5YR36; Loamy coarse sand; Massive grade of structure; 
	Morphological Notes
	Observation Notes
	Site Notes
	THE GAP

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B692	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1
	0.1 - 0.2
	0.18 - 0.24
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.8
	0.8 - 1.1
	1.1 - 1.6
	1.6 - 1.9
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.2
	0.18 - 0.24
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.8
	0.8 - 1.1
	1.1 - 1.6
	1.6 - 1.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.18 - 0.24
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.8
	0.8 - 1.1
	1.1 - 1.6
	1.6 - 1.9

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B692	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile