Project Name:	GYC
	Project Code:	GYC	Site ID:	B695	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	21/10/69	Elevation:	 244 metres
	Map Ref.:	Sheet No. : 9445   1:100000	Rainfall:	1397
	Northing/Long.:	152.798611111111	Runoff:	Moderately rapid
	Easting/Lat.:	-26.4227777777778	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Tv	Substrate Material:	Undisturbed soil core, 0.5 m deep,Basalt 
	Land Form
	Rel/Slope Class: 	Steep hills 90-300m 32-56%	Pattern Type:	Hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	1.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Ferrosol     	Principal Profile Form:	Gn3.11
	ASC Confidence:	Great Soil Group:	Prairie soil
	No analytical data and little or no knowledge of this soil.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Chloris gayana, Bothriochloa species
	Tall Strata - Shrub, , . *Species includes - Alphitonia excelsa, Owenia venosa
	Surface Coarse Fragments:	20-50%, stony, 200-600mm, , Basalt
	Profile Morphology
	A11	0 - 0.03 m	Very dusky red (2.5YR2/2-Moist); ; Loam (Heavy); Strong grade of structure, <2 mm, Granular; 
	Moist; Weak consistence; 2-10%, medium gravelly, 6-20mm, Basalt, coarse fragments; 
	A12	0.03 - 0.1 m	Dark reddish brown (5YR2/2-Moist); ; Clay loam; Moderate grade of structure, 2-5 mm, 
	Polyhedral; Moist; Weak consistence; 2-10%, medium gravelly, 6-20mm, Basalt, coarse 
	fragments; 
	B1	0.1 - 0.2 m	Dark reddish brown (5YR3/3-Moist); ; Light clay; Moderate grade of structure, 2-5 mm, 
	Polyhedral; Moist; Weak consistence; 10-20%, coarse gravelly, 20-60mm, Basalt, coarse 
	fragments; 
	B2	0.2 - 0.4 m	Dark reddish brown (5YR3/4-Moist); ; Light medium clay; Moderate grade of structure, 2-5 mm, 
	Polyhedral; Moist; Firm consistence; 2-10%, medium gravelly, 6-20mm, Basalt, coarse 
	fragments; 
	B3	0.4 - 0.5 m	Dark reddish brown (5YR3/4-Moist); , 5YR44; Medium heavy clay; 2-5 mm, Polyhedral; Moist; 
	Firm consistence; 20-50%, Basalt, coarse fragments; 
	Morphological Notes
	Observation Notes
	LANDFORM - CREST OF SHALLOW SADDLE. 0-3CM POROUS GRANULAR STRUCTURE.                                                    
	Site Notes
	MIDDLE CK DIV.

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B695	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.4 - 0.5
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.4 - 0.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.4 - 0.5

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B695	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile