Project Name:	IDF
	Project Code:	IDF	Site ID:	T470	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	M.G. Cannon	Locality:	TRIAL AREA 3 'SHELL PROJECT' INGHAM: SITE 
	301
	Date Desc.:	22/09/86	Elevation:	No Data
	Map Ref.:	Sheet No. : 8060   1:100000	Rainfall:	0
	Northing/Long.:	145.911111111111	Runoff:	Very slow
	Easting/Lat.:	-18.6222222222222	Drainage:	Poorly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Sheet-flood fan
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	Level
	Slope:	<1 % 	Aspect:	70 degrees
	Surface Soil Condition (dry):	Hardsetting, Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Sodic Eutrophic Grey Kandosol     	Principal Profile Form:	Gn2.91
	ASC Confidence:	Great Soil Group:	Soloth
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.03 m	Dark greyish brown (10YR4/2-Moist); Light grey (10YR7/2-Dry); ; Fine sandy clay loam; Weak 
	grade of structure, 2-5 mm, Cast; Earthy fabric; Moist; Weak consistence; Common, fine (1-
	2mm) roots; Clear change to - 
	A21cb	0.03 - 0.1 m	Greyish brown (10YR5/2-Moist); White (10YR8/2-Dry); , 2-10% , 5-15mm, Prominent; , 2-10% , 5-
	15mm, Prominent; Sandy clay loam; Massive grade of structure; Earthy fabric; Moist; Weak 
	consistence; Few, fine (1-2mm) roots; Gradual change to - 
	B11sb	0.1 - 0.21 m	Light brownish grey (10YR6/2-Moist); White (10YR8/1-Dry); , 10YR68, 20-50% , 5-15mm, 
	Distinct; , 20-50% , 5-15mm, Distinct; Clay loam, fine sandy; Massive grade of structure; Earthy 
	fabric; Moist; Weak consistence; Few, fine (1-2mm) roots; Gradual change to - 
	B12	0.21 - 0.36 m	Light grey (10YR7/2-Moist); , 10YR78, 20-50% , 5-15mm, Prominent; , 20-50% , 5-15mm, 
	Prominent; Medium clay; Massive grade of structure; Earthy fabric; Moist; Firm consistence; 0-
	2%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; Few, fine (1-2mm) roots;
	 Diffuse change to - 
	B21	0.36 - 0.75 m	Light brownish grey (10YR6/2-Moist); , 10YR68, 20-50% , 5-15mm, Prominent; , 10R48, 20-50% ,
	 5-15mm, Prominent; Medium heavy clay; Massive grade of structure; Earthy fabric; Moist; Firm 
	consistence; 2-10%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; Few, 
	fine (1-2mm) roots; Diffuse change to - 
	B22	0.75 - 1.15 m	Grey (2.5Y6/1-Moist); , 10YR68, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, Distinct; 
	Medium heavy clay; Weak grade of structure, 10-20 mm, Angular blocky; Massive grade of 
	structure; Earthy fabric; Moist; Very firm consistence; 10-20%, fine gravelly, 2-6mm, angular, 
	dispersed, Quartz, coarse fragments; Common (10 - 20 %), Manganiferous, Coarse (6 - 20 mm), 
	Nodules; Few, medium (2-5mm) roots; Diffuse change to - 
	B23	1.15 - 1.47 m	Light grey (2.5Y7/1-Moist); , 10YR68, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; 
	Sandy medium clay (Heavy); Moderate grade of structure, 50-100 mm, Angular blocky; Massive 
	grade of structure; Smooth-ped fabric; Moist; Strong consistence; 0-2%, fine gravelly, 2-6mm, 
	angular, dispersed, Quartz, coarse fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 
	mm), Nodules; Few, fine (1-2mm) roots; Diffuse change to - 

	Project Name:	IDF
	Project Code:	IDF	Site ID:	T470	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	1.47 - 1.77 m	Light grey (2.5Y7/1-Moist); , 10YR68, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; 
	Medium heavy clay; Moderate grade of structure, 50-100 mm, Angular blocky; Massive grade of 
	structure; Smooth-ped fabric; Strong consistence; 0-2%, fine gravelly, 2-6mm, angular, 
	dispersed, Quartz, coarse fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; Few, fine (1-2mm) roots; Diffuse change to - 
	B24	1.77 - 2 m	Grey (10YR6/1-Moist); , 10YR68, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; Sandy
	 medium clay; Massive grade of structure; Earthy fabric; Moderately moist; Strong consistence; 
	2-10%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; Very few (0 - 2 %), 
	Manganiferous, Medium (2 -6 mm), Nodules; Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	STRONG ROOTLINE GLEYING BELOW 177CM:                                                                                    
	Site Notes
	LANERCOST

	Project Name:	IDF
	Project Code:	IDF	Site ID:	T470	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	5.4A	 0.05A	 2.03H	 1.04	 0.4	 0.16	 3.2A	 3.6F	5.00
	6A	 5C	3.20
	0.03 - 0.1	5.4A	 0.04A
	0.1 - 0.21	5.4A	 0.02A	 0.09H	 0.73	 0.09	 0.22	 7.7A	 1.1F	2.86
	 3C	7.33
	0.21 - 0.36	5.7A	 0.02A	 3.26H	 4.07	 0.28	 0.15	 2.4A	 7.8F	6.25
	 7C	2.14
	0.36 - 0.75	6A	 0.02A
	0.75 - 1.15	6A	 0.04A	 0.72H	 3.51	 0.07	 0.76	 5.4A	 5.1F	14.07
	 6C	12.67
	1.15 - 1.47	5.9A	 0.1A
	1.47 - 1.77	6.1A	 0.16A
	1.77 - 2	6.4A	 0.17A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 1.23C	 12A	 0.05A	 1	 30A	 39	 22	 9
	 0.99C	 7B
	0.03 - 0.1	 0.061C	 8A	 0.03A	 2	 30A	 32	 29	 9
	 4B
	0.1 - 0.21	 0.03C	 8A	 0.03A	 4	 29A	 33	 28	 10
	 3B
	0.21 - 0.36	 0.02C	 0.03A	 8	 27A	 30	 24	 19
	0.36 - 0.75	 7	 32A	 22	 18	 28
	0.75 - 1.15	 7A	 8	 31A	 24	 16	 28
	 2B
	1.15 - 1.47	 3	 27A	 23	 24	 25
	1.47 - 1.77	 2	 20A	 24	 27	 29
	1.77 - 2	 11	 30A	 23	 23	 24
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.1
	0.1 - 0.21
	0.21 - 0.36
	0.36 - 0.75
	0.75 - 1.15
	1.15 - 1.47
	1.47 - 1.77
	1.77 - 2

	Project Name:	IDF
	Project Code:	IDF	Site ID:	T470	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J1	Effective CEC
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)