Project Name:	LBV
	Project Code:	LBV	Site ID:	B106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.B. Stirk	Locality:
	Date Desc.:	21/11/50	Elevation:	 14 metres
	Map Ref.:	Sheet No. : 8358   1:100000	Rainfall:	850
	Northing/Long.:	147.166666666667	Runoff:	Very slow
	Easting/Lat.:	-19.8	Drainage:	Very poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Cza	Substrate Material:	Auger boring, 2 m deep,Porous, 
	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endohypersodic Epipedal Grey Vertosol     	Principal Profile Form:	Ug5.24
	ASC Confidence:	Great Soil Group:	Grey clay
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , Very sparse. *Species includes - Ophiurous exaltatus
	Tall Strata - Tree, , Isolated plants. *Species includes - Eucalyptus tessellaris
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Grey (2.5Y5/0-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Angular blocky; Dry;
	 Strong consistence; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Field pH 
	5.8 (pH meter); Clear change to - 
	B2	0.05 - 0.46 m	Dark grey (2.5Y4/0-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, Angular blocky; 
	Dry; Strong consistence; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Field 
	pH 7.1 (pH meter); Diffuse change to - 
	B2	0.46 - 0.81 m	Grey (10YR5/1-Moist); , 7.5YR68; Heavy clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Dry; Strong consistence; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; 
	Field pH 7.4 (pH meter); Diffuse change to - 
	B2	0.81 - 1.02 m	Light yellowish brown (10YR6/4-Moist); , 10YR51; Heavy clay; Moderate grade of structure, 20-50
	 mm, Angular blocky; Moist; Firm consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 
	mm), Nodules; 
	Morphological Notes
	Observation Notes
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.8A	 0.09C
	0.05 - 0.46	7.1A	 0.04C	 14.9K	 17.3	 0.38	 2.4	 4.5E	 39.5E
	0.46 - 0.81	7.4A	 0.14C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 1.5F	 6C	 0.018F	 0.11B	 1D	 17	 30	 49
	0.05 - 0.46	<1D	 13	 28	 58
	0.46 - 0.81
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.46
	0.46 - 0.81

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6_DC	Organic carbon (%) - Dry combustion
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance