Project Name:	LBV
	Project Code:	LBV	Site ID:	B14	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	13/10/48	Elevation:	 20 metres
	Map Ref.:	Sheet No. : 8358   1:100000	Rainfall:	800
	Northing/Long.:	147.233333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-19.8333333333333	Drainage:	Well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Cza	Substrate Material:	Auger boring, 2 m deep,Porous, 
	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	No Data	Relief:	2 metres
	Elem. Type:	Levee	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Mesotrophic Yellow Kandosol     	Principal Profile Form:	Dy2.72
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , Closed or dense. *Species includes - Heteropogon contortus
	Mid Strata - Shrub, , . *Species includes - Planchonia careya
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.2 m	Greyish brown (10YR5/2-Moist); ; Loamy fine sand; Massive grade of structure; Earthy fabric; 
	Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Very weak consistence; Field pH 6.9 (pH 
	meter); Many, fine (1-2mm) roots; Diffuse change to - 
	A2	0.2 - 0.36 m	Pale brown (10YR6/3-Moist); , 10YR51; Fine sand; Massive grade of structure; Earthy fabric; 
	Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Very weak consistence; Field pH 6.8 (pH 
	meter); Many, fine (1-2mm) roots; Diffuse change to - 
	A3	0.36 - 0.69 m	Light yellowish brown (10YR6/4-Moist); , 10YR51; Clayey fine sand; Massive grade of structure; 
	Earthy fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Very weak consistence; 
	Field pH 6.9 (pH meter); Common, fine (1-2mm) roots; Diffuse change to - 
	A3	0.69 - 1.04 m	Light yellowish brown (10YR6/4-Moist); , 10YR51; Fine sand; Massive grade of structure; Earthy 
	fabric; Few (<1 per 100mm2) Fine (1-2mm) macropores, Moderately moist; Very weak 
	consistence; Field pH 6.9 (pH meter); Few, fine (1-2mm) roots; Clear change to - 
	B2	1.07 - 1.42 m	Brownish yellow (10YR6/6-Moist); , 7.5YR54; Fine sandy clay loam; Massive grade of structure; 
	Earthy fabric; Moderately moist; Weak consistence; Field pH 6.8 (pH meter); Diffuse change to - 
	B3	1.42 - 1.68 m	Brownish yellow (10YR6/6-Moist); , 7.5YR54; Fine sand; Massive grade of structure; Moist; Very 
	weak consistence; Field pH 6.9 (pH meter); Diffuse change to - 
	B3	1.68 - 2.13 m	Brownish yellow (10YR6/6-Moist); , 7.5YR54; Fine sand; Massive grade of structure; Moist; Very 
	weak consistence; Field pH 7.2 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B14	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.2	6.9H	 0.01B	 4.4K	 1.2	 0.42	 0.13	 1.9D	 8E
	0.2 - 0.36	6.8H	 0.01B
	0.36 - 0.69	6.9H	 0.01B
	0.69 - 1.04	6.9H	 0.01B
	1.07 - 1.42	6.8H	 0.01B	 6.1K	 2.6	 0.32	 0.21	 1.6D	 10.8E
	1.42 - 1.68	6.9H	 0.01B
	1.68 - 2.13	7.2H	 0.01B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.2	 0.73E	 91C	 0.027F	 0.05B	 10C	 72	 10	 7
	0.2 - 0.36	 0.03B	 8C	 71	 9	 9
	0.36 - 0.69	 10C	 62	 12	 13
	0.69 - 1.04	 11C	 65	 11	 12
	1.07 - 1.42	 10C	 62	 8	 17
	1.42 - 1.68	 10C	 66	 8	 14
	1.68 - 2.13	 4C	 67	 9	 17
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.2
	0.2 - 0.36
	0.36 - 0.69
	0.69 - 1.04
	1.07 - 1.42
	1.42 - 1.68
	1.68 - 2.13

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B14	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded