Project Name:	LBV
	Project Code:	LBV	Site ID:	B16	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R. Hare	Locality:
	Date Desc.:	14/10/48	Elevation:	 40 metres
	Map Ref.:	Sheet No. : 8358   1:100000	Rainfall:	800
	Northing/Long.:	147.115277777778	Runoff:	Moderately rapid
	Easting/Lat.:	-19.8383333333333	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Sdr	Substrate Material:	Auger boring, 1.8 m deep,Igneous rock 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached Eutrophic Grey Kandosol     	Principal Profile Form:	Uc2.22
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 3.01-6m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.23 m	Grey (10YR5/1-Moist); ; Coarse sand; Massive grade of structure; Dry; Very weak consistence; 
	Field pH 6.3 (pH meter); Gradual change to - 
	A2	0.25 - 0.41 m	Grey (10YR6/1-Moist); ; Coarse sand; Massive grade of structure; Dry; Very weak consistence; 
	Field pH 6.4 (pH meter); Gradual change to - 
	A2	0.41 - 0.56 m	Light grey (10YR7/2-Moist); ; Coarse sand; Massive grade of structure; Moderately moist; Very 
	weak consistence; Field pH 6.4 (pH meter); Gradual change to - 
	A3	0.56 - 0.86 m	Very pale brown (10YR7/4-Moist); ; Clay loam, sandy; Massive grade of structure; Moderately 
	moist; Very weak consistence; 0-2%, fine gravelly, 2-6mm, Substrate material, coarse 
	fragments; Field pH 6.3 (pH meter); Gradual change to - 
	B1	0.86 - 1.42 m	Grey (10YR6/1-Moist); ; Clay loam, coarse sandy; Massive grade of structure; Moderately moist; 
	Weak consistence; 2-10%, fine gravelly, 2-6mm, Substrate material, coarse fragments; Field pH
	 5.8 (pH meter); Gradual change to - 
	B1	1.42 - 1.68 m	Light grey (10YR7/1-Moist); ; Clay loam, coarse sandy; Massive grade of structure; Moderately 
	moist; Weak consistence; 50-90%, fine gravelly, 2-6mm, Substrate material, coarse fragments; 
	Gradual change to - 
	C	1.68 - 1.78 m	; 
	Morphological Notes
	C	Very light grey decomposing very coarse sandy rock:
	Observation Notes
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B16	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.23	6.3H	 0.006B
	0.25 - 0.41	6.4H	 0.006B
	0.41 - 0.56	6.4H	 0.006B
	0.56 - 0.86	6.3H	 0.006B
	0.86 - 1.42	5.8H	 0.008B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.23	 2C	 0.004F	 0.024B	 52C	 38	 8	 3
	0.25 - 0.41
	0.41 - 0.56	 37C	 46	 8	 8
	0.56 - 0.86
	0.86 - 1.42	 49C	 24	 8	 19
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.23
	0.25 - 0.41
	0.41 - 0.56
	0.56 - 0.86
	0.86 - 1.42

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B16	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded