Project Name:	LBV
	Project Code:	LBV	Site ID:	B28	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	I. Nankivell	Locality:
	Date Desc.:	17/08/49	Elevation:	 17 metres
	Map Ref.:	Sheet No. : 8358   1:100000	Rainfall:	750
	Northing/Long.:	147.099444444445	Runoff:	Slow
	Easting/Lat.:	-19.7805555555556	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 CZA	Substrate Material:	Auger boring, 1 m deep,Slightly porous, 
	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Subnatric Black Sodosol     	Principal Profile Form:	Dd1.43
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , Mid-dense. *Species includes - Heteropogon contortus, Chloris species
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus papuana, Eucalyptus tessellaris, Eucalyptus 
	polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.09 m	Grey (10YR5/1-Moist); ; Loam; Massive grade of structure; Coarse, (10 - 20) mm crack; Dry; Weak
	 consistence; Field pH 6.3 (pH meter); Abrupt change to - 
	B21	0.1 - 0.33 m	Very dark grey (10YR3/1-Moist); ; Heavy clay; Moderate grade of structure, 100-200 mm, 
	Prismatic; Moderate grade of structure, 20-50 mm, Angular blocky; Coarse, (10 - 20) mm crack; 
	Dry; Strong consistence; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; Field pH 
	7.2 (pH meter); Diffuse change to - 
	B22	0.36 - 0.48 m	Very dark grey (10YR3/1-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Coarse, (10 - 20) mm crack; Dry; Strong consistence; Very few (0 - 2 %), Manganiferous, 
	Fine (0 - 2 mm), Nodules; Very few (0 - 2 %), Calcareous, , Nodules; Field pH 8.7 (pH meter); 
	Diffuse change to - 
	B23	0.48 - 0.61 m	Brown (10YR5/3-Moist); , 10YR42; Heavy clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Coarse, (10 - 20) mm crack; Moist; Very firm consistence; 0-2%, fine gravelly, 2-6mm, 
	Quartz, coarse fragments; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; Few (2 - 
	10 %), Calcareous, , Nodules; Field pH 9.1 (pH meter); Diffuse change to - 
	B3	0.61 - 0.79 m	Greyish brown (2.5Y5/3-Moist); ; Light clay; Weak grade of structure, 10-20 mm, Angular blocky; 
	Very coarse, (20 - 50) mm crack; Moist; Weak consistence; Very few (0 - 2 %), Manganiferous, 
	Fine (0 - 2 mm), Nodules; Very few (0 - 2 %), Calcareous, , Nodules; Field pH 9.1 (pH meter); 
	Diffuse change to - 
	B3	0.79 - 1.09 m	Greyish brown (2.5Y5/3-Moist); ; Sandy medium clay; Weak grade of structure, 10-20 mm, 
	Angular blocky; Moist; Weak consistence; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), 
	Nodules; Very few (0 - 2 %), Calcareous, , Nodules; Field pH 8.9 (pH meter); Diffuse change to - 
	C	1.09 - 1.68 m	Greyish brown (2.5Y5/3-Moist); , 10YR52; Sandy medium clay; Massive grade of structure; Very 
	few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; Very few (0 - 2 %), Calcareous, , 
	Nodules; Field pH 8.9 (pH meter); 
	Morphological Notes
	Observation Notes

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B28	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	MICRO-RELIEF HEXAGONAL CRACKING AROUND COLUMNS 150-200MM IN DIAMETER                                                    
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B28	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.09	6.3H	 0.02B	 3.6K	 2.6	 0.15	 0.3	 4.3D	 11E
	0.1 - 0.33	7.3H	 0.04B	 9.3K	 7.8	 0.12	 2.9	 3.4D	 23.5E
	0.36 - 0.48	8.7H	 0.1B	 8.3K	 8.9	 0.27	 4.9	 22.5E
	0.48 - 0.61	9.1H	 0.27B
	0.61 - 0.79	9.1H	 0.26B	 2.3K	 9.2	 0.23	 6	 17.7E
	0.79 - 1.09	8.9H	 0.2B
	1.09 - 1.68	8.9H	 0.17B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.09	 0.79C	 0.89E	 7C	 0.009F	 0.06B	 14C	 44	 22	 17
	0.1 - 0.33	 8C	 30	 21	 41
	0.36 - 0.48	 0.12C	 3	 9C	 31	 23	 39
	0.48 - 0.61	 0.79C	 5	 8C	 29	 24	 41
	0.61 - 0.79	 0.4C	 3	 12C	 40	 18	 31
	0.79 - 1.09	 0.06C
	1.09 - 1.68	 0.092C	 2	 15C	 45	 15	 27
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.09
	0.1 - 0.33
	0.36 - 0.48
	0.48 - 0.61
	0.61 - 0.79
	0.79 - 1.09
	1.09 - 1.68

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B28	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded