Project Name:	LBV
	Project Code:	LBV	Site ID:	B3	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/10/48	Elevation:	 19 metres
	Map Ref.:	Sheet No. : 8358   1:100000	Rainfall:	800
	Northing/Long.:	147.216666666667	Runoff:	Very slow
	Easting/Lat.:	-19.7805555555556	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Cza	Substrate Material:	Auger boring, 1.5 m deep,Porous, 
	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Subnatric Grey Sodosol     	Principal Profile Form:	Dy2.43
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.15 m	Dark grey (10YR4/1-Moist); ; Loam; Massive grade of structure; Common (1-5 per 100mm2) Fine 
	(1-2mm) macropores, Dry; Weak consistence; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 
	mm), Concretions; Field pH 6.2 (pH meter); Diffuse change to - 
	A2	0.15 - 0.23 m	Light grey (10YR7/2-Moist); ; Fine sandy loam (Heavy); Massive grade of structure; Common (1-5 
	per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; Common (10 - 20 %), 
	Manganiferous, Medium (2 -6 mm), Concretions; Field pH 6.6 (pH meter); Clear, Irregular change
	 to - 
	B21	0.25 - 0.41 m	Greyish brown (2.5Y5/2-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Dry; Strong consistence; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), Concretions; 
	Field pH 7.7 (pH meter); Diffuse change to - 
	B22	0.41 - 0.56 m	Greyish brown (2.5Y5/2-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Dry; Strong consistence; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), Concretions; 
	Field pH 8.7 (pH meter); Diffuse change to - 
	B23	0.56 - 0.66 m	Light brownish grey (2.5Y6/2-Moist); ; Light clay; Moderate grade of structure, 20-50 mm, Angular
	 blocky; Dry; Strong consistence; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), Concretions; 
	Field pH 9 (pH meter); Diffuse change to - 
	B24	0.69 - 0.91 m	Brown (10YR4/3-Moist); ; Light medium clay; Weak grade of structure, 20-50 mm, Angular 
	blocky; Moderately moist; Strong consistence; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), 
	Concretions; Field pH 8.8 (pH meter); Diffuse change to - 
	BC	0.97 - 1.32 m	Greyish brown (10YR5/2-Moist); ; Light medium clay; Weak grade of structure, 20-50 mm, 
	Angular blocky; Moderately moist; Strong consistence; Few (2 - 10 %), Manganiferous, Fine (0 - 
	2 mm), Concretions; Field pH 8.8 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B3	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	6.2H	 0.007B	 3.8K	 1.9	 0.36	 0.09	 3.7D	 9.8E
	0.15 - 0.23	6.6H	 0.006B
	0.25 - 0.41	7.7H	 0.02B	 11.5K	 10.2	 0.2	 1.64	 2.6D	 26.1E
	0.41 - 0.56	8.7H	 0.037B
	0.56 - 0.66	9H	 0.058B	 8.6K	 5.9	 0.18	 1.3	 15.9E
	0.69 - 0.91	8.8H	 0.09B
	0.97 - 1.32	8.8H	 0.041B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 0.73E	 8C	 0.014F	 0.055B	 4D	 52	 29	 13
	0.15 - 0.23	 0.029B	 4D	 52	 34	 12
	0.25 - 0.41	 0.5E	 0.044B	 4D	 37	 20	 38
	0.41 - 0.56	 0.03C	 6D	 43	 22	 31
	0.56 - 0.66	 0.12C	 6D	 46	 16	 29
	0.69 - 0.91	 0.24C	 4D	 39	 16	 43
	0.97 - 1.32	 0.04C	 12D	 28	 29	 32
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.23
	0.25 - 0.41
	0.41 - 0.56
	0.56 - 0.66
	0.69 - 0.91
	0.97 - 1.32

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B3	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance