Project Name:	LBV
	Project Code:	LBV	Site ID:	B59	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	25/10/50	Elevation:	 75 metres
	Map Ref.:	Sheet No. : 8358   1:100000	Rainfall:	800
	Northing/Long.:	147.383333333333	Runoff:	Very slow
	Easting/Lat.:	-19.85	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 SDR	Substrate Material:	Auger boring, 1.6 m deep,Porous, 
	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous Epipedal Grey Vertosol     	Principal Profile Form:	Ug5.16
	ASC Confidence:	Great Soil Group:	Black earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	AB	0 - 0.13 m	Dark grey (10YR4/1-Moist); ; Heavy clay; Weak grade of structure, 10-20 mm, Angular blocky; Dry;
	 Firm consistence; 0-2%, fine gravelly, 2-6mm, rounded, Substrate material, coarse fragments; 
	Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 7 (pH meter); Gradual 
	change to - 
	B2	0.13 - 0.48 m	Dark greyish brown (10YR4/2-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Moist; Firm consistence; 0-2%, fine gravelly, 2-6mm, rounded, Substrate 
	material, coarse fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Very
	 few (0 - 2 %), Calcareous, Coarse (6 - 20 mm), Nodules; Field pH 8.8 (pH meter); Gradual 
	change to - 
	B2	0.48 - 0.91 m	Dark greyish brown (10YR4/2-Moist); ; Heavy clay; Moderate grade of structure, Lenticular; Moist; 
	Firm consistence; 0-2%, fine gravelly, 2-6mm, rounded, Substrate material, coarse fragments; 
	Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Few (2 - 10 %), Calcareous, 
	Medium (2 -6 mm), Nodules; Field pH 9 (pH meter); Gradual change to - 
	B2	0.97 - 1.22 m	Dark greyish brown (10YR4/2-Moist); ; Heavy clay; Moderate grade of structure, Lenticular; Moist; 
	Firm consistence; 0-2%, fine gravelly, 2-6mm, rounded, Substrate material, coarse fragments; 
	Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Few (2 - 10 %), Calcareous, 
	Coarse (6 - 20 mm), Nodules; Field pH 9 (pH meter); Gradual change to - 
	B3	1.37 - 1.63 m	Light yellowish brown (10YR6/4-Moist); ; Medium heavy clay; Weak grade of structure, 
	Lenticular; Moist; Firm consistence; Common (10 - 20 %), Calcareous, Coarse (6 - 20 mm), 
	Nodules; Field pH 9 (pH meter); Gradual change to - 
	C	1.63 - 2.03 m	Light yellowish brown (10YR6/4-Moist); ; Sandy medium clay; Massive grade of structure; 
	Moderately moist; Weak consistence; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Nodules; 
	Field pH 9 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B59	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	7H	 0.02B
	0.13 - 0.48	8.8H	 0.06B
	0.48 - 0.91	9H	 0.15B
	0.97 - 1.22	9H	 0.24B
	1.37 - 1.63	9H	 0.24B
	1.63 - 2.03	9H	 0.15B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	 1.3E	 3C	 0.01F	 0.09B	 2	 15C	 24	 14	 45
	0.13 - 0.48
	0.48 - 0.91
	0.97 - 1.22
	1.37 - 1.63
	1.63 - 2.03
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.48
	0.48 - 0.91
	0.97 - 1.22
	1.37 - 1.63
	1.63 - 2.03

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B59	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded