Project Name:	LBV
	Project Code:	LBV	Site ID:	B60	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	25/10/50	Elevation:	 19 metres
	Map Ref.:	Sheet No. : 8358   1:100000	Rainfall:	800
	Northing/Long.:	147.4	Runoff:	Moderately rapid
	Easting/Lat.:	-19.7833333333333	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 PZG	Substrate Material:	Auger boring, 1.8 m deep,Non-porous, 
	dense, Igneous rock (unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol     	Principal Profile Form:	Dr2.12
	ASC Confidence:	Great Soil Group:	Red-brown earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , Sparse. *Species includes - Heteropogon contortus
	Mid Strata - Shrub, , Sparse. *Species includes - Planchonia careya, Eucalyptus papuana
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus drepanophylla, Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Brown (7.5YR4/2-Moist); ; Clay loam; Weak grade of structure, 5-10 mm, Angular blocky; Moist; 
	Very weak consistence; 2-10%, medium gravelly, 6-20mm, angular, Substrate material, coarse 
	fragments; Field pH 6.2 (pH meter); Gradual change to - 
	A12	0.1 - 0.2 m	Brown (7.5YR4/2-Moist); ; Light clay; Weak grade of structure, 5-10 mm, Angular blocky; Moist; 
	Very weak consistence; 0-2%, medium gravelly, 6-20mm, angular, Substrate material, coarse 
	fragments; Field pH 6.1 (pH meter); Clear, Smooth change to - 
	B21	0.2 - 0.48 m	Dark reddish brown (2.5YR3/4-Moist); ; Heavy clay; Moderate grade of structure, 10-20 mm, 
	Angular blocky; Moist; Weak consistence; 2-10%, medium gravelly, 6-20mm, angular, Substrate 
	material, coarse fragments; Field pH 6.6 (pH meter); Diffuse change to - 
	B22	0.48 - 0.91 m	Dark red (2.5YR3/6-Moist); ; Heavy clay; Moderate grade of structure, 10-20 mm, Angular blocky; 
	Moist; Weak consistence; 0-2%, medium gravelly, 6-20mm, angular, Substrate material, coarse 
	fragments; Field pH 7 (pH meter); Diffuse change to - 
	B22	0.91 - 1.37 m	Dark red (2.5YR3/6-Moist); ; Heavy clay; Moderate grade of structure, 10-20 mm, Angular blocky; 
	Moist; Weak consistence; 0-2%, medium gravelly, 6-20mm, angular, Substrate material, coarse 
	fragments; Field pH 7 (pH meter); Diffuse change to - 
	B3	1.37 - 1.6 m	Yellowish brown (10YR5/6-Moist); , 10YR64; Clay loam; Weak grade of structure, Angular 
	blocky; Moist; Very weak consistence; Field pH 7.4 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B60	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.2H	 0.02B
	0.1 - 0.2	6.1H	 0.01B
	0.2 - 0.48	6.6H	 0.01B	 8.3K	 4	 0.12	 0.07	 6.9D	 19.4E
	0.48 - 0.91	7H	 0.01B
	0.91 - 1.37	7H	 0.01B	 9.8K	 6.2	 0.08	 0.19	 5.6D	 21.9E
	1.37 - 1.6
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.7E	 11C	 0.037D	 0.09B	 3	 5C	 58	 8	 26
	0.1 - 0.2	 1	 22C	 31	 7	 38
	0.2 - 0.48	 3	 9C	 16	 6	 68
	0.48 - 0.91	 2	 9C	 17	 7	 67
	0.91 - 1.37	 5C	 16	 6	 71
	1.37 - 1.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.48
	0.48 - 0.91
	0.91 - 1.37
	1.37 - 1.6

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B60	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded