Project Name:	LBV
	Project Code:	LBV	Site ID:	B68	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	27/09/50	Elevation:	 75 metres
	Map Ref.:	Sheet No. : 8358   1:100000	Rainfall:	850
	Northing/Long.:	147.366666666667	Runoff:	Slow
	Easting/Lat.:	-19.85	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 SDR	Substrate Material:	Auger boring, 1.7 m deep,Non-porous, 
	dense, Igneous rock (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Mottled-Mesonatric Grey Sodosol     	Principal Profile Form:	Dy3.43
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , Isolated clumps. *Species includes - Heteropogon contortus, Chloris species
	Mid Strata - Shrub, , Isolated plants. *Species includes - Acacia farnesiana, Eremophila mitchellii
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus papuana, Grevillea striata
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.04 m	Light brownish grey (10YR6/2-Moist); ; Loam; Weak grade of structure, Platy; , Angular blocky; 
	Dry; Weak consistence; 2-10%, medium gravelly, 6-20mm, subangular, Quartz, coarse 
	fragments; Field pH 7 (pH meter); Clear change to - 
	A2	0.04 - 0.08 m	White (10YR8/1-Moist); ; Sandy loam; Massive grade of structure; Dry; Weak consistence; 0-2%,
	 fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; Very few (0 - 2 %), Manganiferous, 
	Medium (2 -6 mm), ; Field pH 7.2 (pH meter); Abrupt, Irregular change to - 
	B21	0.08 - 0.2 m	Dark greyish brown (10YR4/2-Moist); , 2.5Y52; Heavy clay; Strong grade of structure, 100-200 
	mm, Columnar; Dry; Strong consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse
	 fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), ; Field pH 7.2 (pH meter); 
	Gradual change to - 
	B22	0.2 - 0.38 m	Dark grey (10YR4/1-Moist); , 2.5Y42; Heavy clay; Moderate grade of structure, 20-50 mm, Angular
	 blocky; Dry; Strong consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse 
	fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), ; Field pH 8.8 (pH meter); 
	Diffuse change to - 
	B23	0.38 - 0.86 m	Brown (10YR5/3-Moist); , 2.5Y53; Heavy clay; Weak grade of structure, 20-50 mm, Angular 
	blocky; Moderately moist; Strong consistence; 2-10%, fine gravelly, 2-6mm, subangular, Quartz, 
	coarse fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Soft segregations; Few 
	(2 - 10 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 9.2 (pH meter); Diffuse change to -
	 
	B24	0.86 - 1.32 m	Greyish brown (2.5Y5/2-Moist); , 2.5Y63; Heavy clay; Massive grade of structure; Moist; Firm 
	consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; Very few (0 - 2 
	%), Manganiferous, Medium (2 -6 mm), ; Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), 
	Nodules; Field pH 8.7 (pH meter); Diffuse change to - 
	B3	1.32 - 1.63 m	Greyish brown (2.5Y5/2-Moist); , 2.5Y64; Heavy clay; Massive grade of structure; Moist; Firm 
	consistence; 2-10%, fine gravelly, 2-6mm, subangular, Substrate material, coarse fragments; 
	Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), ; Field pH 8.4 (pH meter); Diffuse change 
	to - 

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B68	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	C	1.68 - 2.08 m	Olive yellow (2.5Y6/6-Moist); , 2.5Y80; Loam; Massive grade of structure; 10-20%, coarse 
	gravelly, 20-60mm, Substrate material, coarse fragments; Field pH 8.6 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B68	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	7.1H	 0.021B
	0.04 - 0.08	7.2H	 0.015B
	0.08 - 0.2	7.2H	 0.046B
	0.2 - 0.38	8.8H	 0.183B
	0.38 - 0.86	9.2H	 0.393B
	0.86 - 1.32	8.7H	 0.318B
	1.32 - 1.63	8.4H	 0.297B
	1.68 - 2.08	8.6H	 0.131B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 0.74E	 6C	 0.011F	 0.052B
	0.04 - 0.08
	0.08 - 0.2
	0.2 - 0.38
	0.38 - 0.86
	0.86 - 1.32
	1.32 - 1.63
	1.68 - 2.08
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.08
	0.08 - 0.2
	0.2 - 0.38
	0.38 - 0.86
	0.86 - 1.32
	1.32 - 1.63
	1.68 - 2.08

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B68	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded