Project Name:	LBV
	Project Code:	LBV	Site ID:	B7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/10/48	Elevation:	 38 metres
	Map Ref.:	Sheet No. : 8358   1:100000	Rainfall:	800
	Northing/Long.:	147.201111111111	Runoff:	Moderately rapid
	Easting/Lat.:	-19.8777777777778	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Pzg	Substrate Material:	Soil pit, 1 m deep,Slightly porous, 
	Metamorphic rock (unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Plain
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol     	Principal Profile Form:	Dr2.12
	ASC Confidence:	Great Soil Group:	Red-brown earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	2-10%, cobbly, 60-200mm, , 
	Profile Morphology
	A1	0 - 0.05 m	Dark grey (10YR4/1-Moist); ; Loam (Heavy); Massive grade of structure; Common (1-5 per 
	100mm2) Very fine (0.075-1mm) macropores, Dry; Very weak consistence; Field pH 6.9 (pH 
	meter); Clear change to - 
	A3	0.05 - 0.18 m	Brown (7.5YR4/3-Moist); ; Clay loam (Heavy); Weak grade of structure, Angular blocky; Dry; Weak
	 consistence; 2-10%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Very few (0 - 2 %),
	 Manganiferous, , Concretions; Field pH 6.9 (pH meter); Clear change to - 
	B2	0.2 - 0.58 m	Reddish brown (5YR4/4-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Moist; Firm consistence; Very few (0 - 2 %), Manganiferous, , Concretions; Field pH 7.1 
	(pH meter); Diffuse change to - 
	B3	0.61 - 0.84 m	Yellowish red (5YR4/6-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Moderate grade of structure, 5-10 mm, Angular blocky; Moist; Firm consistence; Field pH
	 7.5 (pH meter); Diffuse change to - 
	BC	0.89 - 1.04 m	Light yellowish brown (10YR6/4-Moist); ; Light clay (Heavy); Moderate grade of structure, 20-50 
	mm, Angular blocky; Weak grade of structure, 5-10 mm, Angular blocky; Moist; Weak 
	consistence; Field pH 7.9 (pH meter); Diffuse change to - 
	C	1.04 - 1.27 m	Very pale brown (10YR7/3-Moist); ; Clay loam; Massive grade of structure; Moist; Very weak 
	consistence; 20-50%, medium gravelly, 6-20mm, Substrate material, coarse fragments; Field 
	pH 8 (pH meter); 
	Morphological Notes
	Observation Notes
	PROFILE FROM 20CM TENDS TO FORM PRISMS OF 10CM DIAMETER:127CM HARD ROCK:                                                
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.9H	 0.02B	 10.3K	 4.5	 0.71	 0.24	 4.5D	 20.2E
	0.05 - 0.18	6.9H	 0.01B
	0.2 - 0.58	7.1H	 0.01B	 9.4K	 8.2	 0.21	 0.29	 5.5D	 23.6E
	0.61 - 0.84	7.5H	 0.02B
	0.89 - 1.04	7.9H	 0.02B	 31.3K	 35.2	 0.18	 1.46
	1.04 - 1.27	8H	 0.02B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 1.8E	 27C	 0.029F	 0.1B	 22C	 42	 13	 18
	0.05 - 0.18	 0.021F	 0.06B	 18C	 38	 16	 26
	0.2 - 0.58	 0.016F	 0.03B	 12C	 24	 8	 56
	0.61 - 0.84	 12C	 28	 13	 45
	0.89 - 1.04	 11C	 34	 18	 35
	1.04 - 1.27	 0.01C	 19C	 39	 16	 23
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.18
	0.2 - 0.58
	0.61 - 0.84
	0.89 - 1.04
	1.04 - 1.27

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded