Project Name:	LBV
	Project Code:	LBV	Site ID:	B70	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	09/11/50	Elevation:	 20 metres
	Map Ref.:	Sheet No. : 8358   1:100000	Rainfall:	850
	Northing/Long.:	147.25	Runoff:	Very slow
	Easting/Lat.:	-19.8333333333333	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 CZS	Substrate Material:	Auger boring, 2 m deep,Slightly porous, 
	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endocalcareous Epipedal Grey Vertosol     	Principal Profile Form:	Ug5.24
	ASC Confidence:	Great Soil Group:	Grey clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , Closed or dense. *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Grey (10YR6/1-Dry); ; Heavy clay; Moderate grade of structure, 10-20 mm, Angular blocky; Dry; 
	Strong consistence; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; Field pH 6.3 
	(pH meter); Many, very fine (0-1mm) roots; Clear change to - 
	B2	0.08 - 0.41 m	Dark grey (10YR4/1-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, Angular blocky; 
	Dry; Strong consistence; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), Nodules; Field pH 7.7 
	(pH meter); Gradual change to - 
	B2	0.41 - 0.97 m	Dark grey (10YR4/1-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, Angular blocky; 
	Weak grade of structure, Lenticular; Dry; Strong consistence; Few (2 - 10 %), Manganiferous, 
	Fine (0 - 2 mm), Nodules; Very few (0 - 2 %), Calcareous, Coarse (6 - 20 mm), Nodules; Field pH
	 9.1 (pH meter); Diffuse change to - 
	B2	0.97 - 1.52 m	Dark greyish brown (2.5Y4/2-Moist); ; Heavy clay; Weak grade of structure, 20-50 mm, Angular 
	blocky; Weak grade of structure, Lenticular; Moist; Firm consistence; Very few (0 - 2 %), 
	Manganiferous, Fine (0 - 2 mm), Nodules; Few (2 - 10 %), Calcareous, Coarse (6 - 20 mm), 
	Nodules; Field pH 8.8 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B70	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.3H	 0.02B
	0.08 - 0.41	7.7H	 0.02B
	0.41 - 0.97	9.1H	 0.08B
	0.97 - 1.52	8.8H	 0.3B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 2E	 6C	 0.018F	 0.12B	 2C	 24	 23	 46
	0.08 - 0.41
	0.41 - 0.97
	0.97 - 1.52
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.41
	0.41 - 0.97
	0.97 - 1.52

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B70	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded