Project Name:	LBV
	Project Code:	LBV	Site ID:	B81	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	14/11/50	Elevation:	 39 metres
	Map Ref.:	Sheet No. : 8358   1:100000	Rainfall:	850
	Northing/Long.:	147.283333333333	Runoff:	Slow
	Easting/Lat.:	-20.0666666666667	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 CZA	Substrate Material:	Auger boring, 2 m deep,Porous, 
	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Hypernatric Grey Sodosol     	Principal Profile Form:	Dy2.43
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , Isolated clumps. *Species includes - Aristida leptopoda, Heteropogon contortus
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus papuana, Grevillea striata
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.15 m	Light grey (10YR7/2-Moist); ; Loam; Massive grade of structure; Dry; Very weak consistence; 
	Field pH 6.4 (pH meter); Abrupt change to - 
	B21	0.15 - 0.3 m	Dark greyish brown (10YR4/2-Moist); ; Medium clay; Moderate grade of structure, 50-100 mm, 
	Prismatic; Dry; Strong consistence; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules;
	 Field pH 7.1 (pH meter); Gradual change to - 
	B22	0.3 - 0.61 m	Dark greyish brown (10YR4/2-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Dry; Strong consistence; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), 
	Nodules; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 7.9 (pH meter); 
	Gradual change to - 
	B31	0.61 - 1.02 m	Yellowish brown (10YR5/4-Moist); ; Light clay; Weak grade of structure, 20-50 mm, Angular 
	blocky; Moist; Weak consistence; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; 
	Few (2 - 10 %), Calcareous, Coarse (6 - 20 mm), Nodules; Field pH 9.3 (pH meter); Gradual 
	change to - 
	B32	1.07 - 1.52 m	Yellowish brown (10YR5/4-Moist); ; Light clay; Weak grade of structure, 20-50 mm, Angular 
	blocky; Moist; Weak consistence; 2-10%, medium gravelly, 6-20mm, subangular, Substrate 
	material, coarse fragments; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), Nodules; Very few 
	(0 - 2 %), Calcareous, Coarse (6 - 20 mm), Nodules; Field pH 9.2 (pH meter); Gradual change to 
	- 
	B3	1.52 - 1.88 m	Light brownish grey (10YR6/2-Moist); , 7.5YR66; Clay loam; Massive grade of structure; Moist; 
	Very weak consistence; 10-20%, medium gravelly, 6-20mm, subangular, Substrate material, 
	coarse fragments; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), Nodules; Very few (0 - 2 %), 
	Calcareous, Coarse (6 - 20 mm), Nodules; Field pH 9.5 (pH meter); 
	Morphological Notes
	Observation Notes
	0-15CM A1 + A2 HORIZON                                                                                                  
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B81	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B81	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	7.8H	 0.01B	 3.1K	 3.8	 0.19	 0.69	 5.7D	 13.5E
	0.15 - 0.3	8.6H	 0.06B	 5.4K	 11	 0.14	 4	 20.5E
	0.3 - 0.61	9.7H	 0.28B	 5.4K	 10.7	 0.17	 7.5	 23.8E
	0.61 - 1.02	9.5H	 0.34B
	1.07 - 1.52	9.3H	 0.32B
	1.52 - 1.88	9.1H	 0.26B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 0.84E	 5C	 0.015F	 0.05B	 18C	 48	 12	 20
	0.15 - 0.3	 0.02C	 10C	 36	 16	 35
	0.3 - 0.61	 1.3C	 5	 10C	 41	 12	 33
	0.61 - 1.02	 6	 10C	 48	 15	 28
	1.07 - 1.52
	1.52 - 1.88
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.3
	0.3 - 0.61
	0.61 - 1.02
	1.07 - 1.52
	1.52 - 1.88

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B81	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded