Project Name:	LOC
	Project Code:	LOC	Site ID:	B1006	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	152.318055555556	Runoff:	No Data
	Easting/Lat.:	-27.7869444444445	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Mountains
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	50.6 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Ug5.37
	ASC Confidence:	Great Soil Group:	Red clay
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.17 m	Dark brown (7.5YR3/2-Moist); ; Light clay; Weak grade of structure, Subangular blocky; Dry; 
	Strong consistence; 10-20%, cobbly, 60-200mm, Sandstone, coarse fragments; Field pH 7.5 
	(pH meter); CommonClear change to - 
	B21	0.17 - 0.42 m	Yellowish red (5YR4/6-Moist); ; Medium heavy clay; Strong grade of structure, 10-20 mm, 
	Angular blocky; Moist; Firm consistence; Field pH 7.5 (pH meter); Clear change to - 
	B22	0.42 - 0.56 m	; Medium heavy clay; Strong grade of structure, 10-20 mm, Angular blocky; Dry; Very strong 
	consistence; Field pH 8 (pH meter); Gradual change to - 
	BC	0.56 - 1.02 m	Yellowish red (5YR5/6-Moist); ; Clayey sand; Moist; Weak consistence; 10-20%, Sandstone, 
	coarse fragments; Clear change to - 
	C	1.02 - 1.12 m	; 
	Morphological Notes
	C	Weathered pale yellow sandstone.
	Observation Notes
	WAS LV421:                                                                                                              
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B1006	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.17	6A	 0.114A	 10.6J	 5.2	 0.33	 0.1	 19F	0.53
	0.17 - 0.42	6.4A	 0.159A	 14.6J	 10.3	 0.31	 0.3	 28.2F	1.06
	0.42 - 0.56	6.5A	 0.164A	 10.7J	 8.2	 0.33	 0.3	 22.2F	1.35
	0.56 - 1.02	6.4A	 0.124A	 5.7J	 5	 0.31	 0.2	 13.1F	1.53
	1.02 - 1.32	6.4A	 0.141A	 2.2J	 2.3	 0.19	 0.1	 6.8F	1.47
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.17
	0.17 - 0.42
	0.42 - 0.56
	0.56 - 1.02
	1.02 - 1.32
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.17
	0.17 - 0.42
	0.42 - 0.56
	0.56 - 1.02
	1.02 - 1.32

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B1006	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2_AL	Extractable Al(%) - Silver Thiorea
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension