Project Name:	LOC
	Project Code:	LOC	Site ID:	B1025	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	152.453055555556	Runoff:	No Data
	Easting/Lat.:	-27.6216666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	4.4 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn3.96
	ASC Confidence:	Great Soil Group:	Grey clay
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.2 m	Very dark brown (10YR2/2-Moist); ; Clay loam (Heavy); Weak grade of structure, Angular blocky; 
	Moist; Weak consistence; Field pH 7 (pH meter); CommonGradual change to - 
	A2	0.2 - 0.35 m	Brown (10YR5/3-Moist); ; Light clay; Moist; Very weak consistence; Field pH 7 (pH meter); Clear 
	change to - 
	B21	0.35 - 0.6 m	Dark greyish brown (10YR4/2-Moist); ; Medium clay; Moderate grade of structure, Angular blocky; 
	Moist; Firm consistence; Field pH 7.5 (pH meter); Clear change to - 
	BC	0.6 - 0.82 m	Light brownish grey (2.5Y6/2-Moist); ; Fine sandy medium clay; Weak grade of structure, Angular
	 blocky; Moderately moist; Very firm consistence; Field pH 7 (pH meter); Clear change to - 
	C	0.82 - 0.9 m	; 2-10%, Sandstone, coarse fragments; Clear change to - 
	0.9 - 1.2 m	; 
	Morphological Notes
	Weathered sandstone.
	Observation Notes
	CLEARED BRIGALOW:                                                                                                       
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B1025	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.6A	 0.059A	 8.5J	 3.1	 1.26	 0.1	 14.4F	0.69
	0.1 - 0.2	6.8A	 0.043A	 8.6J	 2.5	 1.03	 0.2	 13.9F	1.44
	0.2 - 0.4	7.1A	 0.063A	 9.6J	 2.8	 1.12	 0.2	 15.5F	1.29
	0.4 - 0.5	7A	 0.091A	 10.1J	 8.9	 0.54	 0.7	 22.2F	3.15
	0.5 - 0.9	6.9A	 0.088A	 6.5J	 8.1	 0.57	 1	 16.7F	5.99
	0.9 - 1	9.1A	 0.197A	 5.4J	 9.2	 0.61	 2.2	 18.3F	12.02
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.4 - 0.5
	0.5 - 0.9
	0.9 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.4 - 0.5
	0.5 - 0.9
	0.9 - 1

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B1025	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2_AL	Extractable Al(%) - Silver Thiorea
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension