Project Name:	LOC
	Project Code:	LOC	Site ID:	B907	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	152.270833333333	Runoff:	No Data
	Easting/Lat.:	-27.5791666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy4.43
	ASC Confidence:	Great Soil Group:	Solodic soil
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/2-Moist); ; Sandy loam; Moderate grade of structure, Granular; Dry; Loose 
	consistence; Field pH 6 (pH meter); ManyClear change to - 
	A2	0.1 - 0.23 m	Brown (10YR5/3-Moist); Light brownish grey (10YR6/2-Dry); ; Sandy loam; Massive grade of 
	structure; Dry; Loose consistence; 10-20%, Gravel, coarse fragments; Field pH 5.5 (pH meter); 
	FewAbrupt change to - 
	B21	0.23 - 0.35 m	Red (2.5YR4/6-Moist); , 5YR51; , 10YR53; Medium heavy clay; Moderate grade of structure, 
	Subangular blocky; Moderately moist; Very firm consistence; Field pH 5.8 (pH meter); 
	FewGradual change to - 
	B22	0.35 - 0.5 m	Yellowish brown (10YR5/4-Moist); ; Medium heavy clay; Strong grade of structure, Subangular 
	blocky; Moderately moist; Very firm consistence; Few (2 - 10 %), Manganiferous, , Nodules; 
	Gradual change to - 
	B23	0.5 - 0.63 m	Yellowish brown (10YR5/6-Moist); ; Heavy clay; Strong grade of structure, Subangular blocky; 
	Moderately moist; Very firm consistence; Few (2 - 10 %), Manganiferous, , Nodules; Field pH 8.5
	 (pH meter); Gradual change to - 
	B24	0.63 - 0.8 m	Yellow (10YR7/8-Moist); ; Medium clay; Moderate grade of structure, Subangular blocky; Dry; 
	Strong consistence; Common (10 - 20 %), Manganiferous, , Nodules; Field pH 9 (pH meter); 
	Clear change to - 
	C	0.8 - 1 m	Brownish yellow (10YR6/8-Moist); ; Light medium clay; Weak grade of structure, Subangular 
	blocky; Dry; Strong consistence; Common (10 - 20 %), Manganiferous, , Nodules; 
	Morphological Notes
	Observation Notes
	WAS LV110:                                                                                                              
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B907	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6A	 0.083A	 4.4J	 1.1	 0.65	 0.2	 8.9F	2.25
	0.1 - 0.23	4.9A	 0.03A	 0.7J	 0.4	 0.16	 0.1	 3.4F	2.94
	0.23 - 0.35	5.5A	 0.13A	 7.9J	 6.9	 0.35	 1.7	 34.9F	4.87
	0.35 - 0.5	7A	 0.193A	 8.5J	 7.1	 0.29	 2.3	 33.3F	6.91
	0.5 - 0.63	8.6A	 0.408A	 17.5J	 8.3	 0.38	 3.4	 38.7F	8.79
	0.63 - 0.8	8.8A	 0.366A	 17.9J	 5.5	 0.52	 2.4	 27.3F	8.79
	0.8 - 1	9A	 0.359A	 10.7J	 5.5	 0.66	 2.3	 21.9F	10.50
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.23
	0.23 - 0.35
	0.35 - 0.5
	0.5 - 0.63
	0.63 - 0.8
	0.8 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.23
	0.23 - 0.35
	0.35 - 0.5
	0.5 - 0.63
	0.63 - 0.8
	0.8 - 1

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B907	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2_AL	Extractable Al(%) - Silver Thiorea
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension