Project Name:	LOC
	Project Code:	LOC	Site ID:	B910	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	152.4625	Runoff:	No Data
	Easting/Lat.:	-27.7583333333333	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Conglomerate 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	11.1 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy2.41
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Mid Strata - Tree, 3.01-6m, Mid-dense. *Species includes - Acacia species
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.05 m	Dark brown (7.5YR3/2-Moist); ; Sandy loam; Strong grade of structure, 2-5 mm, Granular; 
	Moderately moist; Very weak consistence; Field pH 5.5 (pH meter); Clear change to - 
	A2	0.05 - 0.15 m	Brown (7.5YR4/4-Moist); Pinkish grey (7.5YR7/2-Dry); ; Clayey sand; Massive grade of structure; 
	Dry; Very weak consistence; Field pH 5 (pH meter); Abrupt change to - 
	B21	0.15 - 0.45 m	Strong brown (7.5YR5/6-Moist); ; Light medium clay; Weak grade of structure, Columnar; 
	Moderate grade of structure, Subangular blocky; Dry; Very strong consistence; Field pH 5.5 (pH 
	meter); Gradual change to - 
	B3	0.45 - 0.55 m	Strong brown (7.5YR5/8-Moist); ; Light medium clay; Weak grade of structure, Subangular 
	blocky; Moderately moist; Very firm consistence; Field pH 5.5 (pH meter); 
	0.55 - 0.6 m	; Field pH 5.7 (pH meter); 
	Morphological Notes
	Weathered sandstone.
	Observation Notes
	WAS LV115:                                                                                                              
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B910	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.4A	 0.167A	 8.7J	 4.5	 0.67	 0.5	 14.9F	3.36
	0.1 - 0.2	5.1A	 0.064A	 0.8J	 1.2	 0.22	 0.2	 2.3F	8.70
	0.15 - 0.45	0A	 0A	 0.1J	 8.2	 0.41	 1.2	 12.3F	9.76
	0.5 - 0.6	4.7A	 0.159A	 0.2J	 10.4	 0.38	 2.5	 14.8F	16.89
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.2
	0.15 - 0.45
	0.5 - 0.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.15 - 0.45
	0.5 - 0.6

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B910	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2_AL	Extractable Al(%) - Silver Thiorea
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension