Project Name:	LOC
	Project Code:	LOC	Site ID:	B924	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	152.469444444445	Runoff:	No Data
	Easting/Lat.:	-27.7425	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial fan
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	4.4 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dd1.13
	ASC Confidence:	Great Soil Group:	Solodic soil
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.02 m	Very dark grey (10YR3/1-Moist); ; Clay loam (Heavy); Moderate grade of structure, <2 mm, 
	Granular; Moderately moist; Very weak consistence; Field pH 5.7 (pH meter); CommonAbrupt 
	change to - 
	B21	0.02 - 0.42 m	Very dark grey (10YR3/1-Moist); ; Heavy clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Dry; Very strong consistence; Field pH 6.5 (pH meter); FewDiffuse change to - 
	B22	0.42 - 0.58 m	Dark greyish brown (2.5Y4/2-Moist); ; Heavy clay; Strong grade of structure, Subangular blocky; 
	Dry; Very strong consistence; Field pH 8 (pH meter); FewGradual change to - 
	B23	0.58 - 0.75 m	Greyish brown (2.5Y5/3-Moist); ; Heavy clay; Strong grade of structure, Subangular blocky; 
	Moderately moist; Very firm consistence; Field pH 8.5 (pH meter); 
	B24	0.75 - 1 m	Brown (10YR4/3-Moist); ; Medium heavy clay; Moderate grade of structure, Subangular blocky; 
	Moderately moist; Very firm consistence; Few (2 - 10 %), Calcareous, , Nodules; Field pH 8.8 
	(pH meter); 
	Morphological Notes
	Observation Notes
	WAS LV140:                                                                                                              
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B924	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.2A	 0.304A	 4.5J	 6.6	 1.08	 0.8	 14.6F	5.48
	0.02 - 0.42	6.9A	 1.29A	 8.7J	 19.9	 0.31	 6	 34.5F	17.39
	0.42 - 0.58	8.3A	 1.48A	 9.2J	 21.8	 0.24	 8.4	 38.6F	21.76
	0.58 - 0.75	8.5A	 0.598A	 8.2J	 20.5	 0.29	 8.9	 36.8F	24.18
	0.75 - 1	9.1A	 0.647A	 7.3J	 15.3	 0.38	 7.4	 29.4F	25.17
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.02 - 0.42
	0.42 - 0.58
	0.58 - 0.75
	0.75 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.02 - 0.42
	0.42 - 0.58
	0.58 - 0.75
	0.75 - 1

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B924	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2_AL	Extractable Al(%) - Silver Thiorea
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension