Project Name:	LOC
	Project Code:	LOC	Site ID:	B926	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:	Brimblecomb property.
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	152.437777777778	Runoff:	No Data
	Easting/Lat.:	-27.6963888888889	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn2.24
	ASC Confidence:	Great Soil Group:	Black earth
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (10YR3/3-Moist); ; Loamy sand; Weak grade of structure, 10-20 mm, Subangular 
	blocky; Strong grade of structure, <2 mm, Granular; Moist; Very weak consistence; Field pH 6 
	(pH meter); CommonGradual change to - 
	A2	0.1 - 0.32 m	Brown (10YR4/3-Moist); ; Clay loam, sandy; Weak grade of structure, 10-20 mm, Subangular 
	blocky; Moist; Very weak consistence; Field pH 5.8 (pH meter); Diffuse change to - 
	B	0.32 - 0.6 m	Strong brown (7.5YR5/6-Moist); ; Sandy clay loam; Massive grade of structure; Dry; Very weak 
	consistence; 2-10%, Sandstone, coarse fragments; Field pH 5.8 (pH meter); Gradual change to 
	C	0.6 - 0.8 m	; 
	Morphological Notes
	C	Reddish weathered sandstone.
	Observation Notes
	WAS LV161:                                                                                                              
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B926	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5A	 0.12A	 2.7J	 0.9	 0.4	 0.1	 4.8F	2.08
	0.1 - 0.32	4.7A	 0.04A	 1.4J	 0.5	 0.06	 0.1	 3.3F	3.03
	0.32 - 0.6	4.6A	 0.037A	 1.1J	 0.4	 0.04	 0.1	 2.8F	3.57
	0.6 - 0.8	4.3A	 0.035A	 0.9J	 0.3	 0.08	 0.1	 3.9F	2.56
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.32
	0.32 - 0.6
	0.6 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.32
	0.32 - 0.6
	0.6 - 0.8

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B926	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2_AL	Extractable Al(%) - Silver Thiorea
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension