Project Name:	LOC
	Project Code:	LOC	Site ID:	B938	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	152.356944444444	Runoff:	No Data
	Easting/Lat.:	-27.7277777777778	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	22 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dd3.13
	ASC Confidence:	Great Soil Group:	Grey clay
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tree, 3.01-6m, Mid-dense. *Species includes - Acacia harpophylla
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.08 m	Very dark brown (10YR2/2-Moist); ; Clay loam (Heavy); Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Moderately moist; Very firm consistence; 2-10%, cobbly, 60-200mm, 
	Sandstone, coarse fragments; Field pH 5.8 (pH meter); CommonClear change to - 
	B1	0.08 - 0.45 m	Very dark grey (10YR3/1-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Moderately moist; Very firm consistence; Field pH 7 (pH meter); CommonGradual 
	change to - 
	BC	0.45 - 0.68 m	Yellowish brown (10YR5/4-Moist); ; Medium clay; Moderate grade of structure, Subangular 
	blocky; Moderately moist; Very firm consistence; Common (10 - 20 %), Calcareous, , Nodules; 
	Field pH 8.5 (pH meter); 
	0.68 - 0.78 m	; Field pH 9 (pH meter); 
	Morphological Notes
	Observation Notes
	WAS LV193:                                                                                                              
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B938	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.4A	 0.157A	 15.4J	 1.7	 1.23	 0.2	 21.7F	0.92
	0.08 - 0.45	6.4A	 0.215A	 17J	 3.6	 1.93	 0.8	 30F	2.67
	0.45 - 0.68	7.4A	 0.45A	 24.5J	 4.3	 1.25	 1.6	 31.3F	5.11
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 0.45
	0.45 - 0.68
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.45
	0.45 - 0.68

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B938	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2_AL	Extractable Al(%) - Silver Thiorea
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension