Project Name:	LOC
	Project Code:	LOC	Site ID:	B958	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	152.425833333333	Runoff:	No Data
	Easting/Lat.:	-27.775	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	11 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn4.83
	ASC Confidence:	Great Soil Group:	Brown earth
	Confidence level not specified
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.15 m	Dark brown (7.5YR3/4-Moist); ; Sandy loam; Moderate grade of structure, 2-5 mm, Subangular 
	blocky; Dry; Strong consistence; Field pH 5 (pH meter); Diffuse change to - 
	A12	0.15 - 0.28 m	Dark brown (7.5YR3/4-Moist); ; Sandy clay loam; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Dry; Strong consistence; Gradual change to - 
	B21	0.28 - 0.4 m	Yellowish red (5YR5/6-Moist); ; Fine sandy medium clay; Moderate grade of structure, 10-20 
	mm, Angular blocky; Dry; Strong consistence; Field pH 7 (pH meter); 
	0.4 - 0.5 m	Yellowish red (5YR5/6-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Strong consistence; Gradual change to - 
	B22	0.5 - 0.67 m	Reddish yellow (7.5YR7/8-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, Angular 
	blocky; Dry; Strong consistence; Many (20 - 50 %), Manganiferous, , Nodules; Field pH 8.5 (pH 
	meter); Gradual change to - 
	BC	0.67 - 0.85 m	Reddish yellow (7.5YR7/8-Moist); ; Light medium clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Dry; Strong consistence; 2-10%, Sandstone, coarse fragments; Many (20 - 50 
	%), Manganiferous, , Nodules; Few (2 - 10 %), Calcareous, , Nodules; Field pH 8.5 (pH meter); 
	Clear change to - 
	C	0.85 - 0.9 m	; Field pH 8.5 (pH meter); 
	Morphological Notes
	C	Weathered yellow and white speckled sandstone.
	Observation Notes
	WAS LV299:                                                                                                              
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B958	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.5A	 0.081A	 5J	 2.8	 0.94	 0.1	 11.9F	0.84
	0.15 - 0.28	5.8A	 0.109A	 6.4J	 3.3	 1.09	 0.1	 12.3F	0.81
	0.4 - 0.5	6.2A	 0.166A	 11.6J	 10.4	 1.17	 0.4	 23.2F	1.72
	0.5 - 0.67	6.9A	 0.446A	 13.5J	 15	 0.95	 1	 27.3F	3.66
	0.67 - 0.85	7.2A	 0.585A	 11.4J	 13.5	 0.93	 2.3	 22.8F	10.09
	0.85 - 0.9	7.2A	 0.555A	 7.7J	 8.9	 0.68	 1.3	 14.3F	9.09
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.15 - 0.28
	0.4 - 0.5
	0.5 - 0.67
	0.67 - 0.85
	0.85 - 0.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.15 - 0.28
	0.4 - 0.5
	0.5 - 0.67
	0.67 - 0.85
	0.85 - 0.9

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B958	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2_AL	Extractable Al(%) - Silver Thiorea
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension