Project Name:	LOC
	Project Code:	LOC	Site ID:	B962	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	152.379444444444	Runoff:	No Data
	Easting/Lat.:	-27.7794444444445	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	39.6 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn4.13
	ASC Confidence:	Great Soil Group:	Brown earth
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tree, 3.01-6m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.06 m	Dark brown (7.5YR3/4-Moist); ; Clay loam; Strong grade of structure, Subangular blocky; Moist; 
	Very weak consistence; Field pH 7 (pH meter); Clear change to - 
	A12	0.06 - 0.6 m	Dark brown (7.5YR3/4-Moist); ; Clay loam (Heavy); Moderate grade of structure, Subangular 
	blocky; Moist; Very weak consistence; Field pH 7 (pH meter); Clear change to - 
	B21	0.6 - 0.87 m	Red (2.5YR4/7-Moist); ; Medium heavy clay; Strong grade of structure, Subangular blocky; Wet; 
	Field pH 8 (pH meter); Clear change to - 
	BC	0.87 - 1 m	Yellowish red (5YR5/8-Moist); ; Sandy medium clay; Weak grade of structure, Subangular 
	blocky; Field pH 8.2 (pH meter); Gradual change to - 
	C	1 - 1.1 m	; Field pH 8.2 (pH meter); 
	Morphological Notes
	C	Weathered reddish yellow sandstone.
	Observation Notes
	WAS LV312; SOFT WOOD SCRUB VEGETATION:                                                                                  
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B962	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.6A	 0.414A	 10.3J	 11.1	 0.21	 0.7	 20.6F	3.40
	0.4 - 0.5	6.7A	 0.332A	 2.7J	 11.6	 0.3	 5	 15.2F	32.89
	0.6 - 0.87	6.8A	 0.502A	 12.6J	 8.9	 1.97	 1.7	 25F	6.80
	0.9 - 1	6.6A	 0.416A	 5.4J	 3.6	 0.14	 0.8	 9.9F	8.08
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.4 - 0.5
	0.6 - 0.87
	0.9 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.4 - 0.5
	0.6 - 0.87
	0.9 - 1

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B962	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2_AL	Extractable Al(%) - Silver Thiorea
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension