Project Name:	LOC
	Project Code:	LOC	Site ID:	B965	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	152.368333333333	Runoff:	No Data
	Easting/Lat.:	-27.8069444444444	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	22 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy2.11
	ASC Confidence:	Great Soil Group:	Brown earth
	Confidence level not specified
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.22 m	Reddish brown (5YR4/4-Moist); ; Sandy loam; Weak grade of structure, Subangular blocky; Dry; 
	Very weak consistence; Field pH 6.7 (pH meter); Diffuse change to - 
	A12	0.22 - 0.53 m	Yellowish red (5YR5/6-Moist); ; Sandy loam (Light); Weak grade of structure, Subangular blocky;
	 Moderately moist; Weak consistence; Field pH 6.7 (pH meter); Abrupt change to - 
	B21	0.43 - 0.77 m	Yellowish red (5YR5/7-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, Subangular 
	blocky; Moderately moist; Firm consistence; Field pH 6.5 (pH meter); Diffuse change to - 
	B22	0.77 - 1 m	Yellowish red (5YR5/8-Moist); , 10YR61, 10-20% , 0-5mm, Distinct; , 10-20% , 0-5mm, Distinct; 
	Light medium clay; Strong grade of structure, 20-50 mm, Subangular blocky; Moderately moist; 
	Firm consistence; Field pH 5.5 (pH meter); 
	Morphological Notes
	Observation Notes
	WAS LV332:                                                                                                              
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B965	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.22	6.6A	 0.071A	 3.2J	 1.4	 0.83	 0	 5.5F	0.00
	0.22 - 0.53	6.3A	 0.037A	 2.4J	 0.6	 0.3	 0.1	 3.9F	2.56
	0.53 - 0.77	6A	 0.066A	 4.7J	 6.3	 0.77	 0.7	 13.7F	5.11
	0.77 - 1	5.2A	 0.176A	 2.5J	 7.3	 0.75	 1.9	 13.4F	14.18
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.22
	0.22 - 0.53
	0.53 - 0.77
	0.77 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.22
	0.22 - 0.53
	0.53 - 0.77
	0.77 - 1

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B965	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2_AL	Extractable Al(%) - Silver Thiorea
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension