Project Name:	LOC
	Project Code:	LOC	Site ID:	B973	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	152.3225	Runoff:	No Data
	Easting/Lat.:	-27.7483333333333	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plateau
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	4.4 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.13
	ASC Confidence:	Great Soil Group:	Red-brown earth
	Confidence level not specified
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	Ap	0 - 0.08 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam, fine sandy; Moderate grade of structure, 
	Granular; Dry; Strong consistence; Field pH 6 (pH meter); Clear change to - 
	B21	0.08 - 0.4 m	Red (2.5YR4/6-Moist); ; Medium clay; Moderate grade of structure, Subangular blocky; Moist; 
	Firm consistence; Field pH 7.5 (pH meter); Diffuse change to - 
	B22	0.4 - 0.6 m	Brown (7.5YR5/4-Moist); ; Medium clay; Moderate grade of structure, Subangular blocky; Moist; 
	Firm consistence; Field pH 8.5 (pH meter); Gradual change to - 
	B3	0.6 - 0.7 m	Strong brown (7.5YR5/6-Moist); , 5YR58, 20-50% , 0-5mm, Distinct; , 20-50% , 0-5mm, Distinct; 
	Medium clay; Weak grade of structure, Subangular blocky; Moist; Very firm consistence; Field 
	pH 8.5 (pH meter); Clear change to - 
	C	0.7 - 0.8 m	; 
	Morphological Notes
	C	Yellow & white weathered sandstone some patches of clay.
	Observation Notes
	WAS LV347:                                                                                                              
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B973	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.4A	 0.08A	 10.2J	 2.1	 0	 0	 17F	0.00
	0.08 - 0.4	7A	 0.054A	 15.6J	 3	 0	 0.1	 23.5F	0.43
	0.4 - 0.5	8.2A	 0.362A	 19.8J	 3.4	 0	 0.1	 27.5F	0.36
	0.6 - 0.7	8.2A	 0.35A	 16.4J	 2.9	 0	 0.2	 23.1F	0.87
	0.9 - 1	8.3A	 0.33A	 13.9J	 2.5	 0	 0.1	 20F	0.50
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.08 - 0.4
	0.4 - 0.5
	0.6 - 0.7
	0.9 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.08 - 0.4
	0.4 - 0.5
	0.6 - 0.7
	0.9 - 1

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B973	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2_AL	Extractable Al(%) - Silver Thiorea
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension