Project Name:	LOC
	Project Code:	LOC	Site ID:	B975	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	152.219444444444	Runoff:	No Data
	Easting/Lat.:	-27.68	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	4.4 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.13
	ASC Confidence:	Great Soil Group:	Solodic soil
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.15 m	Brown (7.5YR4/2-Moist); ; Sandy loam; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Moist; Weak consistence; Field pH 6 (pH meter); Few, fine (1-2mm) roots; Clear change 
	to - 
	B21	0.15 - 0.4 m	Brownish yellow (10YR6/6-Moist); , 5YR58, 10-20% , 0-5mm, Distinct; , 10-20% , 0-5mm, 
	Distinct; Medium heavy clay; Moderate grade of structure, Subangular blocky; Moderately moist; 
	Firm consistence; Field pH 5.8 (pH meter); Clear change to - 
	B22	0.4 - 0.6 m	Brownish yellow (10YR6/6-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Moderately moist; Firm consistence; Common (10 - 20 %), Manganiferous, , Soft
	 segregations; Field pH 8.5 (pH meter); Abrupt change to - 
	C	0.6 - 0.62 m	; 
	Morphological Notes
	C	white sandstone.
	Observation Notes
	WAS LV352:                                                                                                              
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B975	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.8A	 0.024A	 4J	 3.4	 0.57	 0.2	 9.7F	2.06
	0.15 - 0.4	5.6A	 0.053A	 6.8J	 9.6	 0.46	 1	 21.4F	4.67
	0.4 - 0.5	7.3A	 0.084A	 7.5J	 10.3	 0.43	 1.4	 23.5F	5.96
	0.6 - 0.62	7.8A	 0.16A	 5.2J	 4.5	 0.42	 0.6	 11.8F	5.08
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.15 - 0.4
	0.4 - 0.5
	0.6 - 0.62
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.15 - 0.4
	0.4 - 0.5
	0.6 - 0.62

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B975	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2_AL	Extractable Al(%) - Silver Thiorea
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension