Project Name:	LOC
	Project Code:	LOC	Site ID:	B987	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	Runoff:	No Data
	Easting/Lat.:	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	1.28 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.41
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.22 m	Brown (7.5YR5/4-Moist); ; Fine sandy loam; Weak grade of structure, Subangular blocky; Dry; 
	Very weak consistence; 20-50%, coarse gravelly, 20-60mm, Detrital sedimentary rock 
	(unidentified), coarse fragments; CommonGradual change to - 
	A2	0.22 - 0.53 m	Yellowish red (5YR5/6-Moist); Light reddish brown (5YR6/4-Dry); ; Moderate grade of structure, 
	Subangular blocky; Dry; Firm consistence; 20-50%, coarse gravelly, 20-60mm, Detrital 
	sedimentary rock (unidentified), coarse fragments; Gradual change to - 
	B21	0.53 - 1.15 m	Yellowish red (5YR4/6-Moist); ; Medium clay; Strong grade of structure, Angular blocky; Dry; Very
	 firm consistence; 20-50%, coarse gravelly, 20-60mm, Detrital sedimentary rock (unidentified), 
	coarse fragments; Few, coarse (>5mm) roots; Diffuse change to - 
	B22	1.15 - 1.33 m	Yellowish red (5YR4/6-Moist); , 7.5YR54; Medium clay; Strong grade of structure, Angular 
	blocky; Dry; Very firm consistence; 20-50%, coarse gravelly, 20-60mm, Detrital sedimentary rock 
	(unidentified), coarse fragments; FewClear change to - 
	BC	1.33 - 1.7 m	Very pale brown (10YR7/4-Moist); , 5YR58; Medium clay; Strong grade of structure, Polyhedral; 
	Moist; Very weak consistence; 2-10%, medium gravelly, 6-20mm, Detrital sedimentary rock 
	(unidentified), coarse fragments; Few, fine (1-2mm) roots; Abrupt change to - 
	R	1.7 - 1.8 m	Rock 
	Morphological Notes
	R	Sandstone.
	Observation Notes
	WAS LV372:                                                                                                              
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B987	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.22	5.3A	 0.003A	 3.6F	 0.29	 0.1	 0.1	 8.3F	 5.1F	1.20
	0.22 - 0.53	4.4A	 0.004A	 0.43F	 0.07	 0.71	 0.71	 6.3F	 2.4F	11.27
	0.53 - 1.15	4.2A	 0.005A	 0.56F	 0.3	 0.11	 0.11	 17.7F	 7.4F	0.62
	1.15 - 1.33	4.4A	 0.004A	 0.18F	 0.36	 0.39	 0.39	 20.8F	 9.5F	1.88
	1.33 - 1.7	4.3A	 0.007A	 0.14F	 0.34	 0.28	 0.28	 17.7F	 8.1F	1.58
	1.7 - 2	4.4A	 0.006A	 0.27F	 0.1	 0.06	 0.06	 4.2F	 1.7F	1.43
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.22	 0.041A	 0.9A
	0.22 - 0.53	 0.04A	 0.89A
	0.53 - 1.15	 0.05A	 1.01A
	1.15 - 1.33	 0.032A	 1.1A
	1.33 - 1.7	 0.026A	 1.34A
	1.7 - 2	 0.015A	 0.94A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.22
	0.22 - 0.53
	0.53 - 1.15
	1.15 - 1.33
	1.33 - 1.7
	1.7 - 2

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B987	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_XRF_CU	Total element - Cu(mg/kg) - X-Ray Fuoresence
	12_XRF_ZN	Total element - Zn(mg/kg) - X-Ray Fuoresence
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2_AL	Extractable Al(%) - Silver Thiorea
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	9A1	Total phosphorus - X-ray fluorescence
	MIN_EC	Exchange Capacity - Minerology
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_St	Smectite - X-Ray Diffraction