Project Name:	LOC
	Project Code:	LOC	Site ID:	B996	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	152.451388888889	Runoff:	No Data
	Easting/Lat.:	-27.7916666666667	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	8.8 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy2.23
	ASC Confidence:	Great Soil Group:	Solodic soil
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus crebra, Eucalyptus tessellaris
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.05 m	Brown (7.5YR4/4-Moist); ; Loamy fine sand; Weak grade of structure, 5-10 mm, Subangular 
	blocky; Moist; Very weak consistence; Field pH 6 (pH meter); Clear change to - 
	A2	0.05 - 0.22 m	Yellowish red (5YR5/6-Moist); ; Loamy fine sand; Weak grade of structure, Subangular blocky; 
	Moist; Weak consistence; Field pH 6.5 (pH meter); Clear change to - 
	B21	0.22 - 0.35 m	Red (2.5YR4/6-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, Angular blocky; Moist; 
	Weak consistence; Field pH 5.5 (pH meter); FewGradual change to - 
	B22	0.35 - 0.63 m	Red (2.5YR4/6-Moist); , 10YR66, 20-50% , 0-5mm, Distinct; , 20-50% , 0-5mm, Distinct; Medium 
	clay; Strong grade of structure, 20-50 mm, Angular blocky; Moist; Firm consistence; Field pH 6.5
	 (pH meter); Clear change to - 
	B23	0.63 - 0.75 m	Reddish yellow (7.5YR6/8-Moist); ; Light medium clay; Massive grade of structure; Moist; Firm 
	consistence; Field pH 6.8 (pH meter); Clear change to - 
	BC	0.75 - 0.95 m	Reddish yellow (7.5YR6/8-Moist); ; Fine sandy clay loam; 10-20%, Sandstone, coarse 
	fragments; Field pH 8 (pH meter); Gradual change to - 
	C	0.95 - 1 m	; 
	Morphological Notes
	C	Weathered white sandstone.
	Observation Notes
	WAS LV397:                                                                                                              
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B996	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.6A	 0.111A	 2.4J	 1.1	 0.54	 0	 4.9F	0.00
	0.05 - 0.22	5.5A	 0.035A	 1.9J	 0.8	 0.34	 0.1	 4.1F	2.44
	0.22 - 0.35	6A	 0.051A	 10.4J	 4.9	 0.36	 0.7	 20.6F	3.40
	0.35 - 0.63	6.4A	 0.035A	 10.8J	 4.5	 0.35	 0.8	 19.1F	4.19
	0.63 - 0.75	8.4A	 0.118A	 8.3J	 2.8	 0.58	 0.7	 14.2F	4.93
	0.75 - 0.95	8.8A	 0.08A	 10.3J	 2.2	 0.69	 0.7	 15.1F	4.64
	0.95 - 1	7A	 0.083A	 8.7J	 1.6	 0.71	 0.5	 12F	4.17
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.22
	0.22 - 0.35
	0.35 - 0.63
	0.63 - 0.75
	0.75 - 0.95
	0.95 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.22
	0.22 - 0.35
	0.35 - 0.63
	0.63 - 0.75
	0.75 - 0.95
	0.95 - 1

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B996	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2_AL	Extractable Al(%) - Silver Thiorea
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension