Project Name:	Regional
	Project Code:	REG	Site ID:	T11	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	Parent material granitic alluvium:site near levee 
	crest+blazed pop.gum:
	Date Desc.:	05/06/64	Elevation:	No Data
	Map Ref.:	Sheet No. : 8259   1:100000	Rainfall:	1143
	Northing/Long.:	146.583333333333	Runoff:	Rapid
	Easting/Lat.:	-19.2916666666667	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Terrace (alluvial)
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Levee	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Brown Kandosol     	Principal Profile Form:	Db1.22
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Heteropogon contortus, Imperata cylindrica
	Mid Strata - Shrub, 3.01-6m, Sparse. *Species includes - Planchonia careya, Panicum species
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus polycarpa, Eucalyptus tessellaris, Eucalyptus alba
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.15 m	Very dark greyish brown (10YR3/2-Moist); Greyish brown (10YR5/2-Dry); ; Loamy sand; Weak 
	grade of structure, 5-10 mm, Subangular blocky; Very weak consistence; 
	A21	0.15 - 0.3 m	Brown (10YR4/3-Moist); Pale brown (10YR6/3-Dry); ; Loamy sand; Massive grade of structure; 
	Very weak consistence; Gradual change to - 
	A22	0.3 - 0.51 m	Yellowish brown (10YR5/4-Moist); Light yellowish brown (10YR6/4-Dry); ; Loamy sand; Massive 
	grade of structure; Weak consistence; Gradual change to - 
	A3	0.51 - 0.71 m	Strong brown (7.5YR4/6-Moist); Reddish yellow (7.5YR6/6-Dry); ; Loamy sand (Heavy); Weak 
	grade of structure, 10-20 mm, Subangular blocky; Weak consistence; 2-10%, fine gravelly, 2-
	6mm, Granite, coarse fragments; Gradual change to - 
	A3	0.71 - 0.91 m	Strong brown (7.5YR4/6-Moist); Reddish yellow (7.5YR6/6-Dry); ; Sandy loam (Light); Weak 
	grade of structure, 10-20 mm, Subangular blocky; Weak consistence; 2-10%, fine gravelly, 2-
	6mm, Granite, coarse fragments; Gradual change to - 
	B2	0.91 - 1.22 m	Strong brown (7.5YR4/6-Moist); Reddish yellow (7.5YR6/6-Dry); ; Light clay; Weak grade of 
	structure, 10-20 mm, Subangular blocky; Very firm consistence; 2-10%, fine gravelly, 2-6mm, 
	Quartz, coarse fragments; Clear change to - 
	B3	1.22 - 1.47 m	Strong brown (7.5YR4/6-Moist); Reddish yellow (7.5YR6/6-Dry); ; Sandy clay loam; Weak grade 
	of structure, 10-20 mm, Subangular blocky; Very firm consistence; 2-10%, fine gravelly, 2-6mm, 
	Granite, coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes
	BLACK RIVER

	Project Name:	Regional
	Project Code:	REG	Site ID:	T11	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	6.5A	 0.032A	 4B	 0.8	 0.18	 0.2	 6C	3.33
	0.15 - 0.3	6.4A	 0.032A	 2.6B	 0.4	 0.18	 0.2	 4C	5.00
	0.3 - 0.51	6.4A	 0.017A
	0.51 - 0.71	6.6A	 0.011A	 1.8B	 0.4	 0.18	 0.3
	0.71 - 0.91	6.6A	 0.017A
	0.91 - 1.22	6.7A	 0.017A	 5.1B	 2.2	 0.24	 0.4
	1.22 - 1.47	6.6A	 0.017A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 1.09D	 13B	 0.014A	 0.06A	 59D	 24	 10	 7
	0.15 - 0.3	 0.4D	 10B	 0.009A	 4	 55D	 28	 11	 7
	0.3 - 0.51	 4B	 0.005A
	0.51 - 0.71	 3B	 8	 65D	 19	 10	 8
	0.71 - 0.91	 4B
	0.91 - 1.22	 3B	 6	 40D	 27	 10	 26
	1.22 - 1.47	 3B
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.3
	0.3 - 0.51
	0.51 - 0.71
	0.71 - 0.91
	0.91 - 1.22
	1.22 - 1.47

	Project Name:	Regional
	Project Code:	REG	Site ID:	T11	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance