Project Name:	Regional
	Project Code:	REG	Site ID:	T111	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	Turnoff on Harvey's Range Road to old Beef Road 
	12.8KM south of Inghamhighway:
	Date Desc.:	12/02/70	Elevation:	No Data
	Map Ref.:	Sheet No. : 8259   1:100000	Rainfall:	1115
	Northing/Long.:	146.55	Runoff:	Moderately rapid
	Easting/Lat.:	-19.3166666666667	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  QA	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Prior stream	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melanic Eutrophic Red Kandosol     	Principal Profile Form:	GN3.14
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus alba, Eucalyptus polycarpa, Eucalyptus tessellaris
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Dark reddish brown (5YR2/2-Moist); ; Sandy loam (Heavy); Weak grade of structure, 2-5 mm, 
	Granular; Weak consistence; 2-10%, fine gravelly, 2-6mm, Charcoal, coarse fragments; 
	Common, fine (1-2mm) roots; Clear change to - 
	A12	0.05 - 0.1 m	Dark reddish brown (5YR3/2-Moist); ; Sandy loam (Heavy); Weak grade of structure, 10-20 mm, 
	Angular blocky; Weak consistence; Common, fine (1-2mm) roots; Gradual change to - 
	A2	0.1 - 0.2 m	Dark reddish brown (5YR3/2-Moist); ; Sandy loam (Heavy); Weak grade of structure, 10-20 mm, 
	Angular blocky; Earthy fabric; Weak consistence; 2-10%, fine gravelly, 2-6mm, Charcoal, coarse
	 fragments; Few, fine (1-2mm) roots; Gradual change to - 
	B1	0.2 - 0.3 m	Dark reddish brown (2.5YR3/4-Moist); ; Sandy clay loam; Weak grade of structure, 10-20 mm, 
	Angular blocky; Earthy fabric; Few (<1 per 100mm2) Fine (1-2mm) macropores, Weak 
	consistence; Few, fine (1-2mm) roots; Gradual change to - 
	B21	0.3 - 0.45 m	Dark red (2.5YR3/6-Moist); ; Light clay; Weak grade of structure, 20-50 mm, Angular blocky; 
	Earthy fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Weak consistence; Few, 
	fine (1-2mm) roots; Gradual change to - 
	B22	0.45 - 0.6 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; Smooth-ped fabric; Few (<1 per 100mm2) Fine (1-2mm) macropores, Weak consistence;
	 Few, fine (1-2mm) roots; Gradual change to - 
	B23	0.6 - 0.75 m	Dark red (2.5YR3/6-Moist); ; Sandy medium clay; Weak grade of structure, 20-50 mm, Angular 
	blocky; Earthy fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Weak consistence; 
	Gradual change to - 
	BC	0.75 - 0.9 m	Dark red (2.5YR3/7-Moist); ; Sandy clay loam (Light); Weak grade of structure, 20-50 mm, 
	Angular blocky; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Weak consistence; 2-
	10%, medium gravelly, 6-20mm, Gravel, coarse fragments; Gradual change to - 
	BC	0.9 - 1.13 m	Dark red (2.5YR3/8-Moist); ; Clay loam, sandy (Heavy); Massive grade of structure; Few (<1 per 
	100mm2) Fine (1-2mm) macropores, Very weak consistence; Gradual change to - 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T111	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	C	1.13 - 1.2 m	Yellowish red (5YR4/8-Moist); ; Clay loam, sandy; Massive grade of structure; Very weak 
	consistence; 
	C	1.2 - 1.5 m	Yellowish red (5YR4/8-Moist); ; Clay loam, sandy (Light); Single grain grade of structure; Loose 
	consistence; 2-10%, medium gravelly, 6-20mm, rounded, Gravel, coarse fragments; 
	C	1.5 - 1.8 m	Yellowish red (5YR4/8-Moist); ; Clay loam, sandy (Light); Single grain grade of structure; Loose 
	consistence; 2-10%, medium gravelly, 6-20mm, rounded, Gravel, coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes
	HARVEY'S RANGE

	Project Name:	Regional
	Project Code:	REG	Site ID:	T111	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.4A	 0.044A	 8.1B	 1.9	 0.36	 0.18	 12.2C	1.48
	0.05 - 0.1	6.4A	 0.035A
	0.1 - 0.2	6.5A	 0.026A	 3.5B	 1	 0.17	 0.14	 6.3C	2.22
	0.2 - 0.3	6.4A	 0.077A
	0.3 - 0.45	6.4A	 0.026A	 3.7B	 1.6	 0.27	 0.14	 6.6C	2.12
	0.45 - 0.6	6.3A	 0.035A
	0.6 - 0.75	6.2A	 0.032A	 4.6B	 2	 0.33	 0.19	 7.2C	2.64
	0.75 - 0.9	6A	 0.029A
	0.9 - 1.13	6.3A	 0.026A
	1.13 - 1.2	6.3A	 0.077A
	1.2 - 1.5	6.4A	 0.023A
	1.5 - 1.8	6.5A	 0.023A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 2.02D	 11A	 0.041A	 0.13A	 2.9A	 44A	 26	 11	 13
	 28B
	0.05 - 0.1
	0.1 - 0.2	 0.59D	 6B	 0.022A	 0.05A	 3A	 42A	 29	 16	 17
	0.2 - 0.3
	0.3 - 0.45	 5B	 0.019A	 2.7A	 35A	 23	 11	 33
	0.45 - 0.6
	0.6 - 0.75	 31A	 21	 14	 35
	0.75 - 0.9
	0.9 - 1.13
	1.13 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.45
	0.45 - 0.6
	0.6 - 0.75
	0.75 - 0.9
	0.9 - 1.13
	1.13 - 1.2
	1.2 - 1.5
	1.5 - 1.8

	Project Name:	Regional
	Project Code:	REG	Site ID:	T111	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method