Project Name:	Regional
	Project Code:	REG	Site ID:	T113	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:	.6KM east of railway line on Bluewater Beach Road:
	Date Desc.:	25/02/70	Elevation:	No Data
	Map Ref.:	Sheet No. : 8259   1:100000	Rainfall:	1170
	Northing/Long.:	146.566666666667	Runoff:	Moderately rapid
	Easting/Lat.:	-19.1666666666667	Drainage:	No Data
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Auger boring, No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Terrace (alluvial)
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Red Kandosol     	Principal Profile Form:	Gn2.14
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Melaleuca species, Acacia species
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus drepanophylla, Eucalyptus polycarpa, Eucalyptus 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Brown (7.5YR4/2-Moist); ; Loam; Weak grade of structure, 5-10 mm, Angular blocky; Moist; Weak
	 consistence; Gradual change to - 
	A2	0.1 - 0.2 m	Brown (7.5YR4/4-Moist); ; Loam; Weak grade of structure, 5-10 mm, Angular blocky; Moist; Weak
	 consistence; Gradual change to - 
	B11	0.2 - 0.3 m	Reddish brown (5YR4/4-Moist); ; Loam (Heavy); Massive grade of structure; Earthy fabric; Moist; 
	Weak consistence; 
	B12	0.3 - 0.45 m	Reddish brown (5YR4/4-Moist); ; Clay loam, fine sandy; Massive grade of structure; Moist; Weak 
	consistence; 
	B12	0.45 - 0.6 m	Yellowish red (5YR4/6-Moist); ; Clay loam, fine sandy; Massive grade of structure; Moist; Weak 
	consistence; 
	B2	0.6 - 0.75 m	Reddish yellow (7.5YR6/6-Moist); , 5YR56, 2-10% , 5-15mm, Distinct; , 2-10% , 5-15mm, 
	Distinct; Light clay; Massive grade of structure; Moist; Weak consistence; Few (2 - 10 %), 
	Argillaceous, Coarse (6 - 20 mm), Nodules; 
	B2	0.75 - 0.9 m	Reddish yellow (7.5YR6/6-Moist); , 5YR56, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Light clay; Massive grade of structure; Moist; Weak consistence; 0-2%, fine gravelly, 2-
	6mm, Gravel, coarse fragments; Very few (0 - 2 %), Argillaceous, Coarse (6 - 20 mm), Nodules; 
	Gradual change to - 
	B2	0.9 - 1.2 m	Reddish yellow (7.5YR6/6-Moist); , 5YR58, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Light clay; Massive grade of structure; Moist; Weak consistence; 2-10%, fine gravelly, 
	2-6mm, Gravel, coarse fragments; 
	B2	1.2 - 1.42 m	Reddish yellow (7.5YR6/6-Moist); , 5YR58, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Light clay; Massive grade of structure; Moist; Weak consistence; 2-10%, fine gravelly, 
	2-6mm, Gravel, coarse fragments; Few (2 - 10 %), Ferromanganiferous, , ; Clear change to - 
	D	1.42 - 1.5 m	Very pale brown (10YR8/4-Moist); , 5YR58, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Medium clay; Massive grade of structure; Moderately moist; Very firm consistence; 
	Common (10 - 20 %), Ferromanganiferous, , ; 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T113	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	D	1.5 - 1.8 m	Very pale brown (10YR8/4-Moist); , 10YR68, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Medium clay; Massive grade of structure; Moderately moist; Very firm consistence; 
	Morphological Notes
	Observation Notes
	10-30CM SOME A1 MATERIAL DOWN WORM CASTS: LAYERS RENUMBERED 22-9-92                                                     
	Site Notes
	BLUEWATER BCH

	Project Name:	Regional
	Project Code:	REG	Site ID:	T113	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6A	 0.03A	 5.3B	 1.5	 0.55	 0.17	 1.6F	 8.2C	 9.1F	2.07
	0.1 - 0.2	6.1A	 0.029A	 2.6B	 0.98	 0.36	 0.19	 1.7F	 5.1C	 5.8F	3.73
	0.2 - 0.3	6.4A	 0.023A	 2.08B	 0.94	 0.21	 0.17	 1.8F	 6.3C	 5.2F	2.70
	0.3 - 0.45	6.3A	 0.02A	 2B	 1.1	 0.2	 0.19	 1.2F	 4.3C	 4.7F	4.42
	0.45 - 0.6	6.3A	 0.02A
	0.6 - 0.75	6.2A	 0.02A	 2.3B	 1.6	 0.26	 0.2	 1.3F	 4.7C	 5.7F	4.26
	0.75 - 0.9	6.3A	 0.014A
	0.9 - 1.2	6.4A	 0.014A	 2.1B	 1.6	 0.2	 0.22	 1.3F	 5.4F
	1.2 - 1.42	6.5A	 0.011A
	1.42 - 1.5	6.3A	 0.017A	 2.9B	 2.2	 0.28	 0.23	 1.3F	 6.9F
	1.5 - 1.8	6.4A	 0.014A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.28D	 4A	 0.014A	 0.103A	 0.41A	 17A	 48	 22	 13
	 7B
	0.1 - 0.2	 0.59D	 4B	 0.065A	 8A	 52	 25	 17
	0.2 - 0.3	 0.32D	 2B	 0.01A	 0.43A	 7A	 53	 23	 17
	0.3 - 0.45	 3B	 6A	 53	 22	 20
	0.45 - 0.6
	0.6 - 0.75	 5A	 49	 21	 25
	0.75 - 0.9
	0.9 - 1.2	 0.007A	 0.41A	 10A	 49	 20	 24
	1.2 - 1.42
	1.42 - 1.5	 5A	 47	 17	 31
	1.5 - 1.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.45
	0.45 - 0.6
	0.6 - 0.75
	0.75 - 0.9
	0.9 - 1.2
	1.2 - 1.42
	1.42 - 1.5
	1.5 - 1.8

	Project Name:	Regional
	Project Code:	REG	Site ID:	T113	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction