Project Name:	Regional
	Project Code:	REG	Site ID:	T129	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	Opposite Comalco turnoff on Moreton/Jardine Road:
	Date Desc.:	13/07/70	Elevation:	No Data
	Map Ref.:	Sheet No. : 7374   1:100000	Rainfall:	1680
	Northing/Long.:	142.45	Runoff:	Moderately rapid
	Easting/Lat.:	-11.65	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Jkb	Substrate Material:	Undisturbed soil core, 5.9 m 
	deep,Sandstone 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	15 metres
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Dystrophic Red Kandosol     	Principal Profile Form:	Gn2.44
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - None recorded
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Panicum species, Acacia species
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus tetrodonta, Eucalyptus polycarpa, Grevillea glauca
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11A12	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); Brown (10YR4/3-Dry); ; Loamy sand; Single grain 
	grade of structure; Dry; Loose consistence; Clear change to - 
	A12	0.05 - 0.1 m	Dark brown (7.5YR3/4-Moist); Brown (7.5YR4/4-Dry); ; Loamy sand; Single grain grade of 
	structure; Dry; Loose consistence; Gradual change to - 
	A21	0.1 - 0.2 m	Reddish brown (5YR4/4-Moist); Yellowish red (5YR4/6-Dry); ; Sandy loam; Single grain grade of 
	structure; Moderately moist; Weak consistence; Gradual change to - 
	A22	0.2 - 0.3 m	Yellowish red (5YR4/6-Moist); ; Sandy loam; Single grain grade of structure; Many (>5 per 
	100mm2) Fine (1-2mm) macropores, Moderately moist; Weak consistence; Gradual change to - 
	A23	0.3 - 0.4 m	Yellowish red (5YR4/6-Moist); ; Loamy sand; Single grain grade of structure; Many (>5 per 
	100mm2) Fine (1-2mm) macropores, Moderately moist; Weak consistence; Gradual change to - 
	B1	0.4 - 0.5 m	Red (2.5YR4/6-Moist); ; Sandy loam; Massive grade of structure; Many (>5 per 100mm2) Fine (1-
	2mm) macropores, Moderately moist; Weak consistence; Gradual change to - 
	B1	0.5 - 0.6 m	Red (2.5YR5/8-Moist); ; Sandy loam; Massive grade of structure; Moderately moist; Weak 
	consistence; Gradual change to - 
	B1	0.6 - 0.7 m	Red (2.5YR4/7-Moist); ; Sandy loam; Massive grade of structure; Moderately moist; Weak 
	consistence; Gradual change to - 
	B21	0.7 - 0.8 m	Red (2.5YR4/8-Moist); , 10YR68, 0-2% , 5-15mm, Distinct; , 0-2% , 5-15mm, Distinct; Sandy 
	loam; Massive grade of structure; Moderately moist; Weak consistence; Gradual change to - 
	B21	0.8 - 0.9 m	Red (2.5YR4/8-Moist); , 10YR68, 2-10% , 5-15mm, Distinct; , 2-10% , 5-15mm, Distinct; Sandy 
	loam; Massive grade of structure; Moderately moist; Weak consistence; Gradual change to - 
	B21	0.9 - 1.05 m	Red (2.5YR4/8-Moist); , 10YR68, 2-10% , 5-15mm, Distinct; , 2-10% , 5-15mm, Distinct; Sandy 
	loam; Massive grade of structure; Moderately moist; Very weak consistence; Gradual change to - 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T129	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B22	1.05 - 1.2 m	Red (2.5YR4/8-Moist); , 10YR68, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; 
	Sandy clay loam (Light); Massive grade of structure; Moderately moist; Very weak consistence; 
	Gradual change to - 
	B22	1.2 - 1.35 m	Red (2.5YR4/8-Moist); , 10YR68, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; 
	Sandy clay loam; Massive grade of structure; Moderately moist; Very weak consistence; Gradual
	 change to - 
	B22	1.35 - 1.5 m	Red (2.5YR4/8-Moist); , 10YR68, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; 
	Sandy clay loam; Massive grade of structure; Moderately moist; Very weak consistence; Gradual
	 change to - 
	1.5 - 1.65 m	Red (2.5YR4/8-Moist); , 10YR68, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; 
	Sandy clay loam; Massive grade of structure; Very weak consistence; Gradual change to - 
	1.65 - 1.8 m	Red (2.5YR4/8-Moist); , 10YR68, 10-20% , 15-30mm, Prominent; , 10-20% , 15-30mm, 
	Prominent; Sandy clay loam; Massive grade of structure; Very weak consistence; Gradual 
	change to - 
	1.8 - 2.1 m	Red (2.5YR4/8-Moist); , 10YR68, 10-20% , 15-30mm, Prominent; , 5YR58, 10-20% , 15-30mm, 
	Prominent; Sandy clay loam (Heavy); Massive grade of structure; Firm consistence; Gradual 
	change to - 
	2.1 - 2.4 m	Red (10R4/8-Moist); , 5YR58, 10-20% , 5-15mm, Distinct; , 10YR68, 10-20% , 5-15mm, Distinct; 
	Sandy clay loam (Heavy); Massive grade of structure; Firm consistence; Gradual change to - 
	2.4 - 2.7 m	Red (10R4/8-Moist); , 10YR68, 10-20% , 15-30mm, Prominent; , 5YR58, 10-20% , 15-30mm, 
	Prominent; Sandy clay loam (Heavy); Massive grade of structure; Weak consistence; Gradual 
	change to - 
	2.7 - 3 m	Red (10R4/8-Moist); , 10YR68, 2-10% , 5-15mm, Distinct; , 5YR58, 2-10% , 5-15mm, Distinct; 
	Sandy clay loam (Heavy); Massive grade of structure; Weak consistence; Gradual change to - 
	3 - 3.3 m	Red (10R4/8-Moist); , 10YR68, 0-2% , 5-15mm, Distinct; , 0-2% , 5-15mm, Distinct; Sandy clay 
	loam (Heavy); Massive grade of structure; Weak consistence; Gradual change to - 
	3.3 - 3.6 m	Red (10R4/8-Moist); , 10YR68, 0-2% , 5-15mm, Distinct; , 0-2% , 5-15mm, Distinct; Sandy clay 
	loam (Heavy); Massive grade of structure; Weak consistence; Gradual change to - 
	3.6 - 4.1 m	Red (10R4/8-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Weak consistence; 
	Gradual change to - 
	4.1 - 4.6 m	Red (10R4/8-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Weak consistence; 
	Common (10 - 20 %), Ferruginous, Medium (2 -6 mm), Nodules; Clear change to - 
	4.6 - 4.85 m	Red (10R4/8-Moist); ; Sandy loam (Heavy); Massive grade of structure; Weak consistence; Many 
	(20 - 50 %), Ferruginous, Very coarse (20 - 60 mm), Nodules; Gradual change to - 
	4.85 - 5.1 m	Red (2.5YR4/8-Moist); ; Sandy loam; Massive grade of structure; Weak consistence; 0-2%, 
	angular platy, Sandstone, coarse fragments; Many (20 - 50 %), Ferruginous, Very coarse (20 - 60
	 mm), Nodules; Gradual change to - 
	5.1 - 5.6 m	Red (2.5YR4/8-Moist); ; Sandy loam (Light); Massive grade of structure; Very weak consistence; 
	10-20%, coarse gravelly, 20-60mm, angular, Sandstone, coarse fragments; Few (2 - 10 %), 
	Ferruginous, Coarse (6 - 20 mm), Nodules; Gradual change to - 
	C	5.6 - 5.95 m	Reddish yellow (5YR6/8-Moist); ; Loamy coarse sand; Massive grade of structure; Moist; Very 
	weak consistence; 10-20%, coarse gravelly, 20-60mm, angular, Sandstone, coarse fragments; 
	Many (20 - 50 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Gradual change to - 
	5.95 - 6.05 m	Reddish yellow (7.5YR7/6-Moist); , 10YR68; , 10YR86; Clayey coarse sand; Massive grade of 
	structure; Very weak consistence; 20-50%, fine gravelly, 2-6mm, Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	1-2CMS DARKER SURFACE:20-60CM A1 MATERIAL DOWN WORM CASTS:595-+CM MOTTLED COARSE SST:                      
	             
	Site Notes
	HEATHLANDS

	Project Name:	Regional
	Project Code:	REG	Site ID:	T129	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.4A	 0.017A	 0.53B	 0.33	 0.05	 0.11	 4.5F	 5.5C	 5.5F	2.00
	0.05 - 0.1	5.5A	 0.023A
	0.1 - 0.2	5.4A	 0.026A
	0.2 - 0.3	5.4A	 0.017A	 0.07B	 0.16	 0.02	 0.05	 3F	 3.3C	 3.3F	1.52
	0.3 - 0.4	5.5A	 0.017A
	0.4 - 0.5	5.8A	 0.017A
	0.5 - 0.6	5.8A	 0.02A	 0.07B	 0.21	 0.03	 0.07	 1.7F	 2.1C	 2.1F	3.33
	0.6 - 0.7	5.8A	 0.017A
	0.7 - 0.8	5.7A	 0.02A
	0.8 - 0.9	5.8A	 0.014A
	0.9 - 1.05	5.8A	 0.017A
	1.05 - 1.2	5.8A	 0.017A	 0.07B	 0.37	 0.04	 0.05	 0.6F	 1.1C	 1.1F	4.55
	1.2 - 1.35	5.7A	 0.017A
	1.35 - 1.5	5.7A	 0.017A
	1.5 - 1.65	5.7A	 0.017A
	1.65 - 1.8	5.7A	 0.02A
	1.8 - 2.1	5.7A	 0.017A	 0.04B	 0.39	 0.04	 0.06	 1.1F	 1.1C	 1.6F	5.45
	2.1 - 2.4	5.7A	 0.017A
	2.4 - 2.7	5.7A	 0.02A
	2.7 - 3	5.8A	 0.023A
	3 - 3.3	5.8A	 0.026A
	3.3 - 3.6	6A	 0.029A
	3.6 - 4.1	5.6A	 0.029A
	4.1 - 4.6	5.8A	 0.026A
	4.6 - 4.85	5.8A	 0.029A
	4.85 - 5.1	5.5A	 0.023A
	5.1 - 5.6	5.6A	 0.029A
	5.6 - 5.95	5.5A	 0.029A
	5.95 - 6.25	5.6A	 0.026A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 1.3D	<2A	 0.004A	 0.06A	 0.01A	 0	 65A	 23	 3	 8
	<2B
	0.05 - 0.1	 0.89D	 0.05A	 0	 63A	 25	 1	 12
	0.1 - 0.2	 0	 58A	 29	 1	 12
	0.2 - 0.3	 0.52D	<2A	 0.005A	 0.04A	 0.01A	 0	 68A	 19	 1	 12
	<2B
	0.3 - 0.4	 0	 52A	 32	 0	 16
	0.4 - 0.5
	0.5 - 0.6	<2B	 0.004A	 0.01A	 0	 65A	 21	 1	 14
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9	 0	 54A	 30	 1	 16
	0.9 - 1.05
	1.05 - 1.2	<2B	 0.006A	 0.02A	 0	 63A	 19	 1	 18
	1.2 - 1.35	 0	 53A	 23	 1	 23
	1.35 - 1.5
	1.5 - 1.65

	Project Name:	Regional
	Project Code:	REG	Site ID:	T129	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	1.65 - 1.8
	1.8 - 2.1	<2B	 0.007A	 0.02A	 0	 55A	 20	 9	 16
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3
	3 - 3.3	 0	 46A	 24	 1	 30
	3.3 - 3.6
	3.6 - 4.1
	4.1 - 4.6
	4.6 - 4.85	 60	 42A	 35	 2	 22
	4.85 - 5.1	 54	 49A	 31	 2	 18
	5.1 - 5.6
	5.6 - 5.95	 40	 66A	 19	 2	 13
	5.95 - 6.25	 41	 70A	 13	 1	 16
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1.05
	1.05 - 1.2
	1.2 - 1.35
	1.35 - 1.5
	1.5 - 1.65
	1.65 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3
	3 - 3.3
	3.3 - 3.6
	3.6 - 4.1
	4.1 - 4.6
	4.6 - 4.85
	4.85 - 5.1
	5.1 - 5.6
	5.6 - 5.95
	5.95 - 6.25

	Project Name:	Regional
	Project Code:	REG	Site ID:	T129	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)